#

# Attribute and Parameter Cross Reference

This appendix contains tables that cross reference RADIUS attributes and MAX parameters. This appendix contains:

Parameters and analogous attributes
Attributes and parameters in numerical order
Attributes and parameters in alphabetical order

## Parameters and analogous attributes

Table B-1 cross references the Ascend RADIUS dictionary's attributes to parameters in the MAX unit's menu-driven user interface. The table is arranged by parameter in alphabetical order.

Table B-1. Parameters and analogous attributes

#### Profile | #### Parameter | #### Analogous attribute
--- | --- | ---
Answer profile Connection profile (no attributes for COMB encapsulation) | Add Pers | Ascend-Add-Seconds
| Auth Req | Ascend-Require-Auth
| BACP | Ascend-BACP-Enable
| Base Ch Count | Ascend-Base-Channel-Count
| Bill # | Ascend-Billing-Number
| Bridge | Ascend-Bridge
| Callback | Ascend-Callback
| Call-by-Call | Ascend-Call-By-Call
| Called # | Client-Port-DNIS
| Calling # | Caller-Id
| Call Type | Ascend-Call-Type
| CBCP Enable | Ascend-CBCP-Enable
| CBCP Mode | Ascend-CBCP-Mode
| CBCP Trunk Group | Ascend-CBCP-Trunk-Group
| Client Gateway | Ascend-Client-Gateway
| Circuit | Ascend-FR-Circuit-Name
| Data Svc | Ascend-Data-Svc
| DBA Monitor | Ascend-DBA-Monitor
| Dec Ch Cnt | Ascend-Dec-Channel-Count
| Dial # | Ascend-Dial-Number
| DLCI | Ascend-FR-DLCI
| Dyn Alg | Ascend-History-Weigh-Type
| Encaps=TCP-CLEAR | Login-Service=TCP-Clear
| Encaps submenu parameters in the Answer profile Encaps parameter in the Connection profile | Framed-Protocol
| Expect Callback | Ascend-Expect-Callback
| Force 56 | Ascend-Force-56
| FR Direct | Ascend-FR-Direct
| FR DLCI | Ascend-FR-Direct-DLCI
| FR Prof | Ascend-FR-Direct-Profile
| Group | Ascend-Group
| Handle IPX | Ascend-Handle-IPX
| Idle | Ascend-Idle-Limit
| Idle Pct | Ascend-MPP-Idle-Percent
| IF Adrs | Ascend-Remote-Addr
| Inc Ch Cnt | Ascend-Inc-Channel-Count
| IP Direct | Ascend-IP-Direct
| IPX Alias# | Ascend-IPX-Alias
| LAN Adrs | Framed-Address Framed-Netmask
| Link Comp | Ascend-Link-Compression
| Login Host | Login-Host
| Login Port | Login-TCP-Port
| Max Call Duration | Ascend-Maximum-Call-Duration
| Max Ch Count | Ascend-Maximum-Channels
| Max Leases | Ascend-DHCP-Maximum-Leases
| Metric | Ascend-Metric
| Min Ch Count | Ascend-Minimum-Channels
| MRU | Framed-MTU
| Multicast Client | Ascend-Multicast-Client
| Multicast Rate Limit | Ascend-Multicast-Rate-Limit
| Net End | Ascend-AppleTalk-Route net_end
| Net Start | Ascend-AppleTalk-Route net_start
| NetWare t/o | Ascend-Netware-timeout
| Peer | Ascend-IPX-Peer-Mode Ascend-AppleTalk-Peer-Mode (in AppleTalk Options submenu)
| Pool | Ascend-Assign-IP-Pool
| Pool Number | Ascend-DHCP-Pool-Number
| Preempt | Ascend-Preempt-Limit
| PRI # Type | Ascend-PRI-Number-Type
| Recv PW | Password Ascend-Receive-Secret
| Reply Enabled | Ascend-DHCP-Reply
| RIP | Framed-Routing
| Route AppleTalk | Ascend-Route-AppleTalk
| Route IP | Ascend-Route-IP
| Route IPX | Ascend-Route-IPX
| Sec Hist | Ascend-Seconds-Of-History
| Send Auth | Ascend-Send-Auth
| Send PW | Ascend-Send-Passwd Ascend-Send-Secret
| Station | User-Name
| Sub Pers | Ascend-Remove-Seconds
| Target Util | Ascend-Target-Util
| Transit # | Ascend-Transit-Number
| TS Idle Limit | Ascend-TS-Idle-Limit
| TS Idle Mode | Ascend-TS-Idle-Mode
| VJ Comp | Framed-Compression
| Zone Name | Ascend-AppleTalk-Route zone_name
Bridging profile | Bridging profile parameters | Ascend-Bridge-Address
Ethernet profile | Acct | Ascend-User-Acct-Type
| Acct Host #1 Acct Host #2 Acct Host #3 | Ascend-User-Acct-Host
| Acct-ID Base | Ascend-User-Acct-Base
| Acct Key | Ascend-User-Acct-Key
| Acct Port | Ascend-User-Acct-Port
| Acct Timeout | Ascend-User-Acct-Time
| Banner (terminal server users only) | Reply-Message
| Dialout OK | Ascend-Dialout-Allowed
| Host #1 Addr, Host #1 Text Host #2 Addr, Host #2 Text Host #3 Addr, Host #3 Text Host #4 Addr, Host #4 Text (terminal server users only) | Ascend-Host-Info
| IP Adrs | NAS-Identifier
| Immed Service (terminal server users only) | Login-Service
| Shared Prof | Ascend-Shared-Profile-Enable
Filter profile | Filter profile parameters | Ascend-Call-Filter Ascend-Data-Filter
Frame Relay profile | Call Type | Ascend-Call-Type
| Data Svc | Ascend-Data-Svc
| DCE N392 | Ascend-FR-DCE-N392
| DCE N393 | Ascend-FR-DCE-N393
| DTE N392 | Ascend-FR-DTE-N392
| DTE N393 | Ascend-FR-DTE-N393
| FR Type | Ascend-FR-Type
| Link Mgmt | Ascend-FR-Link-Mgt
| Link Up | Ascend-FR-LinkUp
| N391 | Ascend-FR-N391
| Nailed Grp | Ascend-FR-Nailed-Grp
| T391 | Ascend-FR-T391
| T392 | Ascend-FR-T392
IPX Route profile | IPX Route profile parameters | Ascend-IPX-Route
Route profile | Route profile parameters | Framed-Route

## Attributes and parameters in numerical order

Table B-2 cross references the Ascend RADIUS dictionary's attributes to parameters in MAX unit's menu-driven user interface. The table is arranged by attribute in numerical order.

Table B-2. Attributes and analogous parameters in numerical order

#### Attribute number | #### Attribute name | #### Attribute values | #### Analogous parameter
--- | --- | --- | ---
1 | User-Name | Text string | Station
2 | Password (User-Password) | Text string | Recv PW
3 | Challenge-Response | Text string | No analogous parameter
4 | NAS-Identifier | IP address | IP Adrs
5 | NAS-Port | Integer | No analogous parameter
6 | User-Service | Login-User (1) Framed-User (2) Dialout-Framed-User (5) (3, 4, and 6 are not supported) | No analogous parameter
7 | Framed-Protocol | PPP (1) SLIP (2) MPP (256) EURAW (257) EUUI (258) COMB (260) FR (261) ARA (262) FR-CIR (263) | No analogous parameter
8 | Framed-Address | IP address | LAN Adrs
9 | Framed-Netmask | IP address | LAN Adrs
10 | Framed-Routing | None (0) Broadcast (1) Listen (2) Broadcast-Listen (3) Broadcast-v2 (4) Listen-v2 (5) Broadcast-Listen-v2 (6) | RIP
11 | Filter-Id | 0 indicates that no filtering is being used (the default). 1-99 indicates that a filter created using the vt100 interface is being used. 100-199 indicates that a filter created using SAM is being used. | No analogous parameter
12 | Framed-MTU | Integer | MRU
13 | Framed-Compression | Van-Jacobson-TCP-IP (1) (No other values supported) | VJ Comp
14 | Login-Host | IP address | Login Host
15 | Login-Service | Telnet (0) Rlogin (1) TCP-Clear (2) | Immed Service Encaps=TCP-CLEAR
16 | Login-TCP-Port | Integer | Login Port
17 | Change-Password | Text string | No analogous parameter
18 | Reply-Message | Text string | Banner (terminal server users only)
21 | Ascend-PW-Expiration | Date | No analogous parameter
22 | Framed-Route | host_ipaddr /subnet_mask router_ ipaddr metric private profile_name preference | Dest Gateway Metric Private Name Preference
23 | Framed-IPX-Network | Integer | IPX Net#
25 | Class | Text string | No analogous parameter
30 | Client-Port-DNIS | Text string | Called #
31 | Caller-Id | Text string | Calling #
40 | Acct-Status-Type | Start (1) Stop (2) | No analogous parameter
41 | Acct-Delay-Time | Integer | No analogous parameter
42 | Acct-Input-Octets | Integer | No analogous parameter
43 | Acct-Output-Octets | Integer | No analogous parameter
44 | Acct-Session-Id | Text string | No analogous parameter
45 | Acct-Authentic | RADIUS (1) Local (2) | No analogous parameter
46 | Acct-Session-Time | Integer | No analogous parameter
47 | Acct-Input-packets | Integer | No analogous parameter
48 | Acct-Output-packets | Integer | No analogous parameter
61 | NAS-Port-Type | Async Sync ISDN-Sync ISDN-Async-v120 ISDN-Async-v110 Virtual | No analogous parameter
64 | Tunnel-Type | PPTP L2TP | No analogous parameter
65 | Tunnel-Medium-Type | IP X25 (not yet supported) ATM (not yet supported) | No analogous parameter
66 | Tunnel-Client-Endpoint | String | No analogous parameter
67 | Tunnel-Server-Endpoint | Host name or IP address, but not both | No analogous parameter.
68 | Tunnel-ID | String | No analogous parameter.
112 | Ascend-CBCP-Enable | CBCP-Enabled (0) CBCP-Not-Enabled (1) | CBCP Enable
113 | Ascend-CBCP-Mode | CBCP-No-Callback (1) CBCP-User-Callback (2) CBCP-Profile-Callback (3) CBCP-User-Or-No (7) | CBCP Mode
115 | Ascend-CBCP-Trunk-Group | Integer between 4 and 9 | CBCP Trunk Group
116 | Ascend-AppleTalk-Route | net_start net_end zone_name profile_name | Net Start Net End Zone Name string
117 | Ascend-AppleTalk-Peer-Mode | Appletalk-Peer-Router (0). Appletalk-Peer-Dialin | Peer (AppleTalk Options submenu)
118 | Ascend-Route-AppleTalk | Route-Appletalk-No (0) Route-Appletalk-Yes (1) | Route AppleTalk
120 | Ascend-Modem-PortNo | Integer | No analogous parameter.
121 | Ascend-Modem-SlotNo | Integer | No analogous parameter
125 | Ascend-Maximum-Call-Duration | Integer | Max Call Duration
126 | Ascend-Preference | Integer | No analogous parameter
127 | Tunneling-Protocol | ATMP | No analogous parameter
128 | Ascend-Shared-Profile-Enable | Yes No | Shared Prof
131 | Ascend-Dialout-Allowed | Dialout-Not-Allowed (0) Dialout-Allowed (1) | Dialout OK
132 | Ascend-Client-Gateway | IP address | Client Gateway
134 | Ascend-BACP-Enable | BACP-No (0) BACP-Yes (1) | BACP
138 | Ascend-User-Acct-Type | Ascend-User-Acct-None (0) Ascend-User-Acct-User (1) Ascend-User-Acct-User-Default (2) | Acct
139 | Ascend-User-Acct-Host | IP address | Acct Host #1 Acct Host #2 Acct Host #3
140 | Ascend-User-Acct-Port | Integer | Acct Port
141 | Ascend-User-Acct-Key | Text string | Acct Key
142 | Ascend-User-Acct-Base | Ascend-User-Acct-Base-10 (0) Ascend-User-Acct-Base-16 (1) | Acct-ID Base
143 | Ascend-User-Acct-Time | Integer | Acct Timeout
144 | Ascend-Assign-IP-Client | IP address | No analogous parameter
145 | Ascend-Assign-IP-Server | IP address | No analogous parameter
146 | Ascend-Assign-IP-Global-Pool | Text string | No analogous parameter
147 | Ascend-DHCP-Reply | DHCP-Reply-No (0) DHCP-Reply-Yes (1) | Reply Enabled
148 | Ascend-DHCP-Pool-Number | Integer | Pool Number
149 | Ascend-Expect-Callback | Expect-Callback-No (0) Expect-Callback-Yes (1) | Expect Callback
150 | Ascend-Event-Type | Ascend-Coldstart (1) Ascend-Session-Event (2) | No analogous parameter
151 | Ascend-Session-Svr-Key | Text string | No analogous parameter
152 | Ascend-Multicast-Client | Multicast-No (0) Multicast-Yes (1) | Multicast Client
153 | Ascend-Multicast-Rate-Limit | Integer | Multicast Rate Limit
154 | Ascend-IF-Netmask | IP address | No analogous parameter
155 | Ascend-Remote-Addr | IP address | IF Adrs
156 | Ascend-FR-Circuit-Name | Text string | Circuit
157 | Ascend-FR-LinkUp | Ascend-LinkUp-Default (0) Ascend-LinkUp-AlwaysUp (1) | Link Up
158 | Ascend-FR-Nailed-Grp | Integer | Nailed Grp
159 | Ascend-FR-Type | Ascend-FR-DTE (0) Ascend-FR-DCE (1) Ascend-FR-NNI (2) | FR Type
160 | Ascend-FR-Link-Mgt | Ascend-FR-No-Link-Mgt (0) Ascend-FR-T1-617D (1) Ascend-FR-Q-933A (2) | Link Mgmt
161 | Ascend-FR-N391 | Integer | N391
162 | Ascend-FR-DCE-N392 | Integer | DCE N392
163 | Ascend-FR-DTE-N392 | Integer | DTE N392
164 | Ascend-FR-DCE-N393 | Integer | DCE N393
165 | Ascend-FR-DTE-N393 | Integer | DTE N393
166 | Ascend-FR-T391 | Integer | T391
167 | Ascend-FR-T392 | Integer | T392
168 | Ascend-Bridge-Address | MAC_address profile_name IP_address | Enet Adrs Net Adrs
169 | Ascend-TS-Idle-Limit | Integer | TS Idle Limit
170 | Ascend-TS-Idle-Mode | TS-Idle-None (0) TS-Idle-Input (1) TS-Idle-Input-Output (2) | TS Idle Mode
171 | Ascend-DBA-Monitor | DBA-Transmit (0) DBA-Transmit-Recv (1) DBA-None (2) | DBA Monitor
172 | Ascend-Base-Channel-Count | Integer | Base Ch Count
173 | Ascend-Minimum-Channels | Integer | Min Ch Count
174 | Ascend-IPX-Route | profile_name network# [node#] [socket#] [server_type] [hop_count] [tick_count] [name] | Connection # Network Node Socket Server Type Hop Count Tick Count Server Name
175 | Ascend-FT1-Caller | FT1-No (0) FT1-Yes (1) | FT1-Caller
176 | Ascend-backup | Text string | Backup
177 | Ascend-Call-Type | Nailed (1) Nailed/Mpp (2) Perm/Switched (3) | Call Type
178 | Ascend-Group | Single integer or comma-separated group of integers | Group
179 | Ascend-FR-DLCI | Integer between 16 and 991 | DLCI
180 | Ascend-FR-Profile-Name | Text string | FR Prof
181 | Ascend-Ara-PW | Text string | Password in the Encaps Options submenu of the Connection profile when Encaps=ARA.
182 | Ascend-IPX-Node-Addr | 12-digit ASCII string | Node
184 | Ascend-Home-Agent-Password | Text string | No analogous parameter
185 | Ascend-Home-Network-Name | Text string | No analogous parameter
186 | Ascend-Home-Agent-UDP-Port | Integer | No analogous parameter
187 | Ascend-Multilink-ID | Integer | No analogous parameter
188 | Ascend-Num-In-Multilink | Integer | No analogous parameter
189 | Ascend-First-Dest | IP address | No analogous parameter
190 | Ascend-Pre-Input-Octets | Integer | No analogous parameter
191 | Ascend-Pre-Output-Octets | Integer | No analogous parameter
192 | Ascend-Pre-Input-packets | Integer | No analogous parameter
193 | Ascend-Pre-Output-packets | Integer | No analogous parameter
194 | Ascend-Maximum-Time | Integer | Max Call Duration
195 | Ascend-Disconnect-Cause | Integer | No analogous parameter
196 | Ascend-Connect-Progress | Integer | No analogous parameter
197 | Ascend-Data-Rate | Integer | No analogous parameter
198 | Ascend-PreSession-Time | Integer | No analogous parameter
199 | Ascend-Token-Idle | Integer | No analogous parameter
200 | Ascend-Token-Immediate | Tok-Imm-No (0) Tok-Imm-Yes (1) | No analogous parameter
201 | Ascend-Require-Auth | Not-Require-Auth (0) Require-Auth (1) | Auth Req
202 | Ascend-Number-Sessions | Text string | No analogous parameter
203 | Ascend-Authen-Alias | Text string | No analogous parameter
204 | Ascend-Token-Expiry | Integer | No analogous parameter
205 | Ascend-Menu-Selector | Text string | No analogous parameter
206 | Ascend-Menu-Item | Text string | No analogous parameter
208 | Ascend-PW-Lifetime | Integer | No analogous parameter
209 | Ascend-IP-Direct | IP address | IP Direct
210 | Ascend-PPP-VJ-Slot-Comp | VJ-Slot-Comp-No (1) | No analogous parameter
211 | Ascend-PPP-VJ-1172 | PPP-VJ-1172 (1) | No analogous parameter
212 | Ascend-PPP-Async-Map | Integer | No analogous parameter
213 | Ascend-Third-Prompt | Text string | 3rd Prompt
214 | Ascend-Send-Secret | Text string | Send PW
215 | Ascend-Receive-Secret | Text string | Recv PW
216 | Ascend-IPX-Peer-Mode | IPX-Peer-Router (0) IPX-Peer-Dialin (1) | No analogous parameter
217 | Ascend-IP-Pool-Definition | Text string | Pool Start #1, #2 Pool Count #1, #2
218 | Ascend-Assign-IP-Pool | Integer | Pool
219 | Ascend-FR-Direct | FR-Direct-No (0) FR-Direct-Yes (1) | FR Direct
220 | Ascend-FR-Direct-Profile | Text string | FR Prof
221 | Ascend-FR-Direct-DLCI | Integer | FR DLCI
222 | Ascend-Handle-IPX | Handle-IPX-None (0) Handle-IPX-Client (1) Handle-IPX-Server (2) | Handle IPX
223 | Ascend-Netware-timeout | Integer | NetWare t/o
224 | Ascend-IPX-Alias | Text string | IPX Alias#
225 | Ascend-Metric | Integer | Metric
226 | Ascend-PRI-Number-Type | Unknown-Number (0) Intl-Number (1) National-Number (2) Local-Number (4) Abbrev-Number (5) | PRI # Type
227 | Ascend-Dial-Number | Text string | Dial #
228 | Ascend-Route-IP | Route-IP-No (0) Route-IP-Yes (1) | Route IP
229 | Ascend-Route-IPX | Route-IPX-No (0) Route-IPX-Yes (1) | Route IPX
230 | Ascend-Bridge | Bridge-No (0) Bridge-Yes (1) | Bridge
231 | Ascend-Send-Auth | Send-Auth-None (0) Send-Auth-PAP (1) Send-Auth-CHAP (2) | Send Auth
232 | Ascend-Send-Passwd | Text string | Send PW
233 | Ascend-Link-Compression | Link-Comp-None (0) Link-Comp-Stac (1) | Link Comp
234 | Ascend-Target-Util | Integer | Target Util
235 | Ascend-Maximum-Channels | Integer | Max Ch Cnt
236 | Ascend-Inc-Channel-Count | Integer | Inc Ch Cnt
237 | Ascend-Dec-Channel-Count | Integer | Dec Ch Cnt
238 | Ascend-Seconds-Of-History | Integer | Sec Hist
239 | Ascend-History-Weigh-Type | History-Constant (0) History-Linear (1) History-Quadratic (2) | Dyn Alg
240 | Ascend-Add-Seconds | Integer | Add Pers
241 | Ascend-Remove-Seconds | Integer | Sub Pers
242 | Ascend-Data-Filter | Filter specification | Filter profile parameters
243 | Ascend-Call-Filter | Filter specification | Filter profile parameters
244 | Ascend-Idle-Limit | Integer | Idle
245 | Ascend-Preempt-Limit | Integer | Preempt
246 | Ascend-Callback | Callback-No (0) Callback-Yes (1) | Callback
255 | Ascend-Xmit-Rate | Integer | No analogous parameter.
247 | Ascend-Data-Svc | Switched-Voice-Bearer (0) Switched-56KR (1) Switched-64K (2) Switched-64KR (3) Switched-56K (4) Nailed-56KR (1) Nailed-64K (2) Switched-384KR (5) Switched-384K (6) Switched-1536K (7) Switched-1536KR (8) Switched-128K (9) Switched-192K (10) Switched-256K (11) Switched-320K (12) Switched-384K-MR (13) Switched-448K (14) Switched-512K (15) Switched-576K (16) Switched-640K (17) Switched-704K (18) Switched-768K (19) Switched-832K (20) Switched-896K (21) Switched-960K (22) Switched-1024K (23) Switched-1088K (24) Switched-1152K (25) Switched-1216K (26) Switched-1280K (27) Switched-1344K (28) Switched-1408K (29) Switched-1472K (30) Switched-1600K (31) Switched-1664K (32) Switched-1728K (33) Switched-1792K (34) Switched-1856K (35) Switched-1920K (36) Switched-inherited (37) Switched-restricted-bearer-x30 (38) Switched-clear-bearer-v110 (39) Switched-restricted-64-x30 (40) Switched-clear-56-v110 (41) Switched-modem (42) Switched-atmodem (43) | Data Svc
248 | Ascend-Force-56 | Force-56-No (0) Force-56-Yes (1) | Force 56
249 | Ascend-Billing-Number | Text string | Bill #
250 | Ascend-Call-By-Call | Integer | Call-by-Call
251 | Ascend-Transit-Number | Text string | Transit #
252 | Ascend-Host-Info | Text string | Host #1 Addr Host #1 Text Host #2 Addr Host #2 Text Host #3 Addr Host #3 Text Host #4 Addr Host #4 Text
253 | Ascend-PPP-Address | IP address | No analogous parameter
254 | Ascend-MPP-Idle-Percent | Integer | Idle Pct

## Attributes and parameters in alphabetical order

Table B-3 cross references the Ascend RADIUS dictionary's attributes to parameters in MAX unit's menu-driven user interface. The table is arranged by attribute in alphabetical order.

Table B-3. Attributes and analogous parameters in alphabetical order

#### Attribute name | #### Attribute number | #### Attribute values | #### Analogous parameter
--- | --- | --- | ---
Acct-Authentic | 45 | RADIUS (1) Local (2) | No analogous parameter
Acct-Delay-Time | 41 | Integer | No analogous parameter
Acct-Input-Octets | 42 | Integer | No analogous parameter
Acct-Input-packets | 47 | Integer | No analogous parameter
Acct-Output-Octets | 43 | Integer | No analogous parameter
Acct-Output-packets | 48 | Integer | No analogous parameter
Acct-Session-Id | 44 | Text string | No analogous parameter
Acct-Session-Time | 46 | Integer | No analogous parameter
Acct-Status-Type | 40 | Start (1) Stop (2) | No analogous parameter
Ascend-Add-Seconds | 240 | Integer | Add Pers
Ascend-AppleTalk-Peer-Mode | 117 | Appletalk-Peer-Router (0). Appletalk-Peer-Dialin | Peer (AppleTalk Options submenu)
Ascend-AppleTalk-Route | 116 | net_start net_end zone_name profile_name | Net Start Net End Zone Name string
Ascend-Ara-PW | 181 | Text string | Password in the Encaps Options submenu of the Connection profile when Encaps=ARA.
Ascend-Assign-IP-Client | 144 | IP address | No analogous parameter
Ascend-Assign-IP-Global-Pool | 146 | Text string | No analogous parameter
Ascend-Assign-IP-Pool | 218 | Integer | Pool
Ascend-Assign-IP-Server | 145 | IP address | No analogous parameter
Ascend-Authen-Alias | 203 | Text string | No analogous parameter
Ascend-backup | 176 | Text string | Backup
Ascend-BACP-Enable | 134 | BACP-No (0) BACP-Yes (1) | BACP
Ascend-Base-Channel-Count | 172 | Integer | Base Ch Count
Ascend-Billing-Number | 249 | Text string | Bill #
Ascend-Bridge | 230 | Bridge-No (0) Bridge-Yes (1) | Bridge
Ascend-Bridge-Address | 168 | MAC_address profile_name IP_address | Enet Adrs Net Adrs
Ascend-Callback | 246 | Callback-No (0) Callback-Yes (1) | Callback
Ascend-Call-By-Call | 250 | Integer | Call-by-Call
Ascend-Call-Filter | 243 | Filter specification | Filter profile parameters
Ascend-Call-Type | 177 | Nailed (1) Nailed/Mpp (2) Perm/Switched (3) | Call Type
Ascend-CBCP-Enable | 112 | CBCP-Enabled (0) CBCP-Not-Enabled (1) | CBCP Enable
Ascend-CBCP-Mode | 113 | CBCP-No-Callback (1) CBCP-User-Callback (2) CBCP-Profile-Callback (3) CBCP-User-Or-No (7) | CBCP Mode
Ascend-CBCP-Trunk-Group | 115 | Integer between 4 and 9 | CBCP Trunk Group
Ascend-Client-Gateway | 132 | IP address | Client Gateway
Ascend-Connect-Progress | 196 | Integer | No analogous parameter
Ascend-Data-Filter | 242 | Filter specification | Filter profile parameters
Ascend-Data-Rate | 197 | Integer | No analogous parameter
Ascend-Data-Svc | 247 | Switched-Voice-Bearer (0) Switched-56KR (1) Switched-64K (2) Switched-64KR (3) Switched-56K (4) Nailed-56KR (1) Nailed-64K (2) Switched-384KR (5) Switched-384K (6) Switched-1536K (7) Switched-1536KR (8) Switched-128K (9) Switched-192K (10) Switched-256K (11) Switched-320K (12) Switched-384K-MR (13) Switched-448K (14) Switched-512K (15) Switched-576K (16) Switched-640K (17) Switched-704K (18) Switched-768K (19) Switched-832K (20) Switched-896K (21) Switched-960K (22) Switched-1024K (23) Switched-1088K (24) Switched-1152K (25) Switched-1216K (26) Switched-1280K (27) Switched-1344K (28) Switched-1408K (29) Switched-1472K (30) Switched-1600K (31) Switched-1664K (32) Switched-1728K (33) Switched-1792K (34) Switched-1856K (35) Switched-1920K (36) Switched-inherited (37) Switched-restricted-bearer-x30 (38) Switched-clear-bearer-v110 (39) Switched-restricted-64-x30 (40) Switched-clear-56-v110 (41) Switched-modem (42) Switched-atmodem (43) | Data Svc
Ascend-DBA-Monitor | 171 | DBA-Transmit (0) DBA-Transmit-Recv (1) DBA-None (2) | DBA Monitor
Ascend-Dec-Channel-Count | 237 | Integer | Dec Ch Cnt
Ascend-DHCP-Maximum-Leases |  | Integer | Max Leases
Ascend-DHCP-Pool-Number | 148 | Integer | Pool Number
Ascend-DHCP-Reply | 147 | DHCP-Reply-No (0) DHCP-Reply-Yes (1) | Reply Enabled
Ascend-Dial-Number | 227 | Text string | Dial #
Ascend-Dialout-Allowed | 131 | Dialout-Not-Allowed (0) Dialout-Allowed (1) | Dialout OK
Ascend-Disconnect-Cause | 195 | Integer | No analogous parameter
Ascend-Event-Type | 150 | Ascend-Coldstart (1) Ascend-Session-Event (2) | No analogous parameter
Ascend-Expect-Callback | 149 | Expect-Callback-No (0) Expect-Callback-Yes (1) | Expect Callback
Ascend-First-Dest | 189 | IP address | No analogous parameter
Ascend-Force-56 | 248 | Force-56-No (0) Force-56-Yes (1) | Force 56
Ascend-FR-Circuit-Name | 156 | Text string | Circuit
Ascend-FR-DCE-N392 | 162 | Integer | DCE N392
Ascend-FR-DCE-N393 | 164 | Integer | DCE N393
Ascend-FR-DTE-N392 | 163 | Integer | DTE N392
Ascend-FR-DTE-N393 | 165 | Integer | DTE N393
Ascend-FR-Direct | 219 | FR-Direct-No (0) FR-Direct-Yes (1) | FR Direct
Ascend-FR-Direct-DLCI | 221 | Integer | FR DLCI
Ascend-FR-Direct-Profile | 220 | Text string | FR Prof
Ascend-FR-DLCI | 179 | Integer between 16 and 991 | DLCI
Ascend-FR-Link-Mgt | 160 | Ascend-FR-No-Link-Mgt (0) Ascend-FR-T1-617D (1) Ascend-FR-Q-933A (2) | Link Mgmt
Ascend-FR-LinkUp | 157 | Ascend-LinkUp-Default (0) Ascend-LinkUp-AlwaysUp (1) | Link Up
Ascend-FR-N391 | 161 | Integer | N391
Ascend-FR-Nailed-Grp | 158 | Integer | Nailed Grp
Ascend-FR-Profile-Name | 180 | Text string | FR Prof
Ascend-FR-T391 | 166 | Integer | T391
Ascend-FR-T392 | 167 | Integer | T392
Ascend-FR-Type | 159 | Ascend-FR-DTE (0) Ascend-FR-DCE (1) Ascend-FR-NNI (2) | FR Type
Ascend-FT1-Caller | 175 | FT1-No (0) FT1-Yes (1) | FT1-Caller
Ascend-Group | 178 | Single integer or comma-separated group of integers | Group
Ascend-Handle-IPX | 222 | Handle-IPX-None (0) Handle-IPX-Client (1) Handle-IPX-Server (2) | Handle IPX
Ascend-History-Weigh-Type | 239 | History-Constant (0) History-Linear (1) History-Quadratic (2) | Dyn Alg
Ascend-Home-Agent-Password | 184 | Text string | No analogous parameter
Ascend-Home-Agent-UDP-Port | 186 | Integer | No analogous parameter
Ascend-Home-Network-Name | 185 | Text string | No analogous parameter
Ascend-Host-Info | 252 | Text string | Host #1 Addr Host #1 Text Host #2 Addr Host #2 Text Host #3 Addr Host #3 Text Host #4 Addr Host #4 Text
Ascend-Idle-Limit | 244 | Integer | Idle
Ascend-IF-Netmask | 154 | IP address | No analogous parameter
Ascend-Inc-Channel-Count | 236 | Integer | Inc Ch Cnt
Ascend-IP-Direct | 209 | IP address | IP Direct
Ascend-IP-Pool-Definition | 217 | Text string | Pool Start #1, #2 Pool Count #1, #2
Ascend-IPX-Alias | 224 | Text string | IPX Alias#
Ascend-IPX-Node-Addr | 182 | 12-digit ASCII string | Node
Ascend-IPX-Peer-Mode | 216 | IPX-Peer-Router (0) IPX-Peer-Dialin (1) | No analogous parameter
Ascend-IPX-Route | 174 | profile_name network# [node#] [socket#] [server_type] [hop_count] [tick_count] [name] | Connection # Network Node Socket Server Type Hop Count Tick Count Server Name
Ascend-Link-Compression | 233 | Link-Comp-None (0) Link-Comp-Stac (1) | Link Comp
Ascend-Maximum-Call-Duration | 125 | Integer | Max Call Duration
Ascend-Maximum-Channels | 235 | Integer | Max Ch Cnt
Ascend-Maximum-Time | 194 | Integer | Max Call Duration
Ascend-Menu-Item | 206 | Text string | No analogous parameter
Ascend-Menu-Selector | 205 | Text string | No analogous parameter
Ascend-Metric | 225 | Integer | Metric
Ascend-Minimum-Channels | 173 | Integer | Min Ch Count
Ascend-Modem-PortNo | 120 | Integer | No analogous parameter
Ascend-Modem-SlotNo | 121 | Integer | No analogous parameter
Ascend-MPP-Idle-Percent | 254 | Integer | Idle Pct
Ascend-Multicast-Client | 152 | Multicast-No (0) Multicast-Yes (1) | Multicast Client
Ascend-Multicast-Rate-Limit | 153 | Integer | Multicast Rate Limit
Ascend-Multilink-ID | 187 | Integer | No analogous parameter
Ascend-Netware-timeout | 223 | Integer | NetWare t/o
Ascend-Number-Sessions | 202 | Text string | No analogous parameter
Ascend-Num-In-Multilink | 188 | Integer | No analogous parameter
Ascend-PPP-Address | 253 | IP address | No analogous parameter
Ascend-PPP-Async-Map | 212 | Integer | No analogous parameter
Ascend-PPP-VJ-1172 | 211 | PPP-VJ-1172 (1) | No analogous parameter
Ascend-PPP-VJ-Slot-Comp | 210 | VJ-Slot-Comp-No (1) | No analogous parameter
Ascend-Preempt-Limit | 245 | Integer | Preempt
Ascend-Pre-Input-Octets | 190 | Integer | No analogous parameter
Ascend-Pre-Input-packets | 192 | Integer | No analogous parameter
Ascend-Pre-Output-Octets | 191 | Integer | No analogous parameter
Ascend-Pre-Output-packets | 193 | Integer | No analogous parameter
Ascend-PreSession-Time | 198 | Integer | No analogous parameter
Ascend-Primary-Home-Agent |  | IP address or hostname | No analogous parameter
Ascend-PRI-Number-Type | 226 | Unknown-Number (0) Intl-Number (1) National-Number (2) Local-Number (4) Abbrev-Number (5) | PRI # Type
Ascend-PW-Expiration | 21 | Date | No analogous parameter
Ascend-PW-Lifetime | 208 | Integer | No analogous parameter
Ascend-Receive-Secret | 215 | Text string | Recv PW
Ascend-Remote-Addr | 155 | IP address | IF Adrs
Ascend-Remove-Seconds | 241 | Integer | Sub Pers
Ascend-Require-Auth | 201 | Not-Require-Auth (0) Require-Auth (1) | Auth Req
Ascend-Route-AppleTalk | 118 | Route-Appletalk-No (0) Route-Appletalk-Yes (1) | Route AppleTalk
Ascend-Route-IP | 228 | Route-IP-No (0) Route-IP-Yes (1) | Route IP
Ascend-Route-IPX | 229 | Route-IPX-No (0) Route-IPX-Yes (1) | Route IPX
Ascend-Secondary-Home-Agent |  | IP address or hostname | No analogous parameter
Ascend-Seconds-Of-History | 238 | Integer | Sec Hist
Ascend-Send-Auth | 231 | Send-Auth-None (0) Send-Auth-PAP (1) Send-Auth-CHAP (2) | Send Auth
Ascend-Send-Passwd | 232 | Text string | Send PW
Ascend-Send-Secret | 214 | Text string | Send PW
Ascend-Session-Svr-Key | 151 | Text string | No analogous parameter
Ascend-Target-Util | 234 | Integer | Target Util
Ascend-Third-Prompt | 213 | Text string | 3rd Prompt
Ascend-Token-Expiry | 204 | Integer | No analogous parameter
Ascend-Token-Idle | 199 | Integer | No analogous parameter
Ascend-Token-Immediate | 200 | Tok-Imm-No (0) Tok-Imm-Yes (1) | No analogous parameter
Ascend-Transit-Number | 251 | Text string | Transit #
Ascend-TS-Idle-Limit | 169 | Integer | TS Idle Limit
Ascend-TS-Idle-Mode | 170 | TS-Idle-None (0) TS-Idle-Input (1) TS-Idle-Input-Output (2) | TS Idle Mode
Ascend-User-Acct-Base | 142 | Ascend-User-Acct-Base-10 (0) Ascend-User-Acct-Base-16 (1) | Acct-ID Base
Ascend-User-Acct-Host | 139 | IP address | Acct Host #1 Acct Host #2 Acct Host #3
Ascend-User-Acct-Key | 141 | Text string | Acct Key
Ascend-User-Acct-Port | 140 | Integer | Acct Port
Ascend-User-Acct-Time | 143 | Integer | Acct Timeout
Ascend-User-Acct-Type | 138 | Ascend-User-Acct-None (0) Ascend-User-Acct-User (1) Ascend-User-Acct-User-Default (2) | Acct
Ascend-Xmit-Rate | 255 | Integer | No analogous parameter
Caller-Id | 31 | Text string | Calling #
Challenge-Response | 3 | Text string | No analogous parameter
Change-Password | 17 | Text string | No analogous parameter
Class | 25 | Text string | No analogous parameter
Client-Port-DNIS | 30 | Text string | Called #
Filter-ID | 11 | 0 indicates that no filtering is being used (the default). 1-99 indicates that a filter created using the vt100 interface is being used. 100-199 indicates that a filter created using SAM is being used. | No analogous parameter
Framed-Address | 8 | IP address | LAN Adrs
Framed-Compression | 13 | Van-Jacobson-TCP-IP (1) (No other values supported) | VJ Comp
Framed-IPX-Network | 23 | Integer | IPX Net#
Framed-MTU | 12 | Integer | MRU
Framed-Netmask | 9 | IP address | LAN Adrs
Framed-Protocol | 7 | PPP (1) SLIP (2) MPP (256) EURAW (257) EUUI (258) COMB (260) FR (261) ARA (262) FR-CIR (263) | No analogous parameter
Framed-Route | 22 | host_ipaddr /subnet_mask router_ ipaddr metric private profile_name preference | Dest Gateway Metric Private Name Preference
Framed-Routing | 10 | None (0) Broadcast (1) Listen (2) Broadcast-Listen (3) Broadcast-v2 (4) Listen-v2 (5) Broadcast-Listen-v2 (6) | RIP
Login-Host | 14 | IP address | Login Host
Login-Service | 15 | Telnet (0) Rlogin (1) TCP-Clear (2) | Immed Service Encaps=TCP-CLEAR
Login-TCP-Port | 16 | Integer | Login Port
NAS-Identifier | 4 | IP address | IP Adrs
NAS-Port | 5 | Integer | No analogous parameter
NAS-Port-Type | 61 | Async Sync ISDN-Sync ISDN-Async-v120 ISDN-Async-v110 Virtual | No analogous parameter
Password (User-Password) | 2 | Text string | Recv PW
Reply-Message | 18 | Text string | Banner (terminal server users only)
Tunnel-Client-Endpoint | 66 | Text string | No analogous parameter
Tunnel-Id | 68 | Text string | No analogous parameter
Tunnel-Medium-Type | 65 | IP X25 (not yet supported) ATM (not yet supported) | No analogous parameter
Tunnel-Server-Endpoint | 67 | Host name or IP address, but not both | No analogous parameter
Tunnel-Type | 64 | PPTP L2TP | No analogous parameter
User-Name | 1 | Text string | Station
User-Service | 6 | Login-User (1) Framed-User (2) Dialout-Framed-User (5) (3, 4, and 6 are not supported) | No analogous parameter

Copyright © 1998, Ascend Communications, Inc. All rights reserved.