# Index

## A

  Answer Defaults profiles

    MAX
    MAX TNT

## B

  bridging tables

    MAX
    MAX TNT

## C

  Call Routes profiles (MAX TNT)

  Change Address button

  configuration file, reusing

  configuration tasks

    adding slot cards
    changing existing configurations
    setting up new Ascend unit
  Configuration window

    description
    Edit icon
    Help
    Help icon
    New icon
    Save icon
  `Configurator.properties` file

  Connect menu

  Connection profiles

    MAX
    MAX TNT

## D

  Destination profiles (MAX)

  device information panel, purpose

  Dial Plan profiles (MAX)

  documentation

    NavisConnect Release Notes
    online
    online help

## E

  Ethernet address

  exit procedures

    NavisConnect
    QuickStart
    Setup (NavisConnect installer)
  Explorer

    Connect menu
    function
    Help
    Help menu
    navigation tree, refreshing
    Tools menu
  External Authentication profiles (MAX TNT)

## F

  Filters profiles

    MAX
    MAX TNT
  Frame Relay profiles

    MAX
    MAX TNT

## H

  Help menu (Explorer)

  Help, using

## I

  IP address

    assigning to a new unit

## L

  language, preference setting

  Local Network folder (navigation tree)

  Log profiles

    MAX
    MAX TNT

## M

  MAC address

  monitoring software for Ascend units

## N

  navigation tree

    IP address display
    Local Network folder
    purpose
    Recent folder
    refreshing
  NavisAccess

  NavisConnect

    description
    exiting
    Explorer See Explorer
    location on PC workstation
    product platforms supported
    Release Notes
    requirements for
    starting
    uninstalling

## O

  online help

    VT100 parameter names
  operating systems supported by NavisConnect

  Options settings

## P

  parameters

    compared to VT100 versions
    help on VT100 parameters
    MAX profiles and settings
    MAX TNT profiles and settings
    online documentation of
    purpose
    saving changes to
  passwords

  PCMCIA card ISDN adapter profiles (MAX 800)

  PCMCIA card modem profiles (MAX 800)

  POST See Power-On Self Test (POST)

  Power-On Self Test (POST)

  preference settings

    `Configurator.properties` file
    default
  profile

    creating a new
    creating a new profile
    deleting an existing
    deleting an existing profile
    displaying content of
    duplicating an existing
    duplicating an existing profile
    MAX
    MAX TNT
    saving changes to
  Protocols profiles

    MAX
    MAX TNT

## Q

  QuickStart

    exiting
    Help
    startup procedure
      usage instructions for
  QuickStart button

## R

  Recent folder (navigation tree)

    changing number of items displayed
    removing entries
  Release Notes (NavisConnect), accessing

  removing NavisConnect

  Reset button

  routing tables

    MAX
    MAX TNT

## S

  Save icon (command, Configuration window)

  Security profiles (MAX)

  Setup (NavisConnect installer)

  Simple Network Management Protocol (SNMP)

    enabling and assigning passwords
    how NavisConnect uses
  slot cards

    adding to a configured unit
    profiles on MAX
    profiles on MAX TNT
  SNMP See Simple Network Management Program (SNMP)

  startup procedure

    NavisConnect
    QuickStart
    Setup (NavisConnect installer)
  Static Routes profiles

    MAX
    MAX TNT
  Syslog

    defined
    defining server for MAX
    disabling
    enabling/disabling history file
    history filename
    opening file
    port used
  System profiles

    MAX
    MAX TNT

## T

  TAOS See True Access Operating System

  Telnet password

  TFTP See Trivial File Transfer Protocol (TFTP)

  Tools menu

  Trivial File Transfer Protocol (TFTP)

    how NavisConnect uses
    port used for
  True Access Operating System

    determining version on Ascend unit
    unsupported software versions
    version supported

## U

  uninstallation procedure

    NavisConnect
  Users profiles

    MAX
    MAX TNT

Copyright © 1998, Ascend Communications, Inc. All rights reserved.