Netserver 8/16 4.1.78 Release Notes

Changes since 4.1.82:

1). Netserver will check user "default" for missing RADIUS authentication
    attibutes.

2). Correct NAS-Port-Type with X.75 calls.

3). Corrected login prompt or PPP session failure to start after previous call
    fails to connect.

4). Corrected bad FCS in ACCM option during PPP causing authentication to fail
    with various Unix clients.

5). Corrected missing CR/LF during login session to network host.

6). "sh events" CLI command now clears properly after login session terminates.

7). PPP_RECEIVE_AUTH catch-22 during dial-out with one way authentication
    corrected.

8). User init scripts (ala USR_int) now sent properly to modem.

9). RADIUS authentication secret does not need to be set to 16 characters to
    allow proper accounting logging.

10). Added watchdog timer.


3COM Technical Support
11/30/1998



