Issues resolved since 4.1.7 release:

1). High volume of dial-in calls may leave NS serial driver locking out modem with CIP error.

2). Corrected Client Port ID value in RADIUS authentication from always reporting value of 0.

3). Fixed hang state in serial driver when using NCSI and init string sent after virtual socket
    closed.

4). Corrected corrupt 'show dial_out" display after virtual port accessed via reverse telnet or
    NCSI dialout. 

5). Corrected IPX SAP type 23 from stopping NCSI server advertisement over time.

6). Fixed CIP error modem port lockup and NS crash when attempting to dialout with reverse telnet
    and/or NCSI.

7). Corrected accounting record digest error in which Microsoft RADIUS reports
    "malformed packet".

8). CBCP now works with NT DUN clients dialing in.

9). Corrected RADIUS accouting stop records for ML/PPP calls.


3COM Technical Support

