# AP-2000 Help Contents |
[ Home ] [Proxim website]

## Command Line Interface (CLI) This section describes the AP’s Command Line (CLI) Interface. CLI commands can be used to initialize, configure, and manage the Access Point. CLI commands may be entered in real time through a keyboard or submitted with CLI scripts. The CLI is available through both the Serial Port interface and over the Ethernet interface using Telnet.
| All CLI commands and parameters are case-sensitive.
General Notes Command Line Interface (CLI) Variations CLI Command Types Using Tables & User Strings Configuring the AP using CLI commands Set Basic Configuration Parameters using CLI Commands Other Network Settings CLI Monitoring Parameters Parameter Tables ## General Notes ### Prerequisite Skills and Knowledge To use this document effectively, you should have a working knowledge of Local Area Networking (LAN) concepts, network access infrastructures, and client-server relationships. In addition, you should be familiar with software setup procedures for typical network operating systems and servers. ### Notation Conventions Computer prompts are shown as constant width type. For example: `[Device-Name]>` Information that you input as shown is displayed in bold constant width type. For example: `[Device name]>` set ipaddr 10.0.0.12 The names of keyboard keys, software buttons, and field names are displayed in bold type. For example: Click the Configure button. Screen names are displayed in bold italics. For example, the System Status screen. ### Important Terminology Configuration Files - Database files containing the current Access Point configuration. Configuration items include the IP Address and other network-specific values. Config files may be downloaded to the Access Point or uploaded for backup or troubleshooting. Download vs. Upload - Downloads transfer files to the Access Point. Uploads transfer files from the Access Point. The TFTP server performs file transfers in both directions. Group - A logical collection of network parameter information. For example, the System Group is composed of several related parameters. Groups can also contain Tables. All items for a given Group can be displayed with a show <Group> CLI Command. Image File - The Access Point software executed from RAM. To update an Access Point you typically download a new Image File. This file is often referred to as the “AP Image”. Parameter - A fundamental network value that can be displayed and may be changeable. For example, the Access Point must have a unique IP Address and the Wireless interface must be assigned an SSID. Change parameters with the CLI set Command, and view them with the CLI show Command. Table - Tables hold parameters for several related items. For example, you can add several potential managers to the SNMP Table. All items for a given Table can be displayed with a show <Table> CLI Command. TFTP - Refers to the TFTP Server, used for file transfers. ### Navigation and Special Keys This CLI supports the following navigation and special key functions to move the cursor along the prompt line.
Key Combination | Operation
Delete or Backspace | Delete previous character
Ctrl-A | Move cursor to beginning of line
Ctrl-E | Move cursor to end of line
Ctrl-F | Move cursor forward one character
Ctrl-B | Move cursor back one character
Ctrl-D | Delete the character the cursor is on
Ctrl-U | Delete all text to left of cursor
Ctrl-P | Go to the previous line in the history buffer
Ctrl-N | Go to the next line in the history buffer
Tab | Complete the command line
? | List available commands
### CLI Error Messages The following table describes the error messages associated with improper inputs or expected CLI behavior.
Error Message | Description
Syntax Error | Invalid syntax entered at the command prompt.
Invalid Command | A non-existent command has been entered at the command prompt.
Invalid Parameter Name | An invalid parameter name has been entered at the command prompt.
Invalid Parameter Value | An invalid parameter value has been entered at the command prompt.
Invalid Table Index | An invalid table index has been entered at the command prompt.
Invalid Table Parameter | An invalid table parameter has been entered at the command prompt.
Invalid Table Parameter Value | An invalid table parameter value has been entered at the command prompt.
Read Only Parameter | User is attempting to configure a read-only parameter.
Incorrect Password | An incorrect password has been entered in the CLI login prompt.
Download Unsuccessful | The download operation has failed due to incorrect TFTP server IP Address or file name.
Upload Unsuccessful | The upload operation has failed due to incorrect TFTP server IP Address or file name.
## ## Command Line Interface (CLI) Variations Administrators use the CLI to control Access Point operation and monitor network statistics. The AP supports two types of CLI: the Bootloader CLI and the normal CLI. The Bootloader CLI provides a limited command set, and is used when the current AP Image is bad or missing. The Bootloader CLI allows you to assign an IP Address and download a new image. Once the image is downloaded and running, the Access Point uses the normal CLI. This guide covers the normal CLI unless otherwise specified. ### Bootloader CLI The Bootloader CLI is a minimal subset of the normal CLI used to perform initial configuration of the AP. This interface is only accessible via the serial interface if the AP does not contain a software image or a download image command over TFTP has failed. The Bootloader CLI provides you with the ability to configure the initial setup parameters as well as download a software image to the device. The following functions are supported by the Bootloader CLI: ## o configuration of initial device parameters using the set command ## o show command to view the device’s configuration parameters ## o help command to provide additional information on all commands supported by the Bootloader CLI ## o reboot command to reboot the device The parameters supported by the Bootloader CLI (for viewing and modifying) are: ## o System Name ## o IP Address Assignment Type ## o IP Address ## o IP Mask ## o Gateway IP Address ## o TFTP Server IP Address ## o Image File Name (including the file extension) The following lists display the results of using the help command in the Bootloader CLI: ## Results of “help” bootloader CLI command The following lists display the results of using the show command in the Bootloader CLI: ## Results of “show” bootloader CLI command ## ## CLI Command Types This guide divides CLI Commands into two categories: Operational and Parameter Controls. ### Operational CLI Commands These commands affect Access Point behavior, such as downloading, rebooting, and so on. After entering commands (and parameters, if any) press the Enter key to execute the Command Line. Operational commands include: ## · ?: Typing a question mark lists CLI Commands or parameters, depending on usage (you do not need to type Enter after typing this command) ## · done, exit, quit: Terminates the CLI session ## · download: Uses TFTP server to download “image”, “config”, or “bootloader upgrade” files to Access Point ## · help: Displays general CLI help information or command help information, such as command usage and syntax ## · history: Remembers commands to help avoid re-entering complex statements ## · passwd: Sets the Access Point’s CLI password ## · reboot: Reboots the Access Point in the specified time ## · search: Lists the parameters in a specified Table ## · upload: Uses TFTP server to upload “config” files from Access Point to TFTP default directory or specified path #### ? (List Commands) This command can be used in a number of ways to display available commands and parameters. The following table lists each operation and provides a basic example. Following the table are detailed examples and display results for each operation.
Operation | Basic Example
Display the Command List (Example 1) | `[Device-Name]>`?
Display commands that start with specified letters (Example 2) | `[Device-Name]>`s?
Display parameters for set and show Commands (Examples 3a and 3b) | `[Device-Name]>`set ? `[Device-Name]>`show ipa?
Prompt to enter successive parameters for Commands (Example 4) | `[Device-Name]>`download ?
##### Example 1. Display Command list To display the Command List, enter ?. `[Device-Name]>`? ##### Result of “?” CLI command ##### Example 2. Display specific Commands To show all commands that start with specified letters, enter one or more letters, then ? with no space between letters and ?. [`Device-Name]>`s? ##### Result of “s?” CLI command ##### Example 3. Display parameters for set and show Example 3a allows you to see every possible parameter for the set (or show) commands. Notice from example 3a that the list is very long. Example 3b shows how to display a subset of the parameters based on initial parameter letters. ##### Example 3a. Display every parameter that can be changed `[Device-Name]>`set ? ##### Result of “set ?” CLI command ##### Example 3b. Display parameters based on letter sequence This example shows entries for parameters that start with the letter “i”. The more letters you enter, the fewer the results returned. Notice that there is no space between the letters and the question mark. `[Device-Name]>` show ipa? ##### Result of “show ipa?” CLI command `[Device-Name]>` show iparp? ##### Result of “show iparp?” CLI command ##### Example 4. Display Prompts for Successive Parameters Enter the command, a space, and then ?. Then, when the parameter prompt appears, enter the parameter value. Result: The parameter is changed and a new CLI line is echoed with the new value (in the first part of the following example, the value is the IP Address of the TFTP server). After entering one parameter, you may add another ? to the new CLI line to see the next parameter prompt, and so on until you have entered all of the required parameters. The following example shows how this is used for the download Command. The last part of the example shows the completed download Command ready for execution. `[Device-Name]>` download ? <TFTP IP Address> `[Device-Name]>` download 192.168.0.101 ? <File Name> `[Device-Name]>` download 192.168.0.101 apimage ? <file type (config/img/bootloader)> `[Device-Name]>` download 192.168.0.101 apimage img <CR> #### done, exit, quit Each of the following commands ends a CLI session: `[Device-Name]>` done `[Device-Name]>` exit `[Device-Name]>` quit #### download Downloads the specified file from a TFTP server to the Access Point. Executing download in combination with the asterisks character (“*”) will make use of the previously set TFTP parameters. Executing download without parameters will display command help and usage information. ##### 1. Syntax to download a file: `Device-Name]>`download <tftp server address> <path and filename> <file type> Example: `[Device-Name]>`download 192.168.1.100 APImage2 img ##### 2. Syntax to display help and usage information: `[Device-Name]>`download ##### 3. Syntax to execute the download Command using previously set (stored) TFTP Parameters: [`Device-Name]>`download * #### help Displays instructions on using control-key sequences for navigating a Command Line and displays command information and examples. ##### 1. Using help as the only argument: `[Device-Name]>`help ##### Results of “help” CLI command ##### 1. Complete command description and command usage can be provided by: `[Device-Name]>`help <command name> `[Device-Name]>`<command name> help #### history Shows content of Command History Buffer. The Command History Buffer stores command statements entered in the current session. To avoid re-entering long command statements, use the keyboard “up arrow” (Ctrl-P) and “down arrow” (Ctrl-N) keys to recall previous statements from the Command History Buffer. When the desired statement reappears, press the Enter key to execute, or you may edit the statement before executing it. `[Device-Name]>` history #### passwd Changes the CLI Password. `[Device-Name]>` passwd oldpassword newpassword newpassword #### reboot Reboots Access Point after specified number of seconds. Specify a value of 0 (zero) for immediate reboot. `[Device-Name]>` reboot 0 `[Device-Name]>` reboot 30 #### search Lists the parameters supported by the specified table. This list corresponds to the table information displayed in the HTTP interface. In this example, the CLI returns the list of parameters that make up an entry in the IP Access Table. [`Device-Name]>` search mgmtipaccesstbl ##### Results of “search mgmtipaccesstbl” CLI command #### upload Uploads a text-based configuration file from the AP to the TFTP Server. Executing upload with the asterisk character (“*”) will make use of the previously set/stored TFTP parameters. Executing upload without parameters will display command help and usage information. ##### 1. Syntax to upload a file: `[Device-Name]>`upload <tftp server address> <path and filename> <filetype> Example: `[Device-Name]>`upload 192.168.1.100 APconfig.sys config ##### 2. Syntax to display help and usage information: `[Device-Name]>`help upload ##### 3. Syntax to execute the upload command using previously set (stored) TFTP Parameters: `[Device-Name]>`upload * ### Parameter Control Commands The following sections cover the two Parameter Control Commands (show and set) and include several tables showing parameter properties. These commands allow you to view (show) all parameters and statistics and to change (set) parameters. ##### · show: To see any Parameter or Statistic value, you can specify a single parameter, a Group, or a Table. ##### · set: Use this CLI Command to change parameter values. You can use a single CLI statement to modify Tables, or you can modify each parameter separately. #### “show” CLI Command Displays the value of the specified parameter, or displays all parameter values of a specified group (parameter table). Groups contain Parameters and Tables. Tables contain parameters for a series of similar entities. To see a definition and syntax example, type only show and then press the Enter key. To see a list of available parameters, enter a question mark (?) after show (example: show ?). ##### · Syntax: `[Device-Name]>`show <parameter> `[Device-Name]>`show <group> `[Device-Name]>`show <table> Examples: `[Device-Name]>`show ipaddr `[Device-Name]>`show network `[Device-Name]>`show mgmtipaccesstbl #### “set” CLI Command Sets (modifies) the value of the specified parameter. To see a definition and syntax example, type only set and then press the Enter key. To see a list of available parameters, enter a space, then a question mark (?) after set (example: set?). Syntax: `[Device-Name]>`set <parameter> <value> `[Device-Name]>`set <table> <index> <argument 1> <value 1> ... <argument N> <value N> Example: `[Device-Name]>`set sysloc “Main Lobby” `[Device-Name]>`set mgmtipaccesstbl 0 ipaddr 10.0.0.10 ipmask 255.255.0.0 #### Configuring Objects that Require Reboot Certain objects supported by the Access Point require a device reboot in order for the changes to take effect. In order to inform the end-user of this behavior, the CLI provides informational messages when the user has configured an object that requires a reboot. The following messages are displayed as a result of the configuring such object or objects. ##### Example 1: Configuring objects that require the device to be rebooted The following message is displayed every time the user has configured an object that requires the device to be rebooted. `[Device-Name]>`set ipaddr 135.114.73.10 The following elements require reboot ipaddr ##### Example 2: Executing the “exit”, “quit”, or “done” commands when an object that requires reboot has been configured In addition to the above informational message, the CLI also provides a message as a result of the exit, quit, or done command if changes have been made to objects that require reboot. If you make changes to objects that require reboot and execute the exit command the following message is displayed: `[Device-Name]>`exit<CR> OR quit<CR> OR done<CR> Modifications have been made to parameters that require the device to be rebooted. These changes will only take effect after the next reboot. #### “set” and “show” Command Examples In general, you will use the CLI show Command to view current parameter values and use the CLI set Command to change parameter values. As shown in the following examples, parameters may be set individually or all parameters for a given table can be set with a single statement. ##### Example 1 - Set the Access Point IP Address Parameter Syntax: `[Device-Name]>`set <parameter name> <parameter value> Example: `[Device-Name]>` set ipaddr 10.0.0.12 Result: IP Address will be changed when you reboot the Access Point. The CLI reminds you when rebooting is required for a change to take effect. To reboot immediately, enter reboot 0 (zero) at the CLI prompt. ##### Example 2 - Create a table entry or row Use 0 (zero) as the index to a table when creating an entry. When creating a table row, only the mandatory table elements are required (comment is usually an optional table element). For optional table elements, the default value is generally applied if you do not specify a value. Syntax: `[Device-Name]>`set <table name> <table index> <element 1> <value 1> … <element n> <value n> Example: `[Device-Name]>` set mgmtipaccesstbl 0 ipaddr 10.0.0.10 ipmask 255.255.0.0 Result: A new table entry is created for IP address 10.0.0.10 with a 255.255.0.0 subnet mask. ##### Example 3 - Modify a table entry or row Use the index to be modified and the table elements you would like to modify. For example, suppose the IP Access Table has one entry and you wanted to modify the IP address: `[Device-Name]>`set mgmtipaccesstbl 1 ipaddr 10.0.0.11 You can also modify several elements in the table entry. Enter the index number and specific table elements you would like to modify. (Hint: Use the search Command to see the elements that belong to the table.) `[Device-Name]>`set mgmtipaccesstbl 1 ipaddr 10.0.0.12 ipmask 255.255.255.248 cmt “First Row” ##### Example 4 - Enable, Disable, or Delete a table entry or row The following example illustrates how to manage the second entry in a table. Syntax: `[Device-Name]>`set <Table> index status <enable, disable, delete> `[Device-Name]>`set <Table> index status <1=enable, 2=disable, 3=delete> Example: `[Device-Name]>`set mgmtipaccesstbl 2 status enable `[Device-Name]>`set mgmtipaccesstbl 2 status disable `[Device-Name]>`set mgmtipaccesstbl 2 status delete `[Device-Name]>`set mgmtipaccesstbl 2 status 2
| You may need to enable a disabled table entry before you can change the entry’s elements.
##### Example 5 - Show the Group Parameters This example illustrates how to view all elements of a group or table. Syntax: `[Device-Name]>` show <group name> Example: `[Device-Name]>`show network Result: The CLI displays network group parameters. Note show network and show ip return the same data. ##### Results of “show network” and “show ip” CLI Commands ##### Example 6 - Show Individual and Table Parameters 1. View a single parameter. Syntax: `[Device-Name]>`show <parameter name> Example: `[Device-Name]>` show ipaddr Result: Displays the Access Point IP address. ##### Result of “show ipaddr” CLI Command 2. View all parameters in a table. Syntax: `[Device-Name]>` show <table name> Example:`[Device-Name]>` show mgmtipaccesstbl Result: Displays the IP Access Table and its entries. ##### ## Using Tables & User Strings ### Working with Tables Each table element (or parameter) must be specified, as in the example below. `[Device-Name]>`set mgmtipaccesstbl 0 ipaddr 10.0.0.10 ipmask 255.255.0.0 Below are the rules for creating, modifying, enabling/disabling, and deleting table entries. ##### · Creation ##### o The table name is required. ##### o The table index is required – for table entry/instance creation the index is always zero (0). ##### o The order in which the table arguments or objects are entered in not important. ##### o Parameters that are not required can be omitted, in which case they will be assigned the default value. ##### · Modification ##### o The table name is required. ##### o The table index is required – to modify the table, “index” must be the index of the entry to be modified. ##### o Only the table objects that are to be modified need to be specified. Not all the table objects are required. ##### o If multiple table objects are to be modified the order in which they are entered is not important. ##### o If the entire table entry is to be modified, all the table objects have to be specified. ##### · Enabling/Disabling ##### o The table name is required. ##### o The table index is required – for table enabling/disabling the index should be the index of the entry to be enabled/disabled. ##### o The entry’s new state (either “enable” or “disable”) is required. ##### · Deletion ##### o The table name is required. ##### o The table index is required – for table deletion the index should be the index of the entry to be deleted. ##### o The word “delete” is required. ### Using Strings Since there are several string objects supported by the AP, a string delimiter is required for the strings to be interpreted correctly by the command line parser. For this CLI implementation, the single quote or double quote character can be used at the beginning and at the end of the string. For example: `[Device-Name]>` set sysname Lobby - Does not need quote marks `[Device-Name]>` set sysname “Front Lobby” - Requires quote marks. The scenarios supported by this CLI are:
“My Desk in the office” | Double Quotes
‘My Desk in the office’ | Single Quotes
“My ‘Desk’ in the office” | Single Quotes within Double Quotes
‘My “Desk” in the office’ | Double Quotes within Single Quotes
“Daniel’s Desk in the office” | One Single Quote within Double Quotes
‘Daniel”s Desk in the office’ | One Double Quote within Single Quotes
The string delimiter does not have to be used for every string object. The single quote or double quote only has to be used for string objects that contain blank space characters. If the string object being used does not contain blank spaces, then the string delimiters, single or double quotes, mentioned in this section are not required. ##### ## Configuring the AP using CLI commands ### Log into the AP using HyperTerminal ##### 1. Open your terminal emulation program (like HyperTerminal) and set the following connection properties: ##### § Com Port: <COM1, COM2, etc., depending on your computer> ##### § Baud rate: 9600 ##### § Data Bits: 8 ##### § Stop bits: 1 ##### § Flow Control: None ##### § Parity: None ##### 2. Under File -> Properties -> Settings -> ASCII Setup, enable the Send line ends with line feeds option. Result: HyperTerminal sends a line return at the end of each line of code. ##### 1. Enter the CLI password (default is public).
| Proxim recommends changing your default passwords immediately. To perform this operation using CLI commands, refer to Change Passwords.
### Log into the AP using Telnet The CLI commands can be used to access, configure, and manage the AP using Telnet. Follow these steps: ##### 1. Confirm that your computer’s IP address is in the same IP subnet as the AP.
| If you have not previously configured the Access Point’s IP address and do not have a DHCP server on the network, the Access Point will default to an IP address of 10.0.0.1.
##### 2. Go to the DOS command prompt on your computer. ##### 3. Type telnet <IP Address of the unit>. ##### 4. Enter the CLI password (default is public).
| Proxim recommends changing your default passwords immediately. To perform this operation using CLI commands, refer to Change Passwords.
##### ## Set Basic Configuration Parameters using CLI Commands There are a few basic configuration parameters that you may want to setup right away when you receive the AP. For example: ##### o Set System Name, Location and Contact Information ##### o Set Static IP Address for the AP ##### o Download an AP Configuration File from your TFTP Server ##### o Set up Auto Configuration ##### o Set Network Names for the Wireless Interface ##### o Configure SSID (Network Name) and VLAN Pairs, and Security Modes ##### o Download an AP Configuration File from your TFTP Server ##### o Backup your AP Configuration File #### Set System Name, Location and Contact Information `[Device-Name]>`set sysname <system name> sysloc <Unit Location> `[Device-Name]>`set sysctname <Contact Name (person responsible for system)> `[Device-Name]>`set sysctphone <Contact Phone Number> sysctemail <Contact E-mail address> `[Device-Name]>`show system ##### Result of “show system” CLI Command #### Set Static IP Address for the AP
| The IP Subnet Mask of the AP must match your network’s Subnet Mask.
`[Device-Name]>`set ipaddrtype static `[Device-Name]>`set ipaddr <fixed IP address of unit> `[Device-Name]>`set ipsubmask <IP Mask> `[Device-Name]>`set ipgw <gateway IP address> `[Device-Name]>`show network #### Change Passwords `[Device-Name]>`passwd <Old Password> <New Password> <Confirm Password> (CLI password) `[Device-Name]>`set httppasswd <New Password> (HTTP interface password) `[Device-Name]>`set snmprpasswd <New Password> (SNMP read password) `[Device-Name]>`set snmprwpasswd <New Password> (SNMP read/write) `[Device-Name]>`set snmpv3authpasswd <New Password> (SNMPv3 authentication password) `[Device-Name]>`set snmpv3privpasswd <New Password> (SNMPv3 privacy password) `[Device-Name]>`reboot 0
| Proxim strongly urges you to change the default passwords to restrict access to your network devices to authorized personnel. If you lose or forget your password settings, you can always perform the Reset to Factory Default Procedure.
#### Set Network Names for the Wireless Interface `[Device-Name]>`set wif <index 3 (Slot A) or 4 (Slot B)> netname <Network Name (SSID) for wireless interface> `[Device-Name]>`show wif ##### Results of “show wif” CLI command for an AP #### Enable and Configure TX Power Control for the Wireless Interface(s) The TX Power Control feature lets the user configure the transmit power level of the card in the AP at one of four levels: ##### · 100% of the maximum transmit power level of the card ##### · 50% ##### · 25% ##### · 12.5% Perform the following commands to enable TX Power Control and set the transmit power level: `[Device-Name]>`set txpowercontrol enable `[Device-Name]>`set wif <interface number> currenttxpowerlevel <value> Allowed values are: 1 (100%), 2 (50%), 3 (25%), 4 (12.5%) #### Configure SSID (Network Name) and VLAN Pairs, and Security Modes Perform the following command to first display the supported security modes on the wireless interfaces: `[Device-Name]>`show wifssidtbl Configure an SSID and VLAN pair, and the security mode associated with the pair. `[Device-Name]>`set wifssidtbl <index> <ssidindex> <ssid> <vlanid> <status> <secmode> <encryptkey0> <encryptkey1> <encryptkey2> <encryptkey3> <encryptkeytx> <encryptkeylength> <rekeyint> <pskey> <passphrase> Example: `[Device-Name]>`set wifssidtbl 3 2 Engineering 1050 enable WPA Depending on the configured security mode, the following parameters must be configured:
Security Mode | Key 0 | Key 1 | Key 2 | Key 3 | Tx Key | Key length | Rekeying Interval | PSK Value | PSK Pass Phrase
None | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive
802.1x | Inactive | Inactive | Inactive | Inactive | Inactive | Active | Active | Inactive | Inactive
Mixed | Inactive | Active | Inactive | Inactive | Inactive | Active | Active | Inactive | Inactive
WPA | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive
WPA-PSK | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Active | Active
WEP | Active | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive | Inactive
#####
| If you have two or more SSIDs per interface with a security mode of None, be aware that security being applied in the VLAN is not being applied in the wireless network.
#####
| If you set Security Mode to 802.1x, WPA, or Mixed, you also need to configure the RADIUS Authentication parameters. If you set Authentication Mode to Mixed, you also need to configure WEP Encryption settings.
#### Download an AP Configuration File from your TFTP Server Begin by starting your TFTP program. It must be running and configured to transmit and receive. `[Device-Name]>`set tftpfilename <file name> tftpfiletype config tftpipaddr <IP address of your TFTP server> `[Device-Name]>`show tftp (to ensure the filename, file type, and the IP address are correct) `[Device-Name]>`download * `[Device-Name]>`reboot 0 After following the complete process (above) once, you can download a file of the same name (so long as all the other parameters are the same), with the following command: `[Device-Name]>`download * #### Backup your AP Configuration File Begin by starting your TFTP program. It must be running and configured to transmit and receive. `[Device-Name]>`upload <TFTP Server IP address> <tftpfilename (such as “config.sys”)> config `[Device-Name]>`show tftp (to ensure the filename, file type, and the IP address are correct) After setting the TFTP parameters, you can backup your current file (so long as all the other parameters are the same), with the following command: `[Device-Name]>`upload * #### Set up Auto Configuration The Auto Configuration feature which allows an AP to be automatically configured by downloading a specific configuration file from a TFTP server during the boot up process. Perform the following commands to enable and set up automatic configuration:
| The configuration filename and TFTP server IP address are configured only when the AP is configured for Static IP. If the AP is configured for Dynamic IP these parameters are not used and obtained from DHCP. The default filename is “config”. The default TFTP IP address is “10.0.0.2” for AP-2000.
`[Device-Name]>`set autoconfigstatus <enable/disable> `[Device-Name]>`set autoconfigfilename <filename> `Enter the filename of the configuration file that is used if the AP is configured for Static IP.` `[Device-Name]>`set autoconfigTFTPaddr <IP address> Enter the TFTP server address that is used if the AP is configured for Static IP. ##### ## Other Network Settings There are other configuration settings that you may want to set for the AP. Some of them are listed below. ##### o Configure the AP as a DHCP Server ##### o Configure the DNS Client ##### o Maintain Client Connections using Link Integrity ##### o Change your Wireless Interface Settings ##### o Set Ethernet Speed and Transmission Mode ##### o Set Interface Management Services ##### o Configure MAC Access Control ##### o Set RADIUS Parameters ##### o Set Rogue Access Point Detection (RAD) Parameters ##### o Set VLAN/SSID Parameters
| Refer to Advanced Configuration for more information on these settings.
#### Configure the AP as a DHCP Server
| You must have at least one entry in the DHCP Server IP Address Pool Table before you can set the DHCP Server Status to Enable.
`[Device-Name]>`set dhcpstatus disable `[Device-Name]>`set dhcpippooltbl 0 startipaddr <start ip address> endipaddr <end ip address> `[Device-Name]>`set dhcpgw <gateway ip address> `[Device-Name]>`set dhcppridnsipaddr <primary dns ip address> `[Device-Name]>`set dhcpsecdnsipaddr <secondary dns ip address> `[Device-Name]>`set dhcpstatus enable `[Device-Name]>`reboot 0
| Before enabling this feature, confirm that the IP address pools you have configured are valid addresses on the network and do not overlap the addresses assigned by any other DHCP server on the network. Enabling this feature with incorrect address pools will cause problems on your network.
#### Configure the DNS Client `[Device-Name]>`set dnsstatus enable `[Device-Name]>`set dnsprisvripaddr <IP address of primary DNS server> `[Device-Name]>`set dnssecsvripaddr <IP address of secondary DNS server> `[Device-Name]>`set dnsdomainname <default domain name> `[Device-Name]>`show dns ##### Results of “show dns” CLI command #### Maintain Client Connections using Link Integrity `[Device-Name]>`show linkinttbl `(this shows the current links)` `[Device-Name]>`set linkinttbl <1-5 `(depending on what table row you wish to address)`> ipaddr <ip address of the host computer you want to check> `[Device-Name]>`set linkintpollint <the interval between link integrity checks> `[Device-Name]>`set linkintpollretx <number of times to retransmit before considering the link down> `[Device-Name]>`set linkintstatus enable `[Device-Name]>`show linkinttbl`(confirm new settings)` `[Device-Name]>`reboot 0 #### Change your Wireless Interface Settings See Interfaces for information on the parameters listed below. Dual-radio APs use index 3 for Slot A and index 4 for Slot B. ##### Operational Mode `[Device-Name]>`set wif <index> mode <see table>
mode | Operational Mode
1 | dot11b-only
2 | dot11g-only
3 | dot11bg
4 | dot11a-only
5 | dot11g-wifi
##### Autoc hannel Select (ACS) ACS is enabled by default. Reboot after disabling or enabling ACS. `[Device-Name]>`set wif <index> autochannel <enable/disable> `[Device-Name]>`reboot 0 ##### Enable/Disable Closed System `[Device-Name]>`set wif <index> closedsys <enable/disable> ##### Enable/Disable Interference Robustness (802.11b Only) `[Device-Name]>`set wif <index> interrobust <enable/disable> ##### Enable/Disable Load Balancing (802.11b Only) `[Device-Name]>`set wif <index> ldbalance <enable/disable> ##### Enable/Disable Medium Density Distribution (802.11b Only) `[Device-Name]>`set wif <index> meddendistrib <enable/disable> ##### Set the Distance Between APs (802.11b Only) `[Device-Name]>`set wif <index> distaps <large, medium, small, minicell, microcell> `[Device-Name]>`reboot 0
| The distance between APs should not be approximated. It is calculated by means of a manual Site Survey, in which an AP is set up and clients are tested throughout the area to determine signal strength and coverage, and local limits such as physical interference are investigated. From these measurements the appropriate cell size and density is determined, and the optimum distance between APs is calculated to suit your particular business requirements.
##### Set the Multicast Rate (802.11b Only) `[Device-Name]>`set wif <index> multrate <1,2,5.5,11 (Mbits/sec)>
| The Distance Between APs must be set before the Multicast Rate.
#### Set Ethernet Speed and Transmission Mode `[Device-Name]>`set etherspeed <value`(see below)`> `[Device-Name]>`reboot 0
Ethernet Speed and Transmission Mode | Value
10 Mbits/sec - half duplex | 10halfduplex
10 Mbits/sec - full duplex | 10fullduplex
10 Mbits/sec - auto duplex | 10autoduplex
100 Mbits/sec - half duplex | 100halfduplex
100 Mbits/sec - full duplex | 100fullduplex
Auto Speed - half duplex | autohalfduplex
Auto Speed - auto duplex | autoautoduplex (default)
#### Set Interface Management Services ##### Edit Management IP Access Table `[Device-Name]>`set mgmtipaccesstbl <index> ipaddr <IP address> ipmask <subnet mask> ##### Configure Management Ports `[Device-Name]>`set snmpifbitmask <`(see below)`> `[Device-Name]>`set httpifbitmask <`(see below)`> `[Device-Name]>`set telifbitmask <`(see below)`> Choose from the following values:
Interface bitmask | Description
0 or 2 = disable (all interfaces) | All management channels disabled
1 or 3 = Ethernet only | Ethernet only enabled
4 or 6 = Wireless A only | Wireless A only enabled
8 or 10 = Wireless B only | Wireless B only enabled
12 = Wireless A and Wireless B | Wireless A and Wireless B enabled
13 or 15 = all interfaces | All management channels enabled
####
##### Set Communication Ports `[Device-Name]>`set httpport <HTTP port number (default is 80)> `[Device-Name]>`set telport <Telnet port number (default is 23)> ##### Configure Secure Socket Layer (HTTPS) Enabling SSL and configuring a passphrase allows encrypted Secure Socket Layer communications to the AP through the HTTPS interface. ##### [Device-Name]>set sslstatus <enable/disable> The user must change the SSL passphrase when uploading a new certificate/private key pair, which will have a corresponding passphrase. [Device-Name]>set sslpassphrase <SSL certificate passphrase> ##### [Device-Name]>show http To view all HTTP configuration information including SSL. HTTP Group Parameters ===================== httpifbitmask : 15 httppasswd : ******** httpport : 80 httphelplink : file:///C:/Program Files/ORiNOCO/AP2000/HTML/home.htm httpsetupwiz : disable sslstatus : enable sslpassphrase : ******** ##### Set Telnet Session Timeouts `[Device-Name]>`set tellogintout <time in seconds between 1 and 300 `(default is 30)`> `[Device-Name]>`set telsessiontout <time in seconds between 1 and 36000 `(default is 900)`> ##### Configure Serial Port Interface
| To avoid unexpected performance issues, leave Flow Control at the default setting (none) unless you are sure what this setting should be.
`[Device-Name]>`set serbaudrate <2400, 4800, 9600, 19200, 38400, 57600> `[Device-Name]>`set serflowctrl <none, xonxoff> `[Device-Name]>`show serial ##### Result of “show serial” CLI Command #### Configure Syslog `[Device-Name]>`set syslogpriority <1-7 (default is 6)> `[Device-Name]>`set syslogstatus <enable/disable> #### Configure Intra BSS `[Device-Name]>`set intrabssoptype <passthru (default)/block)> #### Configure MAC Access Control ##### Setup MAC (Address) Access Control `[Device-Name]>`set macaclstatus enable`` `[Device-Name]>`set macacloptype <passthru, block> `[Device-Name]>`reboot 0 ##### Add an Entry to the MAC Access Control Table `[Device-Name]>`set macacltbl <index> macaddr <MAC Address> status enable `[Device-Name]>`show macacltbl ##### Disable or Delete an Entry in the MAC Access Control Table `[Device-Name]>`set macacltbl <index> status <disable/delete> `[Device-Name]>`show macacltbl
| For larger networks that include multiple Access Points, you may prefer to maintain this list on a centralized location using the RADIUS parameters (see Set RADIUS Parameters).
#### Set RADIUS Parameters ##### Configure RADIUS Authentication server `[Device-Name]>`set radiustbl <index> status enable seraddrfmt <ipaddr or name> ipaddr <RADIUS IP address or name> port <user defined> ssecret <user defined> responsetm <1 to 10 seconds> maxretx <0 to 4 times> `[Device-Name]>`show radiustbl ##### Results of “show radiustbl” CLI command ##### Enable RADIUS MAC Access Control `[Device-Name]>`set radmacaccctrl enable `[Device-Name]>`reboot 0 ##### Set MAC Address Format Type `[Device-Name]>`set radmacaddrformat <dashdelimited, colondelimited, singledashdelimited, nodelimiter> ##### Set Authorization Lifetime (MAC-based authentication only) `[Device-Name]>`set radauthlifetm <900-43200 seconds; default is 0> ##### Enable RADIUS Accounting `[Device-Name]>`set radaccstatus enable `[Device-Name]>`set radaccinactivetmr <inactivity timer in minutes> `[Device-Name]>`show radius ##### Result of “show radius” CLI Command ##### Configure RADIUS Accounting server `[Device-Name]>`set radacctbl <index> status <enable> seraddrfmt <ipaddr or name> ipaddr <RADIUS IP address or name> port <user defined> ssecret <user defined> responsetm <1 to 4 seconds> maxretx <1 to 10 times> `[Device-Name]>`show radacctbl ##### Results of “show radacctbl” CLI command #### Set Rogue Access Point Detection (RAD) Parameters The Rogue AP Detection (RAD) feature enables an additional security level for wireless LAN deployments. The RAD feature provides a mechanism for detecting Rogue Access Points by utilizing the coverage of the trusted Access Point deployment. The Rogue AP Scan employs background scanning using low-level 802.11 scanning functions for effective wireless detection of Access Points in its coverage area with minimal impact on the normal operation of the Access Point. The set radstatus command enables Rogue Access Point Detection. The scan repetition duration (radscanint) is also configurable.If the Access Point uses directional antennas to provide directional coverage, then the interface bitmask (radifbitmask) can be configured to maximize the scanning coverage area. `[Device-Name]>`set radstatus enable `[Device-Name]>`set radscanint <15-1440> `[Device-Name]>`set radifbitmask <4 (WiF A), 8 (WiF B), or 12 (both interfaces)> `[Device-Name]>`show rad ##### Results of “show rad” CLI command #### Set VLAN/SSID Parameters ##### Enable VLAN Management `[Device-Name]>`set vlanstatus enable `[Device-Name]>`set vlanmgmtid <1-4094> [Device-Name]>show vlandidtbl (to review your settings) [Device-Name]>reboot 0 ##### Disable VLAN Management [Device-Name]>set vlanstatus disable or [Device-Name]>set vlanmgmtid 0 [Device-Name]>reboot 0 ##### Add an Entry to the VLAN ID Table `[Device-Name]>`set vlanidtbl <index number; see table> id <1-4094, -1=untagged> ssid <enter network name> [Device-Name]>show vlandidtbl (to review your settings) [Device-Name]>reboot 0
| 16 VLAN/SSID pairs are available for 802.11b/g APs and APs with an 11a Upgrade Kit. 802.11b APs and APs with a 5 GHz Upgrade Kit only support one VLAN/SSID pair.
##### ## CLI Monitoring Parameters Using the show command with the following table parameters will display operating statistics for the AP (these are the same statistics that are described in Monitor Information for the HTTP Web interface). ##### · staticmp: Displays the ICMP Statistics. ##### · statarptbl: Displays the IP ARP Table Statistics. ##### · statbridgetbl: Displays the Learn Table. ##### · statiapp: Displays the IAPP Statistics. ##### · statradius: Displays the RADIUS Authentication Statistics. ##### · statif: Displays information and statistics about the Ethernet and wireless interfaces. ##### · stat802.11: Displays additional statistics for the wireless interfaces. ##### · statethernet: Displays additional statistics for the Ethernet interface. ##### · statmss: Displays station statistics and Wireless Distribution System links. ##### ## Parameter Tables Objects contain groups that contain both parameters and parameter tables. Use the following Tables to configure the Access Point. Columns used on the tables include: ##### § Name - Parameter, Group, or Table Name ##### § Type - Data type ##### § Values - Value range, and default value, if any ##### § Access = access type, R = Read Only (show), RW = Read-Write (can be “set”), W = Write Only ##### § CLI Parameter - Parameter name as used in the Access Point Access Point network objects are associated with Groups. The network objects are listed below and associated parameters are described in the following Parameter Tables: ##### · System Parameters - Access Point system information ##### o Inventory Management Information - Hardware, firmware, and software version information ##### · Network Parameters - IP and Network Settings ##### o IP Configuration Parameters - Configure the Access Point’s IP settings ##### § DNS Client for RADIUS Name Resolution - Configure the Access Point as a DNS client ##### o DHCP Server Parameters - Enable or disable dynamic host configuration ##### o Link Integrity Parameters - Monitor link status ##### · Interface Parameters - Configure Wireless and Ethernet settings ##### o Wireless Interface Parameters ##### § Wireless Distribution System (WDS) Parameters - Configure the WDS partnerships ##### o Wireless Interface SSID/VLAN/Security Parameters - Configure the SSID and VLAN pairs and the security mode for each pair. Up to 16 pairs can be configured per wireless interface. ##### o Wireless Distribution System (WDS) Security Table Parameters ##### o Ethernet Interface Parameters - Set the speed and duplex of the Ethernet port ##### · Management Parameters - Control access to the AP’s management interfaces ##### o SNMP Parameters - Set read and read/write passwords ##### o HTTP (web browser) Parameters - Set up the graphical web browser interface. If required, enable SSL and configure the SSL certificate passphrase. ##### o Telnet Parameters - Telnet Port setup ##### o Serial Port Parameters - Serial Port setup ##### o TFTP Server Parameters - Set up for file transfers; specify IP Address, file name, and file type ##### o IP Access Table Parameters - Configure range of IP addresses that can access the AP ##### o Auto Configuration Parameters - Configure the Auto Configuration feature which allows an AP to be automatically configured by downloading a configuration file from a TFTP server during boot up. ##### · Filtering Parameters ##### o Ethernet Protocol Filtering Parameters - Control network traffic based on protocol type ##### o Static MAC Address Filter Table - Enable and disable specific addresses ##### o Proxy ARP Parameters - Enable or disable proxy ARP for wireless clients ##### o IP ARP Filtering Parameters - Control which ARP messages are sent to wireless clients based on IP settings ##### o Broadcast Filtering Table - Control the type of broadcast packets forwarded to the wireless network ##### o TCP/UDP Port Filtering - Filter IP packets based on TCP/UDP port ##### · Alarms Parameters ##### o SNMP Table Host Table Parameters - Enter the list of IP addresses that will receive alarms from the AP ##### o Syslog Parameters - Configure the AP to send Syslog information to network servers ##### · Bridge Parameters ##### o Spanning Tree Parameters - Used to help prevent network loops ##### o Storm Threshold Parameters - Set threshold for number of broadcast packets ##### o Intra BSS Subscriber Blocking - Enable or disable peer to peer traffic on the same AP ##### o Packet Forwarding Parameters - Redirect traffic from wireless clients to a specified MAC address ##### · Security Parameters - Access Point security settings ##### o Refer to Configure SSID (Network Name) and VLAN Pairs, and Security Modes for information on configuring security modes for the AP. ##### o MAC Access Control Parameter - Control wireless access based on MAC address ##### · RADIUS Parameters ##### o Primary and Backup RADIUS Server Table Parameters - RADIUS Authentication and Accounting information ##### · Rogue Access Point Detection (RAD) Parameters - Enable and configure Rogue Access Point Detection. ##### · VLAN/SSID Parameters - Configure mutiple subnetworks based on VLAN ID and SSID pairs. ##### · Other Parameters ##### o IAPP Parameters - Enable or disable the Inter-Access Point Protocol ##### o SpectraLink VoIP Parameters (802.11b and bg Modes Only) - Enable or disable SpectraLink Voice over IP feature ### System Parameters
Name | Type | Values | Access | CLI Parameter
System | Group | N/A | R | system
Name | DisplayString | User Defined | RW | sysname
Location | DisplayString | User Defined | RW | sysloc
Contact Name | DisplayString | User Defined | RW | sysctname
Contact E-mail | DisplayString | User Defined | RW | sysctemail
Contact Phone | DisplayString | User Defined max 254 characters | RW | sysctphone
FLASH Backup Interval | Integer | 0 - 65535 seconds | RW | sysflashbckint
Flash Update |  | 0 1 | RW | sysflashupdate
System OID | DisplayString | N/A | R | sysoid
Descriptor | DisplayString | System Name, flash version, S/N, bootloader version | R | sysdescr
Up Time | Integer | dd:hh:mm:ss dd – days hh – hours mm – minutes ss – seconds | R | sysuptime
Emergency Restore to defaults |  | Resets all parameters to default factory values | RW | sysresettodefaults Note: You must enter the following command twice to reset to defaults: set sysresettodefaults 1
#### Inventory Management Information
Name | Type | Values | Access | CLI Parameter
System Inventory Management | Subgroup | N/A | R | sysinvmgmt
Component Table | Subgroup | N/A | R | sysinvmgmtcmptbl
Component Interface Table | Subgroup | N/A | R | sysinvmgmtcmpiftbl
###
| The inventory management commands display advanced information about the AP’s installed components. You may be asked to report this information to a representative if you contact customer support.
### Network Parameters #### IP Configuration Parameters
Name | Type | Values | Access | CLI Parameter
Network | Group | N/A | R | network
IP Configuration | Group | N/A | R | ip (Note: The network and ip parameters display the same information)
IP Address | IpAddress | User Defined | RW | ipaddr
IP Mask | IpAddress | User Defined | RW | ipmask
Default Router IP Address | IpAddress | User Defined | RW | ipgw
Default TTL | Integer | User Defined (seconds) 64 (default) | RW | ipttl
Address Type | Integer | static dynamic (default) | RW | ipaddrtype
#####
| The IP Address Assignment Type (ipaddrtype) must be set to static before the IP Address (ipaddr), IP Mask (ipmask) or Default Gateway IP Address (ipgw) values can be entered.
##### DNS Client for RADIUS Name Resolution
Name | Type | Values | Access | CLI Parameter
DNS Client | Group | N/A | R | dns
DNS Client status | Integer | enable disable (default) | RW | dnsstatus
Primary DNS Server IP Address | IpAddress | User Defined | RW | dnspridnsipaddr
Secondary DNS Server IP Address | IpAddress | User Defined | RW | dnssecdnsipaddr
Default Domain Name | Integer32 | User Defined (up to 254 characters) | RW | dnsdomainname
#### DHCP Server Parameters
Name | Type | Values | Access | CLI Parameter
DHCP Server | Group | N/A | R | dhcp
DHCP Server Status | Integer | enable (1) (default) disable (2) delete (3) | RW | dhcpstatus
Gateway IP Address | IpAddress | User Defined | RW | dhcpgw
Primary DNS IP Address | IpAddress | User Defined | RW | dhcppridnsipaddr
Secondary DNS IP Address | IpAddress | User Defined | RW | dhcpsecdnsipaddr
Number of IP Pool Table Entries | Integer32 | N/A | R | dhcpippooltblent
#####
| The DHCP Server (dhcpstatus) can only be enabled after a DHCP IP Pool table entry has been created.
##### DHCP Server table for IP pools
Name | Type | Values | Access | CLI Parameter
DHCP Server IP Address Pool Table | Table | N/A | R | dhcpippooltbl
Table Index | Integer | User Defined | N/A | index
Start IP Address | IpAddress | User Defined | RW | startipaddr
End IP Address | IpAddress | User Defined | RW | endipaddr
Width | Integer | User Defined | RW | width
Default Lease Time (optional) | Integer32 | > 0 86400 sec (default) | RW | defleasetm
Maximum Lease Time (optional) | Integer32 | > 0 86400 sec (default) | RW | maxleasetm
Comment (optional) | DisplayString | User Defined | RW | cmt
Status (optional) | Integer | enable (1) disable (2) delete (3) | RW | status
####
| Set either End IP Address or Width (but not both) when creating an IP address pool.
#### Link Integrity Parameters
Name | Type | Values | Access | CLI Parameter
Link Integrity | Group | N/A | R | linkint
Link Integrity Status | Integer | enable disable (default) | RW | linkintstatus
Link Integrity Poll Interval | Integer | 500 - 15000 ms (in increments of 500ms) 500 ms (default) | RW | linkintpollint
Link Integrity Poll Retransmissions | Integer | 0 - 255 5 (default) | RW | linkintpollretx
##### Link Integrity IP Target Table
Name | Type | Values | Access | CLI Parameter
Link Integrity IP Target Table | Table | N/A | R | linkinttbl
Table Index | Integer | 1-5 | N/A | index
Target IP Address | IpAddress | User Defined | RW | ipaddr
Comment (optional) | DisplayString | User Defined (up to 254 characters) | RW | cmt
Status (optional) | Integer | enable disable (default) delete | RW | status
### Interface Parameters #### Wireless Interface Parameters The wireless interface group parameter is wif. For Dual-radio APs, Slot A uses table index 3 and Slot B uses table index 4. ##### Common Parameters to 802.11a, 802.11b, and 802.11b/g APs
Name | Type | Values | Access | CLI Parameter
Wireless Interfaces | Group | N/A | R | wif
Table Index | Integer | 3 (Slot A) or 4 (Slot B) | R | index
Network Name | DisplayString | 2 – 31 characters My Wireless Network (default) | RW | netname
Auto Channel Select (ACS)1 | Integer | enable (default) disable | RW | autochannel
DTIM Period | Integer | 1 – 255 1 = default | RW | dtimperiod
RTS/CTS Medium Reservation | Integer | 0 – 2347 Default is 2347 (off) | RW | medres
MAC Address | PhyAddress | 12 hex digits | R | macaddr
Closed System | Integer | enable disable (default) | RW | closedsys
Supported Frequency Channels | Octet String | Depends on Regulatory Domain | R | suppchannels
Load Balancing | Integer | enable (default) disable | RW | ldbalance
Note 1: For 802.11a APs in Europe, Auto Channel Select is a read-only parameter; it is always enabled. ##### 802.11a Only Parameters
Name | Type | Values | Access | CLI Parameter
Operating Frequency Channel | Integer | Varies by regulatory domain and country. See 802.11a Channel Frequencies | RW | channel
Supported Data Rates | Octet String | See Transmit Rate, below | R | suppdatarates
Transmit Rate | Integer32 | 0 - Auto Fallback (default) 6 Mbits/sec 9 Mbits/sec 12 Mbits/sec 18 Mbits/sec 24 Mbits/sec 36 Mbits/sec 48 Mbits/sec 54 Mbits/sec | RW | txrate
Physical Layer Type | Integer | ofdm (orthogonal frequency division multiplexing) for 802.11a | R | phytype
##### 802.11b Only Parameters
Name | Type | Values | Access | CLI Parameter
Distance between APs | Integer | large (default) medium small minicell microcell | RW | distaps
Interference Robustness | Integer | enable (default) disable | RW | interrobust
Operating Frequency Channel | Integer | 1 - 14; available channels vary by regulatory domain/country; see 802.11b Channel Frequencies | RW | channel
Multicast Rate | Integer | 1 Mbits/sec (1) 2 Mbits/sec (2) (default) 5.5 Mbits/sec (3) 11 Mbits/sec (4) | RW | multrate
Closed Wireless System | Integer | enable disable (default) | RW | closedsys
Medium Distribution | Integer | enable (default) disable | RW | meddendistrib
MAC Address | PhyAddress | 12 hex digits | R | macaddr
Supported Data Rates | Octet String | 1 Mbits/sec 2 Mbits/sec 5.5 Mbits/sec 11 Mbits/sec | R | suppdatarates
Transmit Rate | Integer32 | 0 (auto fallback - default) 1 Mbits/sec 2 Mbits/sec 5.5 Mbits/sec 11 Mbits/sec | RW | txrate
Supported Frequency Channels | Octet String | Depends on Regulatory Domain | R | suppchannels
Physical Layer Type | Integer | dsss (direct sequence spread spectrum) for 802.11b | R | phytype
Regulatory Domain List | DisplayString | U.S./Canada -- FCC Europe -- ETSI Japan -- MKK | R | regdomain
#####
| There is an inter-dependent relationship between the Distance between APs and the Multicast Rate. In general, larger systems operate a lower average transmit rates.
###
Distance between APs | Multicast Rate
Large | 1 and 2 Mbits/sec
Medium | 1, 2, and 5.5 Mbits/sec
Small | 1, 2, 5.5 and 11 Mbits/sec
Minicell | 1, 2, 5.5 and 11 Mbits/sec
Microcell | 1, 2, 5.5 and 11 Mbits/sec
##### 802.11b/g O nly Parameters
Name | Type | Values | Access | CLI Parameter
Wireless Operational Mode | Integer | dot11b-only dot11g-only dot11bg (default) dot11g-wifi | RW | mode
Operating Frequency Channel | Integer | 1 - 14; available channels vary by regulatory domain/country; see 802.11g Channel Frequencies | RW | channel
Supported Data Rates | Octet String | See Transmit Rate, below | R | suppdatarates
Transmit Rate | Integer32 | For 802.11b-only mode: 0 (auto fallback - default) 1 Mbits/sec 2 Mbits/sec 5.5 Mbits/sec 11 Mbits/sec For 802.11g-only mode: 0 (auto fallback - default) 6 Mbits/sec 9 Mbits/sec 12 Mbits/sec 18 Mbits/sec 24 Mbits/sec 36 Mbits/sec 48 Mbits/sec 54 Mbits/sec For 802.11g-wifi and 802.11bg modes: 0 (auto fallback - default) 1 Mbits/sec 2 Mbits/sec 5.5 Mbits/sec 11 Mbits/sec 6 Mbits/sec 9 Mbits/sec 12 Mbits/sec 18 Mbits/sec 24 Mbits/sec 36 Mbits/sec 48 Mbits/sec 54 Mbits/sec | RW | txrate
Physical Layer Type | Integer | ERP (Extended Rate Protocol) | R | phytype
##### Wireless Distribution System (WDS) Parameters
Name | Type | Values | Access | CLI Parameter
WDS Table | Table | N/A | R | wdstbl
Port Index | Integer | 3.1 - 3.6 (Wireless) | R | portindex
Status | Integer | enable, disable | RW | status
Partner MAC Address | PhysAddress | User Defined | RW | partnermacaddr
#### Wireless Interface SSID/VLAN/Security Parameters The Wireless Interface SSID table manages the SSID and VLAN pairs and the security modes of those pairs.
| The ability to configure up to 16 VLAN/SSID pairs and to configure a security mode per SSID is available only for 802.11b/g APs and 802.11a Upgrade Kit APs.
802.11b APs do not support multiple VLAN/SSID pairs. APs with the 802.11a card support multiple VLAN/SSID pairs, but do not support the security mode per SSID capability.
Name | Type | Values | Access | CLI Parameter
Wireless Interface SSID Table | Table | N/A | R | wifssidtbl
Table Index | Integer | Primary WNIC = 3 Secondary WNIC = 4 | R | index
Table Index | Integer | 1 - 16 (SSID index) | R | ssidindex
SSID | DisplayString | 0 - 32 characters | RW | ssid
VLAN ID | VlanId | -1 - 4094 | RW | vlanid
Table Row Status | RowStatus | enable, disable | RW | status
Security Mode | Integer | none dot1x mixed wpa wpa-psk wep | RW | secmode
Supported Security Modes | DisplayString | none dot1x mixed wpa wpa-psk wep | R | supsecmode
Encryption Key 0 | WEPKeyType | User Defined | WO | encryptkey0
Encryption Key 1 | WEPKeyType | User Defined | WO | encryptkey1
Encryption Key 2 | WEPKeyType | User Defined | WO | encryptkey2
Encryption Key 3 | WEPKeyType | User Defined | WO | encryptkey3
Encryption Transmit Key | Integer32 | 0 - 3 | RW | encryptkeytx
Encryption Key Length | Integer | 64 128 152 | RW | encryptkeylength
Re-keying Interval | Integer32 | 60 – 65535 seconds default is 900 sec | RW | rekeyint
Pre-Shared Key 1 | OctetString | Size 32 | WO | pskey
PSK Pass Phrase 1 | DisplayString | 0 to 255 characters 2 | WO | passphrase
Note 1: Configure either the Pre-Shared Key or the PSK Pass Phrase (but not both) to create a pre-shared key for WPA-PSK mode. Setting Pre-Shared Key will override a previous PSK Pass Phrase setting. Similarly, setting PSK Pass Phrase will override a previous Pre-Shared Key setting. Note 2: Proxim recommends using a PSK Pass Phrase of at least 13 characters to ensure that the generated key cannot be easily deciphered by network infiltrators. ##### Wireless Distribution System (WDS) Security Table Parameters The WDS Security Table manages WDS related security objects.
Name | Type | Values | Access | CLI Parameter
WDS Security Table | Table | N/A | R | wdssectbl
Table Index | Integer | Primary WNIC = 3 Secondary WNIC = 4 | R | index
Security Mode | Integer | none, wep | RW | secmode
Encryption Key 0 | WEPKeyType | N/A | WO | encryptkey0
#### Ethernet Interface Parameters
Name | Type | Values | Access | CLI Parameter
Ethernet Interface | Group | N/A | R | ethernet
Speed | Integer | 10halfduplex 10fullduplex 10autoduplex 100halfduplex 100fullduplex autohalfduplex autoautoduplex (default) | RW | etherspeed
MAC Address | PhyAddress | N/A | R | ethermacaddr
### Management Parameters #### Secure Management Parameters
Name | Type | Values | Access | CLI Parameter
Secure Management | Integer | Enable/Disable | RW | securemgmtstatus
#### SNMP Parameters
Name | Type | Values | Access | CLI Parameter
SNMP | Group | N/A | R | snmp
SNMP Management Interface Bitmask | Interface Bitmask | 0 or 2 - no interfaces (disable) 1 or 3 - Ethernet 4 or 6 - Wireless A 8 or 10 - Wireless B 12 = Wireless A & B 13 or 15 - all interfaces (default is 15) | RW | snmpifbitmask
Read Password | DisplayString | User Defined public (default) max 63 characters | W | snmprpasswd
Read/Write Password | DisplayString | User Defined public (default) max 63 characters | W | snmprwpasswd
SNMPv3 Authentication Password | DisplayString | User Defined public (default) max 63 characters | W | snmpv3authpasswd
SNMPv3 Privacy Password | DisplayString | User Defined public (default) max 63 characters | W | snmpv3privpasswd
#### HTTP (web browser) Parameters
Name | Type | Values | Access | CLI Parameter
HTTP | Group | N/A | R | http
HTTP Management Interface Bitmask | Interface Bitmask | 0 or 2 - no interfaces (disable) 1 or 3 - Ethernet 4 or 6 - Wireless A 8 or 10 - Wireless B 12 = Wireless A & B 13 or 15 - all interfaces (default is 15) | RW | httpifbitmask
HTTP Password | DisplayString | User Defined max 64 characters | W | httppasswd
HTTP Port | Integer | User Defined Default = 80 | RW | httpport
Help Link | DisplayString | User Defined | RW | httphelplink
SSL Status | Integer | Enable/Disable | RW | sslstatus
SSL Certificate Passphrase | DisplayString | User Defined | Write-only | sslpassphrase
####
| The default path for the Help files is C:/Program Files/ORiNOCO/AP/HTML/home.htm. (Use the forward slash character ("/") rather than the backslash character ("\") when configuring the Help Link location.) The AP Help information is available in English, French, German, Italian, Spanish, and Japanese.
#### Telnet Parameters
Name | Type | Values | Access | CLI Parameter
Telnet | Group | N/A | R | telnet
Telnet Management Interface Bitmask | Interface Bitmask | 0 or 2 - no interfaces (disable) 1 or 3 - Ethernet 4 or 6 - Wireless A 8 or 10 - Wireless B 12 = Wireless A & B 13 or 15 - all interfaces (default is 15) | RW | telifbitmask
Telnet Port | Integer | User Defined 23 (default) | RW | telport
Telnet Login Inactivity Time-out | Integer | 1 – 300 seconds 30 sec (default) | RW | tellogintout
Telnet Session Idle Time-out | Integer | 1 - 900 seconds 900 sec (default) | RW | telsessiontout
#### Serial Port Parameters
Name | Type | Values | Access | CLI Parameter
Serial | Group | N/A | R | serial
Baud Rate | Integer | 2400, 4800, 9600 (default), 19200, 38400, 57600 | RW | serbaudrate
Data Bits | Integer | 8 | R | serdatabits
Parity | Integer | none | R | serparity
Stop Bits | Integer | 1 | R | serstopbits
Flow Control | Value | none (default) xonxoff | RW | serflowctrl
#### Auto Configuration Parameters These parameters relate to the Auto Configuration feature which allows an AP to be automatically configured by downloading a specific configuration file from a TFTP server during the boot up process.
Name | Type | Values | Access | CLI Parameter
Auto Configuration | Group | N/A | R | autoconfig
Auto Configuration Status | Integer | enable (default) disable | RW | autoconfigstatus
Auto Config File Name | DisplayString | User Defined | RW | autoconfigfilename
Auto Config TFTP Server IP Address | IpAddress | User Defined | RW | autoconfigTFTPaddr
#### TFTP Server Parameters These parameters relate to upload and download commands. When a user executes an upload and/or download Command, the specified arguments are stored in TFTP parameters for future use. If nothing is specified in the command line when issuing subsequent upload and/or download commands, the stored arguments are used.
Name | Type | Values | Access | CLI Parameter
TFTP | Group | N/A | R | tftp
TFTP Server IP Address | IpAddress | User Defined | RW | tftpipaddr
TFTP File Name | DisplayString | User Defined | RW | tftpfilename
TFTP File Type | Integer | img config bootloader | RW | tftpfiletype
#### IP Access Table Parameters When creating table entries, you may either specify the argument name followed by argument value or simply entering the argument value. When only the argument value is specified, then enter the values in the order depicted by the following table. CLI applies default values to the omitted arguments. Due to the nature of the information, the only argument that can be omitted is the “comment” argument.
Name | Type | Values | Access | CLI Parameter
IP Access Table | Table | N/A | R | mgmtipaccesstbl
Table Index | Integer | User Defined | N/A | index
IP Address | IpAddress | User Defined | RW | ipaddr
IP Mask | IpAddress | User Defined | RW | ipmask
Comment (optional) | DisplayString | User Defined | RW | cmt
Status (optional) | Integer | enable (default) disable delete | RW | status
### Filtering Parameters #### Ethernet Protocol Filtering Parameters
Name | Type | Values | Access | CLI Parameter
Ethernet Filtering | Group | N/A | R | etherflt
Filtering Interface Bitmask | Interface Bitmask | 0 or 2 - no interfaces (disable) 1 or 3 - Ethernet 4 or 6 - Wireless A 8 or 10 - Wireless B 12 = Wireless A & B 13 or 15 - all interfaces (default is 15) | RW | etherfltifbitmask
Operation Type |  | passthru block | RW | etherfltoptype
##### Ethernet Protocol Filtering Table Identify the different filters by using the table index.
Name | Type | Values | Access | CLI Parameter
Ethernet Protocol Filtering Table | Table | N/A | R | etherflttbl
Table Index | N/A | N/A | R | index
Protocol Number | Octet String | N/A | RW | protonumber
Protocol Name (optional) | DisplayString |  | RW | protoname
Status (optional) | Integer | enable (1) disable (2) delete (3) | RW | status
####
| The filter Operation Type (passthru or block) applies only to the protocol filters that are enabled in this table.
####
| The AP requires a reboot for changes to the Ethernet Protocol Filtering Table to take effect.
#### Static MAC Address Filter Table
Name | Type | Values | Access | CLI Parameter
Static MAC Address Filter Table | Table | N/A | R | staticmactbl
Table Index | N/A | N/A | R | index
Static MAC Address on Wired Network | PhysAddress | User Defined | RW | wiredmacaddr
Static MAC Address Mask on Wired Network | PhysAddress | User Defined | RW | wiredmask
Static MAC Address on Wireless Network | PhysAddress | User Defined | RW | wirelessmacaddr
Static MAC Address Mask on Wireless Network | PhysAddress | User Defined | RW | wirelessmask
Comment (optional) | DisplayString | max 255 characters | RW | cmt
Status (optional) | Integer | enable (default) disable delete | RW | status
#### Proxy ARP Parameters
Name | Type | Values | Access | CLI Parameter
Proxy ARP | Group | N/A | R | parp
Status | Integer | enable disable (default) | RW | parpstatus
#### IP ARP Filtering Parameters
Name | Type | Values | Access | CLI Parameter
IP ARP Filtering | Group | N/A | R | iparp
Status | Integer | enable disable (default) | RW | iparpfltstatus
IP Address | IpAddress | User Defined | RW | iparpfltipaddr
Subnet Mask | IpAddress | User Defined | RW | iparpfltsubmask
#### Broadcast Filtering Table
Name | Type | Values | Access | CLI Parameter
Broadcast Filtering Table | Table | N/A | R | broadcastflttbl
Index | Integer | 1-5 | N/A | index
Protocol Name | DisplayString | N/A | R | protoname
Direction | Integer | ethertowireless wirelesstoether both (default) | RW | direction
Status | Integer | enable disable (default) | RW | status
#### TCP/UDP Port Filtering The following parameters are used to enable/disable the Port filter feature.
Name | Type | Values | Access | CLI
Port Filtering | Group | N/A | R | portflt
Port Filter Status | Integer | enable (default) disable | RW | portfltstatus
##### TCP/UDP Port Filtering Table The following parameters are used to configure TCP/UDP Port filters.
Name | Type | Values | Access | CLI
Port Filtering Table | Table | N/A | R | portflttbl
Table Index | N/A | User Defined (there are also 4 pre-defined indices, see Port Number below for more information) | R | index
Port Type | Octet String | tcp udp tcp/udp | RW | porttype
Port Number | Octet String | User Defined (there are also 4 pre-defined protocols: Index 1: NetBios Name Service – 137, Index 2: NetBios Datagram Service – 138, Index 3: NetBios Session Service – 139, Index 4: SNMP Service – 161) | RW | portnum
Protocol Name | DisplayString | User Defined (there are also 4 pre-defined protocols, see Port Number above) | RW | protoname
Interface Bitmask | Integer32 | 0 or 2 - no interfaces (disable) 1 or 3 - Ethernet 4 or 6 - Wireless A 8 or 10 - Wireless B 12 = Wireless A & B 13 or 15 - all interfaces (default is 15) | RW | ifbitmask
Status (optional) | Integer | enable (default for new entries) disable (default for pre-defined entries) delete | RW | status
### Alarms Parameters #### SNMP Table Host Table Parameters When creating table entries, you may either specifying the argument name followed by argument value. CLI applies default values to the omitted arguments. Due to the nature of the information, the only argument that can be omitted is the “comment” argument.
| Up to 10 entries can be added to the SNMP Trap Host Table.
###
Name | Type | Values | Access | CLI Parameter
SNMP Trap Host Table | Table | N/A | R | snmptraphosttbl
Table Index | Integer | User Defined | N/A | index
IP Address | IpAddress | User Defined | RW | ipaddr
Password | DisplayString | User Defined (up to 64 characters) | W | passwd
Comment (optional) | DisplayString | User Defined (up to 254 characters) | RW | cmt
Status (optional) | Integer | enable (default) disable delete | RW | status
#### Syslog Parameters The following parameters configure the Syslog settings.
Name | Type | Values | Access | CLI
Syslog | Group | N/A | R | syslog
Syslog Status | Integer | enable disable (default) | RW | syslogstatus
Syslog Port | Octet String | 514 | R | syslogport
Syslog Lowest Priority Logged | Integer | 1 – 7 1 = LOG_ALERT 2 = LOG_CRIT 3 = LOG_ERR 4 = LOG_WARNING 5 = LOG_NOTICE 6 = LOG_INFO (default) 7 = LOG_DEBUG | RW | syslogpritolog
Heartbeat Status | Integer | enable (1) disable (2) (default) | RW | sysloghbstatus
Heartbeat Interval (seconds) | Integer | 1 – 604800 seconds; 900 sec. (default) | RW | sysloghbinterval
#####
| The Heartbeat parameters are advanced settings not available via the HTTP interface. When Heartbeat is enabled, the AP periodically sends a message to the Syslog server to indicate that it is active. The frequency with which the heartbeat message is sent depends upon the setting of the Heartbeat Interval.
##### Syslog Host Table The table described below configures the Syslog hosts that will receive message from the AP. You can configure up to ten Syslog hosts.
Name | Type | Values | Access | CLI Parameter
Syslog Host Table | Table | N/A | R | sysloghosttbl
Table Index | Integer | 1 – 10 | N/A | index
IP Address | IpAddress | User Defined | RW | ipaddr
Comment (optional) | DisplayString | User Defined | RW | cmt
Status (optional) | Integer | enable disable delete | RW | status
### Bridge Parameters #### Spanning Tree Parameters
Name | Type | Values | Access | CLI Parameter
Spanning Tree | Group | N/A | R | stp
Spanning Tree Status | Integer | enable (default) disable | RW | stpstatus
Bridge Priority | Integer | 0 – 65535 32768 (default) | RW | stppriority
Maximum Age | Integer | 600 – 4000 (in 0.01 sec intervals; i.e., 6 to 40 seconds) 2000 (default) | RW | stpmaxage
Hello Time | Integer | 100 – 1000 (in 0.01 sec intervals; i.e., 1 to 10 seconds) 200 (default) | RW | stphellotime
Forward Delay | Integer | 400 – 3000 (in 0.01 sec intervals; i.e., 4 to 30 seconds) 1500 (default) | RW | stpfwddelay
##### Spanning Tree Priority and Path Cost Table
Name | Type | Values | Access | CLI Parameter
Spanning Tree Table | Table | N/A | R | stpbl
Table Index (Port) | N/A | 1 – 15 | R | index
Priority | Integer | 0 – 255 128 (default) | RW | priority
Path Cost | Integer | 1 – 65535 100 (default) | RW | pathcost
State | Integer | disable blocking listening learning forwarding broken | R | state
Status | Integer | enable disable | RW | status
#### Storm Threshold Parameters
Name | Type | Values | Access | CLI Parameter
Storm Threshold | Group | N/A | N/A | stmthres
Broadcast Threshold | Integer | 0 – 255 packets/sec (default is 0) | RW | stmbrdthres
Multicast Threshold | Integer | 0 – 255 packets/sec (default is 0) | RW | stmmultithres
##### Storm Threshold Table
Name | Type | Values | Access | CLI Parameter
Storm Threshold Table | Table | N/A | R | stmthrestbl
Table Index | Integer | 1 = Ethernet 3 = Wireless | R | index
Broadcast Threshold | Integer | 0 – 255 packets/sec (default is 0) | RW | bcast
Multicast Threshold | Integer | 0 – 255 packets/sec (default is 0) | RW | mcast
#### Intra BSS Subscriber Blocking The following parameters control the Intra BSS traffic feature, which prevent wireless clients that are associated with the same AP from communicating with each other:
Name | Type | Values | Access | CLI
Intra BSS Traffic | Group | N/A | R | intrabss
Intra BSS Traffic Operation | Integer | passthru (default) block | RW | intrabssoptype
#### Packet Forwarding Parameters The following parameters control the Packet Forwarding feature, which redirects wireless traffic to a specific MAC address:
Name | Type | Values | Access | CLI
Packet Forwarding MAC Address | Group | N/A | R | pktfwd
Packet Forwarding MAC Address | MacAddress | User Defined | RW | pktfwdmacaddr
Packet Forwarding Status | Integer | enable disable (default) | RW | pktfwdstatus
Packet Forwarding Interface Port | Integer | 0 (any) (default) 1 (Ethernet) 2 (WDS 1) 3 (WDS 2) 4 (WDS 3) 5 (WDS 4) 6 (WDS 5) 7 (WDS 6) | RW | pktfwdif
###
| The Wireless Distribution System (WDS) feature is not available for 802.11a or 802.11b/g APs at this time.
### Security Parameters Refer to Configure SSID (Network Name) and VLAN Pairs, and Security Modes for information on configuring security modes for the AP. #### MAC Access Control Parameter
Name | Type | Values | Access | CLI Parameter
MAC Address Control | Group | N/A | R | macacl
Status | Integer | enable disable (default) | RW | macaclstatus
Operation Type | Integer | passthru (default) block | RW | macacloptype
##### MAC Access Control Table
Name | Type | Values | Access | CLI Parameter
MAC Address Control Table | Table | N/A | R | macacltbl
Table Index | N/A | N/A | R | index
MAC Address | PhysAddress | User Defined | RW | macaddr
Comment (optional) | DisplayString | User Defined max 254 characters | RW | cmt
Status (optional) | Integer | enable (default) disable delete | RW | status
### RADIUS Parameters #### Primary and Backup RADIUS Server Table Parameters ORiNOCO devices that use RADIUS authentication and/or accounting support a primary and backup RADIUS server for MAC-based authentication and a primary and backup RADIUS server for EAP/802.1x authentication. The configuration parameters and statistics are the same for both primary and backup servers. The CLI differentiates the primary and backup RADIUS parameters by using the table index: ### · Index 1: Primary MAC-based authentication server ### · Index 2: Backup MAC-based authentication server ### · Index 3: Primary EAP/802.1x authentication server ### · Index 4: Backup EAP/802.1x authentication server ##### General RADIUS Parameters
Name | Type | Values | Access | CLI Parameter
RADIUS | Group | N/A | R | radius
MAC Access Control Status | Integer | enable disable (default) | R | radmacacctrl
Authorization Lifetime | Integer32 | 900 – 43200 seconds 0 sec. (default) | RW | radauthlifetm
MAC Address Format | Integer | dashdelimited (default) colondelimited singledashdelimited no delimiter | RW | radmacaddrformat
RADIUS Accounting Status | Integer | enable disable (default) | RW | radaccstatus
Accounting Inactivity Timer | Integer32 | 0 – 2147483647 minutes; default is 5 min. | RW | radaccinactivetmr
##### RADIUS Authentication
| Use a server name only if you have enabled the DNS Client functionality. See DNS Client for RADIUS Name Resolution.
###
Name | Type | Values | Access | CLI Parameter
RADIUS Authentication | Table | N/A | R | radiustbl
Primary MAC-based authentication server | Integer | 1 | R | index
Backup MAC-based authentication server | Integer | 2 | R | index
Primary EAP/802.1x authentication server | Integer | 3 | R | index
Backup EAP/802.1x authentication server | Integer | 4 | R | index
RADIUS Server Status | Integer | enable disable (default) | RW | status
Server Addressing Format (see note) | Integer | ipaddr (default) name | RW | seraddrfmt
Server IP Address or Name | IpAddress DisplayString | User Defined (enter an IP address if seraddrfmt is ipaddr or a name if set to name; up to 254 characters if using a name) | RW | ipaddr
Port (optional) | Integer | User Defined 1812 (default) | RW | port
Shared Secret | DisplayString | User Defined max 63 characters | W | ssecret
Response Time (sec) | Integer | 1 – 4 seconds 3 sec (default) | RW | responsetm
Maximum Retransmissions (optional) | Integer | 0 – 4 3 (default) | RW | maxretx
##### RADIUS Accounting
| Use a server name only if you have enabled the DNS Client functionality. See DNS Client for RADIUS Name Resolution.
Name | Type | Values | Access | CLI Parameter
RADIUS Accounting | Table | N/A | R | radacctbl
Primary RADIUS | Integer | 1 | R | index
Backup RADIUS | Integer | 2 | R | index
RADIUS Server Status | Integer | enable disable (default) | RW | status
Server Addressing Format (see note) | Integer | ipaddr (default) name | RW | seraddrfmt
Server IP Address or Name | IpAddress Display String | User Defined (enter an IP address if seraddrfmt is ipaddr or a name if set to name; up to 254 characters if using a name) | RW | ipaddr
Port (optional) | Integer | User Defined 1813 (default) | RW | port
Shared Secret | DisplayString | User Defined max 63 characters | W | ssecret
Response Time (sec) | Integer | 1 – 4 seconds 3 sec (default) | RW | responsetm
Maximum Retransmissions (optional) | Integer | 1 – 10 3 (default) | RW | maxretx
### Rogue Access Point Detection (RAD) Parameters
Name | Type | Values | Access | CLI Parameter
Rogue Access Point Detection (RAD) | Group | N/A | R | rad
Status | Integer | enable disable (default) | RW | radstatus
Scan Interval | Integer | 15-1440 (minutes) | RW | radscanint
Interface Bitmask | Interface Bitmask | 4 (WiF A), 8 (WiF B), or 12 (both). | RW | radifbitmask
### VLAN/SSID Parameters
Name | Type | Values | Access | CLI Parameter
VLAN | Group | N/A | R | vlan
Status | Integer | enable disable (default) | RW | vlanstatus
Management ID | VlanId | -1 (untagged) or 1-4094 | RW | vlanmgmtid
#### VLAN ID Table
| 16 VLAN/SSID pairs are available for 802.11b/g APs and APs with an 11a Upgrade Kit. 802.11b APs and APs with a 5 GHz Upgrade Kit only support one VLAN/SSID pair.
####
Name | Type | Values | Access | CLI Parameter
VLAN ID Table | Table | N/A | R | vlanidtbl
Index 1 | Integer32 | 3.1 - 3.16 (Wireless A); 4.1 - 4.16 (Wireless B; Dual-radio APs only) | R | index
Identifier (ID) | VlanId | -1 or 0 (both correspond to untagged) or 1-4094 | RW | id
Network Name (SSID) | DisplayString | 2-31 characters | RW | ssid
Status | Integer | enable (default when new entry created) disable delete | RW | status
Note 1: When adding a new entry to the table, you must specify the index instance you want to configure, such as 3.5; the 0 index value is not applicable to this table and does not create a new entry. ### Other Parameters #### IAPP Parameters
Name | Type | Values | Access | CLI Parameter
IAPP | Group | N/A | R | iapp
IAPP Status | Integer | enable (default) disable | RW | iappstatus
Periodic Announce Interval (seconds) | Integer | 80 120 (default) 160 200 | RW | iappannint
Announce Response Time | Integer | 2 seconds | R | iappannresp
Handover Time-out | Integer | 410 ms 512 ms (default) 614 ms 717 ms 819 ms | RW | iapphandtout
Max. Handover Retransmissions | Integer | 1 - 4 (default 4) | RW | iapphandretx
Send Announce Request on Startup | Integer | enable (default) disable | RW | iappannreqstart
####
| These parameters configure the Inter Access Point Protocol (IAPP) for roaming. Leave these settings at their default value unless a technical representative asks you to change them.
#### SpectraLink VoIP Parameters (802.11b and bg Modes Only) These parameters enable or disable the SpectraLink Voice over IP feature. The Spectralink Legacy Support parameter should be enabled if the AP is operating in 802.11bg mode and legacy 802.11 Spectralink telephones are used. This parameter will set the basic rates of the AP to be 1 and 2 Mbps in 802.11bg mode and will allow old telephones that operate only at the 1 and 2 Mbps basic rate to connect to the AP.
Name | Type | Values | Access | CLI Parameter
Spectralink VoIP | Group | N/A | R | spectralink
Spectralink VoIP Status | Integer | enable disable (default) | RW | speclinkstatus
Spectralink Legacy Support | Integer | enable disable (default) | RW | speclinklegacysupport
###