# AP-2000 Help Contents |
[ Home ] [Proxim website]

## Status Information Logging into the HTTP Interface System Status ## Logging into the HTTP Interface Once the AP has a valid IP Address and an Ethernet connection, you may use your web browser to monitor the system status. Follow these steps to monitor an AP’s operating statistics using the HTTP interface: Open a Web browser on a network computer.
| The HTTP interface supports the following Web browser:
Microsoft Internet Explorer 6 with Service Pack 1 or later Netscape 6.1 or later If necessary, disable the Internet proxy settings. For Internet Explorer users, follow these steps: Select Tools > Internet Options.... Click the Connections tab. Click LAN Settings.... If necessary, remove the check mark from the Use a proxy server box. Click OK twice to save your changes and return to Internet Explorer. Enter the Access Point’s IP address in the browser’s Address field and press Enter. Result: The Enter Network Password screen appears. Enter the HTTP password in the Password field and click OK. Leave the User Name field blank. (By default, the HTTP password is “public”). Result: The System Status screen appears. Enter Network Password Screen ## System Status System Status is the first screen to appear each time you connect to the HTTP interface. You can also return to this screen by clicking the Status button. System Status Screen Each section of the System Status screen provides the following information: System Status: This area provides system level information, including the unit’s IP address and contact information. See System for information on these settings. System Alarms: System traps (if any) appear in this area. Each trap identifies a specific severity level: Critical, Major, Minor, and Informational. See Alarms for a list of possible alarms.