# AP-2000 Help Contents |
[ Home ] [ORiNOCO website]

## Recording Your Configuration Settings We recommend keeping a copy of the configuration settings for each of the AP-2000 devices in your network. The information below is hard-coded in your system and can be viewed from the Web Interface pages by clicking the Configure button and viewing the System and Interfaces screens.
MAC Address of the AP-2000 unit |
AP software image version |
BSP/Bootloader firmware version |
Hardware revision level |
MAC Address of the PC Card in Slot A |
Driver version of the PC CArd in Slot A |
MAC Address of the PC Card in Slot B |
Driver version of the PC Card in Slot B |
In the web interface, click the Monitor button and select the Version tab. The table displays the Object ID and version numbers for each piece of hardware. For the Hardware Inventory, the following information may be useful when contacting Technical Support:
Type | Object ID
--- | ---
AP-2000 with Mini-DIN8 serial port adapter | 97
AP-2000 converted to AS-2000 with Mini-DIN8 serial port adapter | 96
Use the following pages to document your configuration. You can use this information to easily recover your network settings if necessary. ## Configuration Settings In the table below, record the configuration settings for each of your AP-2000 units. The shaded cells indicate the location of the parameters within the HTTP web interface. The first column in the table indicates the parameter name, the second column indicates the default value of each parameter (when applicable). Use the third column to record your settings. The last column is an aide which indicates the CLI command syntax required to define the configuration parameters in case you need to re-enter data through the Command Line Interface.