DOS or Windows

First slice, called ad0s1 (C: in DOS)

Second slice, called ad0s2

Partition a, mounted as /, called ad0s2a

Partition b, used as swap, called ad0s2b

Partition e, mounted as /var, called ad0s2e

Partition f, mounted as /usr, called ad0s2f

(not to scale)

Partition c, not mounted, called ad0s2c