-- *****************************************************************
-- IEEE802dot11-MIB :
-- IEEE 802.11 Management Information Base file
--
-- Nov 2002, Francis Pang 
--
-- Copyright (c) 2002 by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

-- **********************************************************************
-- * IEEE 802.11 Management Information Base
-- **********************************************************************

IEEE802dot11-MIB DEFINITIONS ::= BEGIN

    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE, 
        NOTIFICATION-TYPE,Integer32, Counter32,
        Unsigned32 				FROM SNMPv2-SMI

        DisplayString , MacAddress, RowStatus,
        TruthValue                              FROM SNMPv2-TC

        MODULE-COMPLIANCE, OBJECT-GROUP, 
        NOTIFICATION-GROUP                      FROM SNMPv2-CONF 

        ifIndex                                 FROM RFC1213-MIB;

-- **********************************************************************
-- *  Tree Definition
-- **********************************************************************

    member-body     OBJECT IDENTIFIER ::= { iso 2 }
    us              OBJECT IDENTIFIER ::= { member-body 840 }

-- **********************************************************************
-- *  MODULE IDENTITY
-- **********************************************************************

ieee802dot11 MODULE-IDENTITY
    LAST-UPDATED "0208300000Z"
    ORGANIZATION "IEEE 802.11"
    CONTACT-INFO 
           "WG E-mail: stds-802-11@ieee.org

                Chair: Stuart J. Kerry
                Postal: Philips Semiconductors, Inc.
                       1109 McKay Drive
                       M/S 48 SJ
                       San Jose, CA 95130-1706  USA
                  Tel: +1 408 474 7356
                  Fax: +1 408 474 7247
               E-mail: stuart.kerry@philips.com

               Editor: Bob O'Hara
               Postal: Informed Technology, Inc.
                       1750 Nantucket Circle, Suite 138
                       Santa Clara, CA 95054 USA
                  Tel: +1 408 986 9596
                  Fax: +1 408 727 2654
               E-mail: bob@informed-technology.com"
    DESCRIPTION
        "The MIB module for IEEE 802.11 entities.
        iso(1).member-body(2).us(840).ieee802dot11(10036)"
    ::= { us 10036 }

-- **********************************************************************
-- *  Major sections
-- **********************************************************************

--  Station ManagemenT (SMT) Attributes
    --  DEFINED AS "The SMT object class provides the necessary support
    --  at the station to manage the processes in the station such that
    --  the station may work cooperatively as a part of an IEEE 802.11
    --  network."

    dot11smt OBJECT IDENTIFIER ::= { ieee802dot11 1 }

        --  dot11smt GROUPS
        --  dot11StationConfigTable            ::= { dot11smt 1 }
        --  dot11AuthenticationAlgorithmsTable ::= { dot11smt 2 }
        --  dot11WEPDefaultKeysTable           ::= { dot11smt 3 }
        --  dot11WEPKeyMappingsTable           ::= { dot11smt 4 }
        --  dot11PrivacyTable                  ::= { dot11smt 5 }
        --  dot11SMTnotification               ::= { dot11smt 6 }
        --  dot11MultiDomainCapabilityTable    ::= { dot11smt 7 }

--  MAC Attributes
    --  DEFINED AS "The MAC object class provides the necessary support
    --  for the access control, generation, and verification of frame
    --  check sequences (FCSs), and proper delivery of valid data to 
    --  upper layers."

    dot11mac OBJECT IDENTIFIER ::= { ieee802dot11 2 }

      --  MAC GROUPS
      --  reference IEEE Std 802.1f-1993
         --  dot11OperationTable   	    ::= { dot11mac 1 }
         --  dot11CountersTable    	    ::= { dot11mac 2 }
         --  dot11GroupAddressesTable 	    ::= { dot11mac 3 }

--  Resource Type ID
    dot11res 		OBJECT IDENTIFIER 	::= { ieee802dot11 3 }
    dot11resAttribute 	OBJECT IDENTIFIER 	::= { dot11res 1 }

--  PHY Attributes
    --  DEFINED AS "The PHY object class provides the necessary support
    --  for required PHY operational information that may vary from PHY
    --  to PHY and from STA to STA to be communicated to upper layers."

    dot11phy OBJECT IDENTIFIER ::= { ieee802dot11 4 }

    --  PHY GROUPS
    	--  dot11PhyOperationTable    	    ::= { dot11phy 1 }
    	--  dot11PhyAntennaTable   	    ::= { dot11phy 2 }
    	--  dot11PhyTxPowerTable      	    ::= { dot11phy 3 }
    	--  dot11PhyFHSSTable         	    ::= { dot11phy 4 }
    	--  dot11PhyDSSSTable         	    ::= { dot11phy 5 }
    	--  dot11PhyIRTable           	    ::= { dot11phy 6 }
    	--  dot11RegDomainsSupportedTable   ::= { dot11phy 7 }
    	--  dot11AntennasListTable          ::= { dot11phy 8 }
    	--  dot11SupportedDataRatesTxTable  ::= { dot11phy 9 }
    	--  dot11SupportedDataRatesRxTable  ::= { dot11phy 10 }
    	--  dot11PhyOFDMTable               ::= { dot11phy 11 }
    	--  dot11PhyHRDSSSTable 	    ::= { dot11phy 12 }
	--  dot11EHCCHoppingPatternTable    ::= { dot11phy 13 }

-- **********************************************************************
-- *  Textual conventions from 802 definitions
-- **********************************************************************

    WEPKeytype ::= OCTET STRING (SIZE (5))

-- **********************************************************************
-- *  MIB attribute OBJECT-TYPE definitions follow
-- **********************************************************************

-- **********************************************************************
-- *  SMT Station Config  Table
-- **********************************************************************

dot11StationConfigTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11StationConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Station Configuration attributes.  In tablular form to
            allow for multiple instances on an agent."
    ::= { dot11smt 1 }

dot11StationConfigEntry OBJECT-TYPE
        SYNTAX Dot11StationConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11StationConfigTable.  It is
            possible for there to be multiple IEEE 802.11 interfaces
            on one agent, each with its unique MAC address. The
            relationship between an IEEE 802.11 interface and an
            interface in the context of the Internet-standard MIB is
            one-to-one.  As such, the value of an ifIndex object
            instance can be directly used to identify corresponding
            instances of the objects defined herein.  

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11StationConfigTable 1 }

Dot11StationConfigEntry ::=
        SEQUENCE { 	
	    dot11StationID                        MacAddress,
            dot11MediumOccupancyLimit          	  INTEGER,
            dot11CFPollable                    	  TruthValue,
            dot11CFPPeriod                     	  INTEGER, 
            dot11CFPMaxDuration                	  INTEGER,
            dot11AuthenticationResponseTimeOut 	  Unsigned32,
            dot11PrivacyOptionImplemented      	  TruthValue,
	    dot11PowerManagementMode	  	  INTEGER,
	    dot11DesiredSSID		  	  OCTET STRING,
	    dot11DesiredBSSType		  	  INTEGER,
	    dot11OperationalRateSet		  OCTET STRING,
	    dot11BeaconPeriod		  	  INTEGER,
	    dot11DTIMPeriod			  INTEGER,
	    dot11AssociationResponseTimeOut	  Unsigned32,
            dot11DisassociateReason               INTEGER,
            dot11DisassociateStation              MacAddress,
            dot11DeauthenticateReason             INTEGER,
            dot11DeauthenticateStation            MacAddress,
            dot11AuthenticateFailStatus           INTEGER,
            dot11AuthenticateFailStation          MacAddress,
            dot11MultiDomainCapabilityImplemented TruthValue, 
	    dot11MultiDomainCapabilityEnabled TruthValue, 
	    dot11CountryString		  OCTET STRING }

dot11StationID OBJECT-TYPE
        SYNTAX MacAddress
 --       MAX-ACCESS read-write        Jacky.Xue disable write access 2005/05/12
        MAX-ACCESS read-only
        STATUS deprecated
        DESCRIPTION
            "The purpose of dot11StationID is to allow a manager to 
            identify a station for its own purposes.  This attribute
            provides for that eventuality while keeping the true MAC
            address independent.  Its syntax is MAC address, and the
            default value is the station's assigned, unique 
            MAC address."
    ::= { dot11StationConfigEntry 1 }

dot11MediumOccupancyLimit OBJECT-TYPE
        SYNTAX INTEGER (0..1000)
--        MAX-ACCESS read-write          Jacky.Xue disable write access 2005/05/12
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This attribute shall indicate the maximum amount of time,
            in TU, that a point coordinator (PC) may control the usage 
            of the wireless medium (WM) without relinquishing control 
            for long enough to allow at least one instance of DCF access 
            to the medium.  The default value of this attribute shall 
            be 100, and the maximum value shall be 1000."
    ::= { dot11StationConfigEntry 2 }

dot11CFPollable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "When this attribute is true, it shall indicate that 
	        the STA is able to respond to a CF-Poll with a data frame 
	        within a SIFS time. This attribute shall be false if 
	        the STA is not able to respond to a CF-Poll with a data 
	        frame within a SIFS time."
    ::= { dot11StationConfigEntry 3 }

dot11CFPPeriod OBJECT-TYPE
        SYNTAX INTEGER (0..255)
 --       MAX-ACCESS read-write      Jacky.Xue disable write access 2005/05/12
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The attribute shall describe the number of DTIM intervals
            between the start of CFPs.  It is modified by
            MLME-START.request primitive."
    ::= { dot11StationConfigEntry 4 }

dot11CFPMaxDuration OBJECT-TYPE
        SYNTAX INTEGER (0..65535)
--      MAX-ACCESS read-write      Jacky.Xue disable write access 2005/05/12 
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "The attribute shall describe the maximum duration of 
	        the CFP in TU that may be generated by the PCF. It is 
	        modified by MLME-START.request primitive."
    ::= { dot11StationConfigEntry 5 }

dot11AuthenticationResponseTimeOut OBJECT-TYPE
        SYNTAX Unsigned32 (1..4294967295)
--      MAX-ACCESS read-write        Jacky.Xue disable write access 2005/05/12 
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This attribute shall specify the number of time units (TUs)
             that a responding STA should wait for the next frame in the
            authentication sequence."
    ::= { dot11StationConfigEntry 6 }

dot11PrivacyOptionImplemented OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This attribute, when true, shall indicate that the IEEE
            802.11 WEP option is implemented.  The default value of
            this attribute shall be false."
    ::= { dot11StationConfigEntry 7 }

dot11PowerManagementMode OBJECT-TYPE
		SYNTAX INTEGER { active(1), powersave(2) }
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall specify the power management
			mode of the STA. When set to active, it shall 
			indicate that the station is not in power-save 
			(PS) mode. When set to powersave, it shall indicate
			 that the station is in power-save mode. The power 
			management mode is transmitted in all frames 
			according to the rules in  7.1.3.1.7."
	::= { dot11StationConfigEntry 8 }

dot11DesiredSSID OBJECT-TYPE
		SYNTAX OCTET STRING (SIZE(0..32))
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute reflects the Service Set ID (SSID)
			used in the DesiredSSID parameter of the most recent
			MLME_Scan.request.  This value may be modified
			by an external management entity and used by the
			local SME to make decisions about the Scanning 
			process."
	::= { dot11StationConfigEntry 9 }

dot11DesiredBSSType OBJECT-TYPE
		SYNTAX INTEGER { infrastructure(1), independent(2), any(3) }
--		MAX-ACCESS read-write   Jacky.Xue disable write access 2005/05/12 
        MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute shall specify the type of BSS the
			station shall use when scanning for a BSS with 
			which to synchronize. This value is used to filter 
			Probe Response frames and Beacons. When set to 
			infrastructure, the station shall only synchronize 
			with a BSS whose Capability Information field has 
			the ESS subfield set to 1. When set to independent, 
			the station shall only synchronize with a BSS whose 
			Capability Information field has the IBSS subfield 
			set to 1. When set to any, the station may 
			synchronize to either type of BSS."
	::= { dot11StationConfigEntry 10 }

dot11OperationalRateSet OBJECT-TYPE
		SYNTAX OCTET STRING (SIZE(1..126))
--		MAX-ACCESS read-write      Jacky.Xue disable write access 2005/05/12 
        MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute shall specify the set of data 
			rates at which the station may transmit data.  
			Each octet contains a value representing a rate.  
			Each rate shall be within the range from 2 to 127,
			corresponding to data rates in increments of
			500 kbit/s from 1 Mbit/s to 63.5 Mbit/s, and shall 
			be supported (as indicated in the supported rates
			table) for receiving data. This value is reported in
			transmitted Beacon, Probe Request, Probe Response,
			Association Request, Association Response,
			Reassociation Request, and Reassociation Response
			frames, and is used to determine whether a BSS
			with which the station desires to synchronize is
			suitable. It is also used when starting a BSS,
			as specified in  10.3."
	::= { dot11StationConfigEntry 11 }

dot11BeaconPeriod OBJECT-TYPE
		SYNTAX INTEGER (1..65535)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall specify the number of TUs that 
			a station shall use for scheduling Beacon 
			transmissions. This value is transmitted in Beacon 
			and Probe Response frames."
	::= { dot11StationConfigEntry 12 }

dot11DTIMPeriod OBJECT-TYPE
		SYNTAX INTEGER(1..255)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall specify the number of beacon
			intervals that shall elapse between transmission of
			Beacons frames containing a TIM element whose DTIM
			Count field is 0. This value is transmitted in
			the DTIM Period field of Beacon frames."
	::= { dot11StationConfigEntry 13 }

dot11AssociationResponseTimeOut OBJECT-TYPE
		SYNTAX Unsigned32 (1..4294967295)
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall specify the number of TU that a
			requesting STA should wait for a response to a
			transmitted association-request MMPDU."
	::= { dot11StationConfigEntry 14 }

dot11DisassociateReason OBJECT-TYPE
		SYNTAX INTEGER(0..65535)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute holds the most recently
			transmitted Reason Code in a Disassociation
			frame.  If no Disassociation frame has been
			transmitted, the value of this attribute shall
			be 0."
        REFERENCE "IEEE Std 802.11-2002, 7.3.1.7"
	::= { dot11StationConfigEntry 15 }

dot11DisassociateStation OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute holds the MAC address from the
			Address 1 field of the most recently transmitted
			Disassociation frame.  If no Disassociation
			frame has been transmitted, the value of this
			attribute shall be 0."
	::= { dot11StationConfigEntry 16 }

dot11DeauthenticateReason OBJECT-TYPE
		SYNTAX INTEGER(0..65535)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute holds the most recently
			transmitted Reason Code in a Deauthentication
			frame.  If no Deauthentication frame has been
			transmitted, the value of this attribute shall
			be 0."
        REFERENCE "IEEE Std 802.11-2002, 7.3.1.7"
	::= { dot11StationConfigEntry 17 }

dot11DeauthenticateStation OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute holds the MAC address from the
			Address 1 field of the most recently transmitted
			Deauthentication frame.  If no Deauthentication
			frame has been transmitted, the value of this
			attribute shall be 0."
	::= { dot11StationConfigEntry 18 }

dot11AuthenticateFailStatus OBJECT-TYPE
		SYNTAX INTEGER(0..65535)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute holds the most recently
			transmitted Status Code in a failed
			Authentication frame.  If no failed
			Authentication frame has been transmitted, the
			value of this attribute shall be 0."
        REFERENCE "IEEE Std 802.11-2002, 7.3.1.9"
	::= { dot11StationConfigEntry 19 }

dot11AuthenticateFailStation OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute holds the MAC address from the
			Address 1 field of the most recently transmitted
			failed Authentication frame.  If no failed
			Authentication frame has been transmitted, the
			value of this attribute shall be 0."
	::= { dot11StationConfigEntry 20 }

dot11MultiDomainCapabilityImplemented OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute, when TRUE, indicates that the 
			station implementation is capable of supporting 
			multiple regulatory domains.  The capability is 
			disabled, otherwise.  The default value of this 
			attribute is FALSE."
	::= { dot11StationConfigEntry 21 }

dot11MultiDomainCapabilityEnabled OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute, when TRUE, indicates that the 
			capability of the station to operate in multiple 
			regulatory domains is enabled.  The capability is 
			disabled, otherwise.  The default value of this 
			attribute is FALSE."
	::= { dot11StationConfigEntry 22 }

dot11CountryString OBJECT-TYPE
		SYNTAX OCTET STRING (SIZE(3))
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute identifies the country in which the 
			station is operating. The first two octets of this 
			string is the two character country code as described 
			in document ISO/IEC 3166-1.  The third octet shall 
			be one of the following:

			1. an ASCII space character, if the regulations under 
			which the station is operating encompass all 
			environments in the country,

			2. an ASCII 'O' character, if the regulations under 
			which the station is operating are for an Outdoor 
			environment only, or

			3. an ASCII 'I' character, if the regulations under 
			which the station is operating are for an Indoor 
			environment only."
	::= { dot11StationConfigEntry 23 }

-- **********************************************************************
-- *    End of dot11StationConfig  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    AuthenticationAlgorithms  TABLE
-- **********************************************************************

dot11AuthenticationAlgorithmsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11AuthenticationAlgorithmsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This (conceptual) table of attributes shall be a set of
            all the authentication algorithms supported by the
            stations.  The following are the default values and the
            associated algorithm:
                Value = 1: Open System
                Value = 2: Shared Key"
        REFERENCE "IEEE Std 802.11-2002, 7.3.1.1"
    ::= { dot11smt 2 }

dot11AuthenticationAlgorithmsEntry OBJECT-TYPE
        SYNTAX Dot11AuthenticationAlgorithmsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the Authentication
            Algorithms Table.  

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex,
                dot11AuthenticationAlgorithmsIndex }
    ::= { dot11AuthenticationAlgorithmsTable  1 }

Dot11AuthenticationAlgorithmsEntry ::= 
        SEQUENCE {	dot11AuthenticationAlgorithmsIndex	Integer32,
        	       	dot11AuthenticationAlgorithm      	INTEGER,
	    	     	dot11AuthenticationAlgorithmsEnable	TruthValue }

dot11AuthenticationAlgorithmsIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the Authentication Algorithms Table."
    ::= { dot11AuthenticationAlgorithmsEntry 1 }

dot11AuthenticationAlgorithm OBJECT-TYPE
        SYNTAX INTEGER { openSystem(1), sharedKey(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "This attribute shall be a set of all the authentication
	        algorithms supported by the STAs. The following are the
	        default values and the associated algorithm.  
		        Value = 1: Open System 
		        Value = 2: Shared Key"
    ::= { dot11AuthenticationAlgorithmsEntry 2 }

dot11AuthenticationAlgorithmsEnable  OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "This attribute, when true at a station, shall enable the acceptance 
	        of the authentication algorithm described in the corresponding table 
	        entry in authentication frames received by the station that have odd 
	        authentication sequence numbers.  The default value of this attribute 
	        shall be 1 for the Open System table entry and 2 for all other table 
	        entries."
    ::= { dot11AuthenticationAlgorithmsEntry 3 }

-- **********************************************************************
-- *    End of AuthenticationAlgorithms  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    WEPDefaultKeys  TABLE
-- **********************************************************************

dot11WEPDefaultKeysTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11WEPDefaultKeysEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Conceptual table for WEP default keys.  This table shall
            contain the four WEP default secret key values
            corresponding to the four possible KeyID values.  The WEP
            default secret keys are logically WRITE-ONLY.  Attempts to
            read the entries in this table shall return unsuccessful
            status and values of null or zero.  The default value of
            each WEP default key shall be null."
        REFERENCE "IEEE Std 802.11-2002, 8.3.2"
    ::= { dot11smt 3 }

dot11WEPDefaultKeysEntry OBJECT-TYPE
        SYNTAX Dot11WEPDefaultKeysEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the WEP Default Keys Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
       INDEX { ifIndex, 
               dot11WEPDefaultKeyIndex}
    ::= { dot11WEPDefaultKeysTable  1 }

Dot11WEPDefaultKeysEntry ::= 
        SEQUENCE {	dot11WEPDefaultKeyIndex     INTEGER,
        	    	dot11WEPDefaultKeyValue     WEPKeytype }

dot11WEPDefaultKeyIndex OBJECT-TYPE
        SYNTAX INTEGER (1..4)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the WEP Default Keys Table.
           The value of this variable is equal to the WEPDefaultKeyID + 1"
    ::= { dot11WEPDefaultKeysEntry 1 }

dot11WEPDefaultKeyValue OBJECT-TYPE
        SYNTAX WEPKeytype
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A WEP default secret key value."
    ::= { dot11WEPDefaultKeysEntry 2 }

-- **********************************************************************
-- *    End of WEPDefaultKeys  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    WEPKeyMappings  TABLE
-- **********************************************************************

dot11WEPKeyMappingsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11WEPKeyMappingsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Conceptual table for WEP Key Mappings.  The MIB supports
            the ability to share a separate WEP key for each RA/TA
            pair.  The Key Mappings Table contains zero or one entry
            for each MAC address and contains two fields for each
            entry: WEPOn and the corresponding WEP key.  The WEP key
            mappings are logically WRITE-ONLY.  Attempts to read the
            entries in this table shall return unsuccessful status and
            values of null or zero.  The default value for all WEPOn
            fields is false."
        REFERENCE "IEEE Std 802.11-2002, 8.3.2"
    ::= { dot11smt 4 }

dot11WEPKeyMappingsEntry OBJECT-TYPE
        SYNTAX Dot11WEPKeyMappingsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the WEP Key Mappings Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex, 
                dot11WEPKeyMappingIndex }
    ::= { dot11WEPKeyMappingsTable  1 }

Dot11WEPKeyMappingsEntry ::= 
        SEQUENCE {	dot11WEPKeyMappingIndex	    Integer32,
        	    	dot11WEPKeyMappingAddress   MacAddress,
        	    	dot11WEPKeyMappingWEPOn 	TruthValue,
        	    	dot11WEPKeyMappingValue     WEPKeytype,
	    			dot11WEPKeyMappingStatus	RowStatus }

dot11WEPKeyMappingIndex OBJECT-TYPE
        SYNTAX Integer32 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the WEP Key Mappings Table."
    ::= { dot11WEPKeyMappingsEntry 1 }

dot11WEPKeyMappingAddress OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The MAC address of the STA for which the values from this
            key mapping entry are to be used."
    ::= { dot11WEPKeyMappingsEntry 2 }

dot11WEPKeyMappingWEPOn OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Boolean as to whether WEP is to be used when communicating
            with the dot11WEPKeyMappingAddress STA."
    ::= { dot11WEPKeyMappingsEntry 3 }

dot11WEPKeyMappingValue OBJECT-TYPE
        SYNTAX WEPKeytype
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "A WEP secret key value."
    ::= { dot11WEPKeyMappingsEntry 4 }

dot11WEPKeyMappingStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The status column used for creating, modifying, and
            deleting instances of the columnar objects in the WEP key
            mapping Table."
        DEFVAL { active }
    ::= { dot11WEPKeyMappingsEntry 5 }

-- **********************************************************************
-- *    End of WEPKeyMappings  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PrivacyTable  TABLE
-- **********************************************************************

dot11PrivacyTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PrivacyEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group containing attributes concerned with IEEE 802.11
            Privacy.  Created as a table to allow multiple
            instantiations on an agent."
    ::= { dot11smt 5 }

dot11PrivacyEntry OBJECT-TYPE
        SYNTAX Dot11PrivacyEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PrivacyTable Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PrivacyTable 1 }

Dot11PrivacyEntry ::= 
        SEQUENCE {	dot11PrivacyInvoked        	TruthValue,
        	     	dot11WEPDefaultKeyID       	INTEGER,
        	     	dot11WEPKeyMappingLength	Unsigned32,
        	     	dot11ExcludeUnencrypted 	TruthValue,
            	 	dot11WEPICVErrorCount      	Counter32,
            	 	dot11WEPExcludedCount      	Counter32 }

dot11PrivacyInvoked OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "When this attribute is true, it shall indicate that the IEEE
	        802.11 WEP mechanism is used for transmitting frames of type
	        Data. The default value of this attribute shall be false."
    ::= { dot11PrivacyEntry 1 }

dot11WEPDefaultKeyID  OBJECT-TYPE
        SYNTAX INTEGER (0..3)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This attribute shall indicate the use of the first,
            second, third, or fourth element of the WEPDefaultKeys
            array when set to values of zero, one, two, or three.  The
            default value of this attribute shall be 0."
        REFERENCE "IEEE Std 802.11-2002, 8.3.2"
    ::= { dot11PrivacyEntry 2 }

dot11WEPKeyMappingLength  OBJECT-TYPE
        SYNTAX Unsigned32 (10..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The maximum number of tuples that dot11WEPKeyMappings can hold."
        REFERENCE "IEEE Std 802.11-2002, 8.3.2"
    ::= { dot11PrivacyEntry 3 }

dot11ExcludeUnencrypted  OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "When this attribute is true, the STA shall not indicate at
	        the MAC service interface received MSDUs that have the WEP
	        subfield of the Frame Control field equal to zero. When this
	        attribute is false, the STA may accept MSDUs that have the WEP
	        subfield of the Frame Control field equal to zero. The default
	        value of this attribute shall be false."
    ::= { dot11PrivacyEntry 4 }

dot11WEPICVErrorCount  OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when a frame is received with the
            WEP subfield of the Frame Control field set to one and the value
            of the ICV as received in the frame does not match the ICV value
            that is calculated for the contents of the received frame."
    ::= { dot11PrivacyEntry 5 }

dot11WEPExcludedCount  OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when a frame is received with the
            WEP subfield of the Frame Control field set to zero and the value
            of dot11ExcludeUnencrypted causes that frame to be discarded."
    ::= { dot11PrivacyEntry 6 }

-- **********************************************************************
-- *    End of dot11Privacy  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    SMT notification Objects
-- **********************************************************************

dot11SMTnotification OBJECT IDENTIFIER ::= { dot11smt 6 }

dot11Disassociate NOTIFICATION-TYPE
        OBJECTS { ifIndex, dot11DisassociateReason, dot11DisassociateStation }
        STATUS current
        DESCRIPTION
	        "The disassociate notification shall be sent when the STA
	        sends a Disassociation frame. The value of the notification
	        shall include the MAC address of the MAC to which the Disassociation
	        frame was sent and the reason for the disassociation.

  	        ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
    ::= { dot11SMTnotification 0 1 }

dot11Deauthenticate NOTIFICATION-TYPE
        OBJECTS { ifIndex, dot11DeauthenticateReason, dot11DeauthenticateStation }
        STATUS current
        DESCRIPTION
	        "The deauthenticate notification shall be sent when the STA
	        sends a Deauthentication frame. The value of the notification
	        shall include the MAC address of the MAC to which the Deauthentication
	        frame was sent and the reason for the deauthentication.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
    ::= { dot11SMTnotification 0 2 }

dot11AuthenticateFail NOTIFICATION-TYPE
        OBJECTS { ifIndex, dot11AuthenticateFailStatus, dot11AuthenticateFailStation }
        STATUS current
        DESCRIPTION
	        "The authenticate failure notification shall be sent when the STA
	        sends an Authentication frame with a status code other than 
	        'successful'. The value of the notification
	        shall include the MAC address of the MAC to which the Authentication
	        frame was sent and the reason for the authentication failure.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
    ::= { dot11SMTnotification 0 3 }


-- **********************************************************************
-- *    End of SMT notification Objects
-- **********************************************************************

-- ********************************************************************
-- * dot11MultiDomainCapability TABLE
-- ********************************************************************

dot11MultiDomainCapabilityTable OBJECT-TYPE
	    SYNTAX SEQUENCE OF Dot11MultiDomainCapabilityEntry
	    MAX-ACCESS not-accessible
	    STATUS current
	    DESCRIPTION
			"This (conceptual) table of attributes for 
			cross-domain mobility."
	::= { dot11smt 7 }

dot11MultiDomainCapabilityEntry OBJECT-TYPE
		SYNTAX Dot11MultiDomainCapabilityEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"An entry (conceptual row) in the Multiple Domain 
                        Capability Table.

			IfIndex - Each IEEE 802.11 interface is represented 
			by an ifEntry. Interface tables in this MIB are 
			indexed by ifIndex."
		INDEX { ifIndex,
		        dot11MultiDomainCapabilityIndex }
	::= { dot11MultiDomainCapabilityTable 1 }
	
Dot11MultiDomainCapabilityEntry ::=
	SEQUENCE {	dot11MultiDomainCapabilityIndex		Integer32,
			dot11FirstChannelNumber			Integer32,
			dot11NumberofChannels			Integer32,
			dot11MaximumTransmitPowerLevel		Integer32 }

dot11MultiDomainCapabilityIndex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The auxiliary variable used to identify instances of 
			the columnar objects in the Multi Domain Capability Table."
	::= { dot11MultiDomainCapabilityEntry 1 }

dot11FirstChannelNumber OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall indicate the value of the lowest 
			channel number in the subband for the associated domain 
			country string. The default value of this attribute 
			shall be zero."
	::= { dot11MultiDomainCapabilityEntry 2 }

dot11NumberofChannels OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall indicate the value of the total 
			number of channels allowed in the subband for the 
			associated domain country string. The default value of 
			this attribute shall be zero."
	::= { dot11MultiDomainCapabilityEntry 3 }

dot11MaximumTransmitPowerLevel OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall indicate the maximum transmit power, 
			in dBm, allowed in the subband for the associated domain 
			country string. The default value of this attribute shall 
			be zero."
	::= { dot11MultiDomainCapabilityEntry 4 }

-- ********************************************************************
-- * End of dot11MultiDomainCapability TABLE
-- ********************************************************************


-- **********************************************************************
-- *    MAC Attribute Templates
-- **********************************************************************

-- **********************************************************************
-- *    dot11OperationTable  TABLE
-- **********************************************************************

dot11OperationTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11OperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group contains MAC attributes pertaining to the operation
            of the MAC.  This has been implemented as a table in order
            to allow for multiple instantiations on an agent."
    ::= { dot11mac 1 }

dot11OperationEntry OBJECT-TYPE
        SYNTAX Dot11OperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11OperationEntry Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11OperationTable 1 }

Dot11OperationEntry ::= 
        SEQUENCE {	dot11MACAddress                 MacAddress,
            		dot11RTSThreshold               INTEGER,
            		dot11ShortRetryLimit            INTEGER,
            		dot11LongRetryLimit             INTEGER,
            		dot11FragmentationThreshold     INTEGER,
            		dot11MaxTransmitMSDULifetime    Unsigned32,
            		dot11MaxReceiveLifetime         Unsigned32,
            		dot11ManufacturerID             DisplayString,
            		dot11ProductID                  DisplayString }

dot11MACAddress OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
        	"Unique MAC Address assigned to the STA."
    ::= { dot11OperationEntry 1 }

dot11RTSThreshold OBJECT-TYPE
        SYNTAX INTEGER (0..2347)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "This attribute shall indicate the number of octets in an MPDU,
	        below which an RTS/CTS handshake shall not be performed. An
	        RTS/CTS handshake shall be performed at the beginning of any
	        frame exchange sequence where the MPDU is of type Data or
	        Management, the MPDU has an individual address in the Address1
	        field, and the length of the MPDU is greater than
	        this threshold. (For additional details, refer to Table 21 in
	        9.7.) Setting this attribute to be larger than the maximum
	        MSDU size shall have the effect of turning off the RTS/CTS
	        handshake for frames of Data or Management type transmitted by
	        this STA. Setting this attribute to zero shall have the effect
	        of turning on the RTS/CTS handshake for all frames of Data or
	        Management type transmitted by this STA. The default value of
	        this attribute shall be 2347."
    ::= { dot11OperationEntry 2 }

dot11ShortRetryLimit OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "This attribute shall indicate the maximum number of
	        transmission attempts of a frame, the length of which is less
	        than or equal to dot11RTSThreshold, that shall be made before a
	        failure condition is indicated. The default value of this
	        attribute shall be 7."
    ::= { dot11OperationEntry 3 }

dot11LongRetryLimit OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "This attribute shall indicate the maximum number of
	        transmission attempts of a frame, the length of which is
	        greater than dot11RTSThreshold, that shall be made before a
	        failure condition is indicated. The default value of this
	        attribute shall be 4."
    ::= { dot11OperationEntry 4 }

dot11FragmentationThreshold OBJECT-TYPE
        SYNTAX INTEGER (256..2346)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "This attribute shall specify the current maximum size, in
	        octets, of the MPDU that may be delivered to the PHY. An MSDU
	        shall be broken into fragments if its size exceeds the value
	        of this attribute after adding MAC headers and trailers. An MSDU
	        or MMPDU shall be fragmented when the resulting frame has an
	        individual address in the Address1 field, and the length of the
	        frame is larger than this threshold. The default value for this
	        attribute shall be the lesser of 2346 or the aMPDUMaxLength of
	        the attached PHY and shall never exceed the lesser of 2346 or
	        the  aMPDUMaxLength of the attached PHY. The value of this
	        attribute shall never be less than 256. "
    ::= { dot11OperationEntry 5 }

dot11MaxTransmitMSDULifetime OBJECT-TYPE
        SYNTAX Unsigned32 (1..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
	        "The MaxTransmitMSDULifetime shall be the elapsed time in TU,
	        after the initial transmission of an MSDU, after which further
	        attempts to transmit the MSDU shall be terminated. The default
	        value of this attribute shall be 512."
    ::= { dot11OperationEntry 6 }

dot11MaxReceiveLifetime OBJECT-TYPE
        SYNTAX Unsigned32 (1..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The MaxReceiveLifetime shall be the elapsed time in TU,
            after the initial reception of a fragmented MMPDU or MSDU,
            after which further attempts to reassemble the MMPDU or
            MSDU shall be terminated. The default value shall be
            512."
    ::= { dot11OperationEntry 7 }

dot11ManufacturerID OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The ManufacturerID shall include, at a minimum, the name
            of the manufacturer.  It may include additional
            information at the manufacturer's discretion.  The default
            value of this attribute shall be null."
    ::= { dot11OperationEntry 8 }

dot11ProductID OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The ProductID shall include, at a minimum, an identifier
            that is unique to the manufacturer.  It may include
            additional information at the manufacturer's discretion.
            The default value of this attribute shall be null."
    ::= { dot11OperationEntry 9 }

-- **********************************************************************
-- *    End of dot11OperationEntry  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11Counters TABLE
-- **********************************************************************

dot11CountersTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11CountersEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group containing attributes that are MAC counters.
            Implemented as a table to allow for multiple
            instantiations on an agent."
    ::= { dot11mac 2 }

dot11CountersEntry OBJECT-TYPE
        SYNTAX Dot11CountersEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11CountersEntry Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11CountersTable 1 }

Dot11CountersEntry ::= 
        SEQUENCE {	dot11TransmittedFragmentCount       Counter32,
            		dot11MulticastTransmittedFrameCount Counter32,
            		dot11FailedCount                    Counter32,
            		dot11RetryCount                     Counter32,
            		dot11MultipleRetryCount             Counter32,
            		dot11FrameDuplicateCount            Counter32,
            		dot11RTSSuccessCount                Counter32,
            		dot11RTSFailureCount                Counter32,
            		dot11ACKFailureCount                Counter32,
            		dot11ReceivedFragmentCount          Counter32,
            		dot11MulticastReceivedFrameCount    Counter32,
            		dot11FCSErrorCount                  Counter32,
		    		dot11TransmittedFrameCount          Counter32,
		    		dot11WEPUndecryptableCount          Counter32 }

dot11TransmittedFragmentCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall be incremented for an acknowledged MPDU
            with an individual address in the address 1 field or an MPDU
            with a multicast address in the address 1 field of type Data
            or Management."
    ::= { dot11CountersEntry 1 }

dot11MulticastTransmittedFrameCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment only when the multicast bit
            is set in the destination MAC address of a successfully
            transmitted MSDU.  When operating as a STA in an ESS, where
            these frames are directed to the AP, this implies having
            received an acknowledgment to all associated MPDUs."
    ::= { dot11CountersEntry 2 }

dot11FailedCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "This counter shall increment when an MSDU is not transmitted
	        successfully due to the number of transmit attempts exceeding
	        either the  dot11ShortRetryLimit or dot11LongRetryLimit."
    ::= { dot11CountersEntry 3 }

dot11RetryCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when an MSDU is successfully
            transmitted after one or more retransmissions."
    ::= { dot11CountersEntry 4 }

dot11MultipleRetryCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when an MSDU is successfully
            transmitted after more than one retransmission."
    ::= { dot11CountersEntry 5 }

dot11FrameDuplicateCount  OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when a frame is received
            that the Sequence Control field indicates is a
            duplicate."
    ::= { dot11CountersEntry 6 }

dot11RTSSuccessCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when a CTS is received in
            response to an RTS."
    ::= {  dot11CountersEntry 7 }

dot11RTSFailureCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "This counter shall increment when a CTS is not received in
	        response to an RTS."
    ::= { dot11CountersEntry 8 }

dot11ACKFailureCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when an ACK is not received
            when expected."
    ::= {  dot11CountersEntry 9 }

dot11ReceivedFragmentCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall be incremented for each successfully
            received MPDU of type Data or Management."
    ::= { dot11CountersEntry 10 }

dot11MulticastReceivedFrameCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when a MSDU is received
            with the multicast bit set in the destination
            MAC address."
    ::= { dot11CountersEntry 11 }

dot11FCSErrorCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when an FCS error is
            detected in a received MPDU."
    ::= { dot11CountersEntry 12 }

dot11TransmittedFrameCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
			"This counter shall increment for each successfully transmitted MSDU."
    ::= { dot11CountersEntry 13 }

dot11WEPUndecryptableCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "This counter shall increment when a frame is received with
	        the WEP subfield of the Frame Control field set to one and the
	        WEPOn value for the key mapped to the TA's MAC address
	        indicates that the frame should not have been encrypted or
	        that frame is discarded due to the receiving STA not
	        implementing the privacy option."
    ::= { dot11CountersEntry 14 }

-- **********************************************************************
-- *    End of dot11CountersEntry  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    GroupAddresses  TABLE
-- **********************************************************************

dot11GroupAddressesTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11GroupAddressesEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A conceptual table containing a set of MAC addresses
            identifying the multicast addresses for which this STA
            will receive frames.  The default value of this attribute
            shall be null."
    ::= { dot11mac 3 }

dot11GroupAddressesEntry OBJECT-TYPE
        SYNTAX Dot11GroupAddressesEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the Group Addresses Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex, 
                dot11GroupAddressesIndex}
    ::= { dot11GroupAddressesTable  1 }

Dot11GroupAddressesEntry ::= 
        SEQUENCE {	dot11GroupAddressesIndex    Integer32,
            		dot11Address                MacAddress,
            		dot11GroupAddressesStatus   RowStatus }

dot11GroupAddressesIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the Group Addresses Table."
    ::= { dot11GroupAddressesEntry 1 }

dot11Address OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "MAC address identifying a multicast addresses
            from which this STA will receive frames."
    ::= { dot11GroupAddressesEntry 2 }

dot11GroupAddressesStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The status column used for creating, modifying, and
            deleting instances of the columnar objects in the Group
            Addresses Table."
        DEFVAL { active }
    ::= { dot11GroupAddressesEntry 3 }

-- **********************************************************************
-- *    End of GroupAddress  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    Resource Type Attribute Templates
-- **********************************************************************

dot11ResourceTypeIDName OBJECT-TYPE
        SYNTAX DisplayString (SIZE(4))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Contains the name of the Resource Type ID managed object.
            The attribute is read-only and always contains the value
            RTID.  This attribute value shall not be used as a naming
            attribute for any other managed object class."
        REFERENCE "IEEE Std 802.1F-1993,  A.7"
        DEFVAL { "RTID" }
    ::= { dot11resAttribute 1 }

-- **********************************************************************
-- *    dot11ResourceInfo  TABLE
-- **********************************************************************

dot11ResourceInfoTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11ResourceInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Provides a means of indicating, in data readable from a
            managed object, information that identifies the source of
            the implementation."
        REFERENCE "IEEE Std 802.1F-1993,  A.7"
    ::= { dot11resAttribute 2 }

dot11ResourceInfoEntry OBJECT-TYPE
        SYNTAX Dot11ResourceInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11ResourceInfo Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11ResourceInfoTable 1 }

Dot11ResourceInfoEntry ::= 
        SEQUENCE {	dot11manufacturerOUI             OCTET STRING,
            		dot11manufacturerName            DisplayString,
            		dot11manufacturerProductName     DisplayString,
            		dot11manufacturerProductVersion  DisplayString }

dot11manufacturerOUI OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(3))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Takes the value of an organizationally unique identifier."
    ::= { dot11ResourceInfoEntry 1 }

dot11manufacturerName OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "A printable string used to identify the manufacturer of the
            resource.  Maximum string length is 128 octets."
    ::= { dot11ResourceInfoEntry 2 }

dot11manufacturerProductName OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "A printable string used to identify the manufacturer's product
            name of the resource.  Maximum string length is 128 octets."
    ::= { dot11ResourceInfoEntry 3 }

dot11manufacturerProductVersion OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Printable string used to identify the manufacturer's product
            version of the resource.  Maximum string length is 128 octets."
    ::= { dot11ResourceInfoEntry 4 }

-- **********************************************************************
-- *    End of dot11ResourceInfo  TABLE
-- **********************************************************************

-- **********************************************************************
-- *   PHY Attribute Templates
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyOperation  TABLE
-- **********************************************************************

dot11PhyOperationTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyOperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
	        "PHY level attributes concerned with
	        operation.  Implemented as a table indexed on

	        ifIndex to allow for multiple instantiations on an
	        Agent."
    ::= { dot11phy 1 }

dot11PhyOperationEntry OBJECT-TYPE
        SYNTAX Dot11PhyOperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyOperation Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PhyOperationTable 1 }

Dot11PhyOperationEntry ::= 
        SEQUENCE {	dot11PHYType            INTEGER,
            		dot11CurrentRegDomain   Integer32,
            		dot11TempType           INTEGER }

dot11PHYType OBJECT-TYPE
        SYNTAX INTEGER { fhss(1), dsss(2), irbaseband(3), ofdm(4),
			             hrdsss(5) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "This is an 8-bit integer value that identifies the PHY type
	        supported by the attached PLCP and PMD. Currently defined
	        values and their corresponding PHY types are:
	
	        FHSS 2.4 GHz = 01 , DSSS 2.4 GHz = 02, IR Baseband = 03,
			OFDM 5GHz = 04, HRDSSS = 05"
    ::= { dot11PhyOperationEntry 1 }

dot11CurrentRegDomain OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current regulatory domain this instance of the PMD is
            supporting.  This object corresponds to one of the
            RegDomains listed in dot11RegDomainsSupported."
    ::= { dot11PhyOperationEntry 2 }

dot11TempType OBJECT-TYPE
        SYNTAX INTEGER { tempType1(1), tempType2(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "There are different operating temperature requirements
	        dependent on the anticipated environmental conditions. This
	        attribute describes the current PHY's operating temperature
	        range capability. Currently defined values and their
	        corresponding temperature ranges are:

	        Type 1 = X'01'-Commercial range of 0 to 40 degrees C,

	        Type 2 = X'02'-Industrial range of -30 to 70 degrees C."
    ::= { dot11PhyOperationEntry 3 }

-- **********************************************************************
-- *    End of dot11PhyOperation  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyAntenna  TABLE
-- **********************************************************************

dot11PhyAntennaTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyAntennaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group of attributes for PhyAntenna.  Implemented as a
            table indexed on ifIndex to allow for multiple instances on
            an agent."
    ::= { dot11phy 2}

dot11PhyAntennaEntry OBJECT-TYPE
        SYNTAX Dot11PhyAntennaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyAntenna Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PhyAntennaTable 1 }

Dot11PhyAntennaEntry ::= 
        SEQUENCE {	dot11CurrentTxAntenna  Integer32,
             		dot11DiversitySupport  INTEGER,
	     			dot11CurrentRxAntenna  Integer32 }

dot11CurrentTxAntenna OBJECT-TYPE
        SYNTAX Integer32 (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current antenna being used to transmit.  This value
	        is one of the values appearing in dot11SupportedTxAntenna. This 
	        may be used by a management agent to control which antenna is 
	        used for transmission. "
    ::= { dot11PhyAntennaEntry 1 }

dot11DiversitySupport OBJECT-TYPE
        SYNTAX INTEGER { fixedlist(1), notsupported(2), dynamic(3) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
	        "This implementation's support for diversity, encoded as:

	        X'01'-diversity is available and is performed over the fixed
	            list of antennas defined in dot11DiversitySelectionRx.

	        X'02'-diversity is not supported.

	        X'03'-diversity is supported and control of diversity is also
	            available, in which case the attribute 
	            dot11DiversitySelectionRx can be dynamically modified by the
	            LME."
    ::= { dot11PhyAntennaEntry 2 }

dot11CurrentRxAntenna OBJECT-TYPE
        SYNTAX Integer32 (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
			"The current antenna being used to receive, if the dot11 
			DiversitySupport indicates that diversity is not supported.  
			The selected antenna shall be one of the antennae marked 
			for receive in the dot11AntennasListTable."
    ::= { dot11PhyAntennaEntry 3 }

-- **********************************************************************
-- *    End of dot11PhyAntenna  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyTxPower  TABLE
-- **********************************************************************

dot11PhyTxPowerTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyTxPowerEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group of attributes for dot11PhyTxPowerTable.  Implemented
            as a table indexed on STA ID to allow for multiple
            instances on an Agent."
    ::= { dot11phy 3}

dot11PhyTxPowerEntry OBJECT-TYPE
        SYNTAX Dot11PhyTxPowerEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyTxPower Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PhyTxPowerTable 1 }

Dot11PhyTxPowerEntry ::= 
        SEQUENCE {	dot11NumberSupportedPowerLevels  INTEGER,
            		dot11TxPowerLevel1               INTEGER,
            		dot11TxPowerLevel2               INTEGER,
            		dot11TxPowerLevel3               INTEGER,
            		dot11TxPowerLevel4               INTEGER,
            		dot11TxPowerLevel5               INTEGER,
            		dot11TxPowerLevel6               INTEGER,
            		dot11TxPowerLevel7               INTEGER,
            		dot11TxPowerLevel8               INTEGER,
            		dot11CurrentTxPowerLevel         INTEGER }

dot11NumberSupportedPowerLevels OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of power levels supported by the PMD.
            This attribute can have a value of 1 to 8."
    ::= { dot11PhyTxPowerEntry 1 }

dot11TxPowerLevel1 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL1 in mW.
            This is also the default power level."
    ::= { dot11PhyTxPowerEntry 2 }

dot11TxPowerLevel2 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL2 in mW."
    ::= { dot11PhyTxPowerEntry 3 }

dot11TxPowerLevel3 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL3 in mW."
    ::= { dot11PhyTxPowerEntry 4 }

dot11TxPowerLevel4 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL4 in mW."
    ::= { dot11PhyTxPowerEntry 5 }

dot11TxPowerLevel5 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL5 in mW."
    ::= { dot11PhyTxPowerEntry 6 }

dot11TxPowerLevel6 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL6 in mW."
    ::= { dot11PhyTxPowerEntry 7 }

dot11TxPowerLevel7 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL7 in mW."
    ::= { dot11PhyTxPowerEntry 8 }

dot11TxPowerLevel8 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL8 in mW."
    ::= { dot11PhyTxPowerEntry 9 }

dot11CurrentTxPowerLevel OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The TxPowerLevel N currently being used to transmit data.
            Some PHYs also use this value to determine the receiver
            sensitivity requirements for CCA."
    ::= { dot11PhyTxPowerEntry 10 }

-- **********************************************************************
-- *    End of dot11PhyTxPower  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyFHSS  TABLE
-- **********************************************************************

dot11PhyFHSSTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyFHSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group of attributes for dot11PhyFHSSTable.  Implemented as a
            table indexed on STA ID to allow for multiple instances on
            an Agent."
    ::= { dot11phy 4 }

dot11PhyFHSSEntry OBJECT-TYPE
        SYNTAX Dot11PhyFHSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyFHSS Table.
            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PhyFHSSTable 1 }

Dot11PhyFHSSEntry ::= 
        SEQUENCE {	dot11HopTime   				INTEGER,
             		dot11CurrentChannelNumber  		INTEGER,
             		dot11MaxDwellTime  			INTEGER,
             		dot11CurrentDwellTime  			INTEGER,
             		dot11CurrentSet    			INTEGER,
             		dot11CurrentPattern    			INTEGER,
             		dot11CurrentIndex  			INTEGER,
 			dot11EHCCPrimeRadix			Integer32, 
			dot11EHCCNumberofChannelsFamilyIndex	Integer32,
			dot11EHCCCapabilityImplemented		TruthValue, 
			dot11EHCCCapabilityEnabled		TruthValue,
			dot11HopAlgorithmAdopted		INTEGER,
			dot11RandomTableFlag			TruthValue,
			dot11NumberofHoppingSets		Integer32,
			dot11HopModulus				Integer32,
			dot11HopOffset				Integer32 }

dot11HopTime OBJECT-TYPE
        SYNTAX INTEGER (224)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The time in microseconds for the PMD to change from
            channel 2 to channel 80."
    ::= { dot11PhyFHSSEntry 1 }

dot11CurrentChannelNumber OBJECT-TYPE
        SYNTAX INTEGER (0..200)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        	"The current channel number of the frequency output by the RF
        	synthesizer."
    ::= { dot11PhyFHSSEntry 2 }

dot11MaxDwellTime OBJECT-TYPE
        SYNTAX INTEGER (1..65535)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The maximum time in TU that the transmitter
            is permitted to operate on a single channel."
    ::= { dot11PhyFHSSEntry 3 }

dot11CurrentDwellTime OBJECT-TYPE
        SYNTAX INTEGER (1..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current time in TU that the transmitter shall operate
            on a single channel, as set by the MAC.  Default is 19 TU."
    ::= { dot11PhyFHSSEntry 4 }

dot11CurrentSet OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current set of patterns the PLME 
	    is using to determine the hopping sequence. "
    ::= { dot11PhyFHSSEntry 5 }

dot11CurrentPattern OBJECT-TYPE
        SYNTAX INTEGER (0..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current pattern the PLME is
            using to determine the hop sequence."
    ::= { dot11PhyFHSSEntry 6 }

dot11CurrentIndex OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current index value the PLME is using to determine
            the CurrentChannelNumber."
    ::= { dot11PhyFHSSEntry 7 }

dot11EHCCPrimeRadix OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute indicates the value to be 
			used as the prime radix (N) in the HCC and 
			EHCC algorithms."
    ::= { dot11PhyFHSSEntry 8 }

dot11EHCCNumberofChannelsFamilyIndex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute indicates the value to be 
			used as the maximum for the family index (a) 
			in the HCC and EHCC algorithms. The value of 
			this field shall not be less than the prime 
			radix minus 3 (N - 3). The valid range of 
			allowed values is (N - 1), (N - 2), and (N - 3)."
    ::= { dot11PhyFHSSEntry 9 }

dot11EHCCCapabilityImplemented OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute, when TRUE, indicates that the 
			station implementation is capable of generating 
			the HCC or EHCC algorithms for determining Hopping 
			patterns.  The capability is disabled, otherwise.  
			The default value of this attribute is FALSE."
    ::= { dot11PhyFHSSEntry 10 }

dot11EHCCCapabilityEnabled OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute, when TRUE, indicates that the 
			capability of the station to operate using the HCC 
			or EHCC algorithms for determining Hopping Patterns 
			is enabled.  The capability is disabled, otherwise.  
			The default value of this attribute is FALSE."
    ::= { dot11PhyFHSSEntry 11 }

dot11HopAlgorithmAdopted OBJECT-TYPE
		SYNTAX INTEGER { crnt(1), hopindex(2), hcc(3) }
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute, indicates which of the algorithms 
			will be used to generate the Hopping Patterns. 
			Valid values are: 
	
			1 - hopping patterns as defined in clause 14 
			2 - hop index method (with or without table)
			3 - HCC/EHCC method"
    ::= { dot11PhyFHSSEntry 12 }

dot11RandomTableFlag OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute, indicates that a Random Table is 
			present when the value is True. When the value is 
			False it indicates that a Random Table is not 
			present and that the hop index method is to be 
			used to determine the hopping sequence. The default 
			value of this attribute is True."
    ::= { dot11PhyFHSSEntry 13 }

dot11NumberofHoppingSets OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The Number of Sets field indicates the total 
			number of sets within the hopping patterns."
    ::= { dot11PhyFHSSEntry 14 }

dot11HopModulus OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"The number of allowed channels for the hopping 
			set. This is defined by the governing regulatory 
			agency for the country code of the country 
			in which this device is operating."
    ::= { dot11PhyFHSSEntry 15 }

dot11HopOffset OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"The next position in the hopping set."
    ::= { dot11PhyFHSSEntry 16 }

-- **********************************************************************
-- *    End of dot11PhyFHSS  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyDSSSEntry  TABLE
-- **********************************************************************

dot11PhyDSSSTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyDSSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Entry of attributes for dot11PhyDSSSEntry.  Implemented as a
            table indexed on ifIndex allow for multiple instances on
            an Agent."
    ::= { dot11phy 5 }

dot11PhyDSSSEntry OBJECT-TYPE
        SYNTAX Dot11PhyDSSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyDSSSEntry Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PhyDSSSTable 1 }

Dot11PhyDSSSEntry ::= 
        SEQUENCE {	dot11CurrentChannel    INTEGER,
             		dot11CCAModeSupported  INTEGER,
             		dot11CurrentCCAMode    INTEGER,
             		dot11EDThreshold       Integer32 }

dot11CurrentChannel OBJECT-TYPE
        SYNTAX INTEGER (1..14)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current operating frequency channel of the DSSS
            PHY. Valid channel numbers are as defined in 15.4.6.2"
    ::= { dot11PhyDSSSEntry 1 }

dot11CCAModeSupported OBJECT-TYPE
        SYNTAX INTEGER (1..7)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            	"dot11CCAModeSupported is a bit-significant value,
	  	representing all of the CCA modes supported by the PHY.
		Valid values are:

            	   energy detect only (ED_ONLY) = 01,
		   carrier sense only (CS_ONLY) = 02,
		   carrier sense and energy detect (ED_and_CS)= 04
		   or the logical sum of any of these values.  This
		   attribute shall not be used to indicate the CCA modes
		   supported by a higher rate extension PHY.  Rather, the
		   dot11HRCCAModeSupported attribute shall be used to
		   indicate the CCA modes of the higher rate extension PHY."
    ::= { dot11PhyDSSSEntry 2 }

dot11CurrentCCAMode OBJECT-TYPE
        SYNTAX INTEGER { edonly(1), csonly(2), edandcs(4), cswithtimer(8),
			             hrcsanded(16) }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current CCA method in operation.   Valid values are:
                energy detect only (edonly) = 01,
                carrier sense only (csonly) = 02,
                carrier sense and energy detect (edandcs)= 04
                carrier sense with timer (cswithtimer)= 08
                high rate carrier sense and energy detect (hrcsanded)=16."
    ::= { dot11PhyDSSSEntry 3 }

dot11EDThreshold OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current Energy Detect Threshold being used by the DSSS PHY."
    ::= { dot11PhyDSSSEntry 4 }

-- **********************************************************************
-- *    End of dot11PhyDSSSEntry  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyIR  TABLE
-- **********************************************************************

dot11PhyIRTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyIREntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group of attributes for dot11PhyIRTable.  Implemented as a
            table indexed on ifIndex to allow for multiple instances on
            an Agent."
    ::= { dot11phy 6 }

dot11PhyIREntry OBJECT-TYPE
        SYNTAX Dot11PhyIREntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyIR Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PhyIRTable 1 }

Dot11PhyIREntry ::= 
        SEQUENCE {	dot11CCAWatchdogTimerMax       Integer32,
             		dot11CCAWatchdogCountMax       Integer32,
             		dot11CCAWatchdogTimerMin       Integer32,
             		dot11CCAWatchdogCountMin       Integer32 }

dot11CCAWatchdogTimerMax OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This parameter, together with CCAWatchdogCountMax,
            determines when energy detected in the channel can be
            ignored."
    ::= { dot11PhyIREntry 1 }

dot11CCAWatchdogCountMax OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This parameter, together with CCAWatchdogTimerMax,
            determines when energy detected in the channel can be
            ignored."
    ::= { dot11PhyIREntry 2 }

dot11CCAWatchdogTimerMin OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The minimum value to which CCAWatchdogTimerMax can be
            set."
    ::= { dot11PhyIREntry 3 }

dot11CCAWatchdogCountMin OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The minimum value to which CCAWatchdogCount can be set."
    ::= { dot11PhyIREntry 4 }

-- **********************************************************************
-- *    End of dot11PhyIR  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11RegDomainsSupported  TABLE
-- **********************************************************************

dot11RegDomainsSupportedTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11RegDomainsSupportedEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "There are different operational requirements dependent on
            the regulatory domain.  This attribute list describes the
            regulatory domains the PLCP and PMD support in this
            implementation.  Currently defined values and their
            corresponding Regulatory Domains are:

            FCC (USA) = X'10', DOC (Canada) = X'20', ETSI (most of
            Europe) = X'30', Spain = X'31', France = X'32', MKK
            (Japan) = X'40', Others = X'00' "
    ::= { dot11phy 7}

dot11RegDomainsSupportedEntry OBJECT-TYPE
        SYNTAX Dot11RegDomainsSupportedEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11RegDomainsSupportedTable.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex, 
                dot11RegDomainsSupportedIndex }
    ::= { dot11RegDomainsSupportedTable 1 }

Dot11RegDomainsSupportedEntry ::= 
        SEQUENCE {	dot11RegDomainsSupportedIndex    Integer32,
             		dot11RegDomainsSupportedValue    INTEGER }

dot11RegDomainsSupportedIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the RegDomainsSupport Table."
    ::= { dot11RegDomainsSupportedEntry 1 }

dot11RegDomainsSupportedValue OBJECT-TYPE
        SYNTAX INTEGER { fcc(16), doc(32), etsi(48), spain (49), france(50), 
                         mkk (64) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "There are different operational requirements dependent on
            the regulatory domain.  This attribute list describes the
            regulatory domains the PLCP and PMD support in this
            implementation.  Currently defined values and their
            corresponding Regulatory Domains are:

            FCC (USA) = X'10', DOC (Canada) = X'20', ETSI (most of
            Europe) = X'30', Spain = X'31', France = X'32', MKK
            (Japan) = X'40' "
    ::= { dot11RegDomainsSupportedEntry 2 }

-- **********************************************************************
-- *    End of dot11RegDomainsSupported  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11AntennasList  TABLE
-- **********************************************************************

dot11AntennasListTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11AntennasListEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
		"This table represents the list of antennae.  An antenna can be 
		marked to be capable of transmitting, receiving, and/or for 
		participation in receive diversity.  Each entry in this table 
		represents a single antenna with its properties.  The maximum 
		number of antennae that can be contained in this table is 255."
    ::= { dot11phy 8 }

dot11AntennasListEntry OBJECT-TYPE
        SYNTAX Dot11AntennasListEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11AntennasListTable, representing the properties 
            of a single antenna.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex, 
                dot11AntennaListIndex }
    ::= { dot11AntennasListTable 1 }

Dot11AntennasListEntry ::= 
        SEQUENCE {	dot11AntennaListIndex     Integer32,
             		dot11SupportedTxAntenna   TruthValue,
             		dot11SupportedRxAntenna   TruthValue,
             		dot11DiversitySelectionRx TruthValue }

dot11AntennaListIndex OBJECT-TYPE
        SYNTAX Integer32 (1..255)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The unique index of an antenna which is used to identify the columnar 
            objects in the dot11AntennasList Table."
    ::= { dot11AntennasListEntry 1 }

dot11SupportedTxAntenna OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "When true, this object indicates that the antenna represented by 
            dot11AntennaIndex can be used as a transmit antenna."
    ::= { dot11AntennasListEntry 2 }

dot11SupportedRxAntenna OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "When true, this object indicates that the antenna represented by the 
            dot11AntennaIndex xan be used as a receive antenna."
    ::= { dot11AntennasListEntry 3 }

dot11DiversitySelectionRx OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "When true, this object indicates that the antenna represented by 
            dot11AntennaIndex can be used for receive diversity.  This object 
            may only be true if the antenna can be used as a receive antenna, 
            as indicated by dot11SupportedRxAntenna."
    ::= { dot11AntennasListEntry 4 }

-- **********************************************************************
-- *    End of dot11AntennasList  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    SupportedDataRatesTx  TABLE
-- **********************************************************************

dot11SupportedDataRatesTxTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11SupportedDataRatesTxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The Transmit bit rates supported by the PLCP and PMD,
            represented by a count from X'02-X'7f, corresponding to data
            rates in increments of 500kbit/s from 1 Mbit/s to 63.5 Mbit/s subject
            to limitations of each individual PHY."
    ::= { dot11phy 9 }

dot11SupportedDataRatesTxEntry OBJECT-TYPE
        SYNTAX Dot11SupportedDataRatesTxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the dot11SupportedDataRatesTx
            Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex, 
                dot11SupportedDataRatesTxIndex }
    ::= { dot11SupportedDataRatesTxTable  1 }

Dot11SupportedDataRatesTxEntry ::= 
        SEQUENCE {	dot11SupportedDataRatesTxIndex  Integer32,
            		dot11SupportedDataRatesTxValue  Integer32 }

dot11SupportedDataRatesTxIndex OBJECT-TYPE
        SYNTAX Integer32 (1..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Index object which identifies which data rate to access.
            Range is 1..8."
    ::= { dot11SupportedDataRatesTxEntry 1 }

dot11SupportedDataRatesTxValue OBJECT-TYPE
        SYNTAX Integer32 (2..127)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The Transmit bit rates supported by the PLCP and PMD,
            represented by a count from X'02-X'7f, corresponding to data
            rates in increments of 500kbit/s from 1 Mbit/s to 63.5 Mbit/s subject
            to limitations of each individual PHY."
    ::= { dot11SupportedDataRatesTxEntry 2 }

-- **********************************************************************
-- *    End of dot11SupportedDataRatesTx  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    SupportedDataRatesRx  TABLE
-- **********************************************************************

dot11SupportedDataRatesRxTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11SupportedDataRatesRxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The receive bit rates supported by the PLCP and PMD,
            represented by a count from X'002-X'7f, corresponding to data
            rates in increments of 500kbit/s from 1 Mbit/s to 63.5 Mbit/s."
    ::= { dot11phy 10 }

dot11SupportedDataRatesRxEntry OBJECT-TYPE
        SYNTAX Dot11SupportedDataRatesRxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the dot11SupportedDataRatesRx Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex, 
                dot11SupportedDataRatesRxIndex }
    ::= { dot11SupportedDataRatesRxTable  1 }

Dot11SupportedDataRatesRxEntry ::= 
        SEQUENCE {	dot11SupportedDataRatesRxIndex  Integer32,
            		dot11SupportedDataRatesRxValue  Integer32 }

dot11SupportedDataRatesRxIndex OBJECT-TYPE
        SYNTAX Integer32 (1..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Index object which identifies which data rate to access.
            Range is 1..8."
    ::= { dot11SupportedDataRatesRxEntry 1 }

dot11SupportedDataRatesRxValue OBJECT-TYPE
        SYNTAX Integer32 (2..127)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The receive bit rates supported by the PLCP and PMD,
            represented by a count from X'02-X'7f, corresponding to data
            rates in increments of 500kbit/s from 1 Mbit/s to 63.5 Mbit/s."
    ::= { dot11SupportedDataRatesRxEntry 2 }

-- **********************************************************************
-- *    End of dot11SupportedDataRatesRx  TABLE
-- **********************************************************************

--**********************************************************************
-- * dot11PhyOFDM TABLE
--**********************************************************************

dot11PhyOFDMTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyOFDMEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Group of attributes for dot11PhyOFDMTable. Implemented as a
            table indexed on ifindex to allow for multiple instances on
            an Agent."
    ::= { dot11phy 11 }

dot11PhyOFDMEntry OBJECT-TYPE
        SYNTAX Dot11PhyOFDMEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyOFDM Table.

            ifIndex - Each IEEE 802.11 interface is represented by an
            ifEntry. Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX { ifIndex }
    ::= { dot11PhyOFDMTable 1 }

Dot11PhyOFDMEntry ::= 
        SEQUENCE {	dot11CurrentFrequency        INTEGER,
            		dot11TIThreshold             Integer32,
            		dot11FrequencyBandsSupported INTEGER }

dot11CurrentFrequency OBJECT-TYPE
        SYNTAX INTEGER (0..99)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The number of the current operating frequency channel of the OFDM PHY."
    ::= { dot11PhyOFDMEntry 1 }

dot11TIThreshold OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The Threshold being used to detect a busy medium (frequency).
            CCA shall report a busy medium upon detecting the RSSI above 
	    this threshold."
    ::= { dot11PhyOFDMEntry 2 }

dot11FrequencyBandsSupported OBJECT-TYPE
        SYNTAX INTEGER (1..7)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The capability of the OFDM PHY implementation to operate in 
	    the three U-NII bands. Coded as an integer value of a three 
	    bit field as follows:
                bit 0 .. capable of operating in the lower (5.15-5.25 GHz)
		U-NII band
                bit 1 .. capable of operating in the middle (5.25-5.35 GHz) 
		U-NII band
                bit 2 .. capable of operating in the upper (5.725-5.825 GHz) 
		U-NII band
            For example, for an implementation capable of operating in the 
	    lower and mid bands this attribute would take the value 3."
    ::= { dot11PhyOFDMEntry 3 }

-- **********************************************************************
-- * End of dot11PhyOFDM TABLE
-- **********************************************************************

-- **********************************************************************
-- *	dot11PhyHRDSSSEntry TABLE
-- **********************************************************************

dot11PhyHRDSSSTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Dot11PhyHRDSSSEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"Entry of attributes for dot11PhyHRDSSSEntry.
			Implemented as a table indexed on ifIndex to allow for
			multiple instances on an Agent."
    ::= { dot11phy 12 }

dot11PhyHRDSSSEntry OBJECT-TYPE
		SYNTAX Dot11PhyHRDSSSEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"An entry in the dot11PhyHRDSSSEntry Table.

			ifIndex - Each IEEE 802.11 interface is represented by an
			ifEntry. Interface tables in this MIB module are indexed
			by ifIndex."
	INDEX { ifIndex }
    ::= { dot11PhyHRDSSSTable 1 }

Dot11PhyHRDSSSEntry ::= 
        SEQUENCE {	dot11ShortPreambleOptionImplemented	TruthValue,
			dot11PBCCOptionImplemented		TruthValue,
			dot11ChannelAgilityPresent 		TruthValue,
			dot11ChannelAgilityEnabled 		TruthValue,
			dot11HRCCAModeSupported			INTEGER }

dot11ShortPreambleOptionImplemented OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute, when true, shall indicate that the
			short preamble option as defined in subclause 18.2.2.2
			is implemented.  The default value of this attribute
			shall be false."
    ::= {dot11PhyHRDSSSEntry 1 }

dot11PBCCOptionImplemented OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute, when true, shall indicate that the PBCC
			modulation option as defined in subclause 18.4.6.6 is
			implemented.  The default value of this attribute shall
			be false."
    ::= {dot11PhyHRDSSSEntry 2 }

dot11ChannelAgilityPresent OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute indicates that the PHY is capable of
			channel agility."
    ::= { dot11PhyHRDSSSEntry 3 }

dot11ChannelAgilityEnabled OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"This attribute indicates that the PHY channel agility
			functionality is enabled."
    ::= { dot11PhyHRDSSSEntry 4 }

dot11HRCCAModeSupported OBJECT-TYPE
		SYNTAX INTEGER (1..31)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"dot11HRCCAModeSupported is a bit-significant value,
			representing all of the CCA modes supported by the PHY.
			Valid values are:
			    energy detect only (ED_ONLY) = 01,
			    carrier sense only (CS_ONLY) = 02,
			    carrier sense and energy detect (ED_and_CS)= 04,
			    carrier sense with timer (CS_and_Timer)= 08,
			    high rate carrier sense and energy detect 
			    (HRCS_and_ED)= 16
			    or the logical sum of any of these values.  In 
			    the high rate extension PHY, this attribute shall 
			    be used in preference to the dot11CCAModeSupported 
			    attribute."
    ::= { dot11PhyHRDSSSEntry 5 }

-- **********************************************************************
-- * End of dot11PhyHRDSSSEntry TABLE
-- **********************************************************************

-- ********************************************************************
-- * dot11 Hopping Pattern TABLE
-- ********************************************************************

dot11HoppingPatternTable OBJECT-TYPE
		SYNTAX SEQUENCE OF Dot11HoppingPatternEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The (conceptual) table of attributes necessary for 
			a frequency hopping implementation to be able to 
			create the hopping sequences necessary to operate 
			in the subband for the associated domain country string."
		::= { dot11phy 13 }

dot11HoppingPatternEntry OBJECT-TYPE
		SYNTAX Dot11HoppingPatternEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"An entry (conceptual row) in the Hopping Pattern Table 
			that indicates the random hopping sequence to be followed. 

			IfIndex - Each IEEE 802.11 interface is represented 
			by an ifEntry. Interface tables in this MIB are indexed 
			by ifIndex."
		INDEX { ifIndex,
				dot11HoppingPatternIndex }
    ::= { dot11HoppingPatternTable 1 }

Dot11HoppingPatternEntry ::=
		SEQUENCE {	
			dot11HoppingPatternIndex		Integer32,
			dot11RandomTableFieldNumber		Integer32 }

dot11HoppingPatternIndex OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"The auxiliary variable used to identify instances of 
			the columnar objects in the Hopping Pattern Table."
    ::= { dot11HoppingPatternEntry 1}

dot11RandomTableFieldNumber OBJECT-TYPE
		SYNTAX Integer32
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
			"This attribute shall indicate the value of the 
			starting channel number in the hopping sequence of 
			the subband for the associated domain country string. 
			The default value of this attribute shall be zero."
    ::= { dot11HoppingPatternEntry 2}

-- **********************************************************************
-- * End of dot11 Hopping Pattern TABLE 
--**********************************************************************

-- **********************************************************************
-- * Conformance Information
-- **********************************************************************

dot11Conformance  	OBJECT IDENTIFIER ::= { ieee802dot11 5 }
dot11Groups  		OBJECT IDENTIFIER ::= { dot11Conformance 1 }
dot11Compliances  	OBJECT IDENTIFIER ::= { dot11Conformance 2 }

-- **********************************************************************
-- * Compliance Statements
-- **********************************************************************

dot11Compliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
            "The compliance statement for SNMPv2 entities
            that implement the IEEE 802.11 MIB."
    	MODULE  -- this module
    	MANDATORY-GROUPS {
		dot11SMTbase2,
        	dot11MACbase, dot11CountersGroup,
        	dot11SmtAuthenticationAlgorithms, 
        	dot11ResourceTypeID, dot11PhyOperationComplianceGroup }

   GROUP dot11PhyDSSSComplianceGroup
        DESCRIPTION
        	"Implementation of this group is required when object
            dot11PHYType has the value of dsss.  This group is
            mutually exclusive with the groups dot11PhyIRComplianceGroup,
            dot11PhyFHSSComplianceGroup, dot11PhyOFDMComplianceGroup
	        and dot11PhyHRDSSSComplianceGroup."

    GROUP dot11PhyIRComplianceGroup
        DESCRIPTION
            "Implementation of this group is required when object
            dot11PHYType has the value of irbaseband.  This group is
            mutually exclusive with the groups dot11PhyDSSSComplianceGroup,
            dot11PhyFHSSComplianceGroup, dot11PhyOFDMComplianceGroup
	        and dot11PhyHRDSSSComplianceGroup."

    GROUP dot11PhyFHSSComplianceGroup
        DESCRIPTION
            "Implementation of this group is required when object
            dot11PHYType has the value of fhss.  This group is
            mutually exclusive with the groups dot11PhyDSSSComplianceGroup,
            dot11PhyIRComplianceGroup, dot11PhyOFDMComplianceGroup
	        and dot11PhyHRDSSSComplianceGroup."

    GROUP dot11PhyOFDMComplianceGroup
        DESCRIPTION
            "Implementation of this group is required when object
            dot11PHYType has the value of ofdm. This group is
            mutually exclusive with the groups dot11PhyDSSSComplianceGroup,
            dot11PhyIRComplianceGroup, dot11PhyFHSSComplianceGroup
	        and dot11PhyHRDSSSComplianceGroup."

    GROUP dot11PhyHRDSSSComplianceGroup
	    DESCRIPTION
	    "Implementation of this group is required when object
	    dot11PHYType has the value of hrdsss. This group is
	    mutually exclusive with the groups
	    dot11PhyDSSSComplianceGroup, dot11PhyIRComplianceGroup,
	    dot11PhyFHSSComplianceGroup and dot11PhyOFDMComplianceGroup."

    -- OPTIONAL-GROUPS { dot11SMTprivacy, dot11MACStatistics,
    --    dot11PhyAntennaComplianceGroup, dot11PhyTxPowerComplianceGroup, 
    --    dot11PhyRegDomainsSupportGroup,
    --    dot11PhyAntennasListGroup, dot11PhyRateGroup }

    ::= { dot11Compliances 1 }

-- **********************************************************************
-- *   Groups - units of conformance
-- **********************************************************************

dot11SMTbase OBJECT-GROUP
        OBJECTS {	dot11StationID, dot11MediumOccupancyLimit, 
             		dot11CFPollable,
             		dot11CFPPeriod,
             		dot11CFPMaxDuration,
             		dot11AuthenticationResponseTimeOut,
				 	dot11PrivacyOptionImplemented,
			     	dot11PowerManagementMode,
		    	 	dot11DesiredSSID, dot11DesiredBSSType,
		     		dot11OperationalRateSet,
		     		dot11BeaconPeriod, dot11DTIMPeriod,
		     		dot11AssociationResponseTimeOut }
        STATUS deprecated
        DESCRIPTION
        	"The SMT object class provides the necessary support at the
         	STA to manage the processes in the STA such that the STA may
         	work cooperatively as a part of an IEEE 802.11 network."
    ::= { dot11Groups 1 }

dot11SMTprivacy OBJECT-GROUP
        OBJECTS { 	dot11PrivacyInvoked, 
			dot11WEPKeyMappingLength, dot11ExcludeUnencrypted,
			dot11WEPICVErrorCount , dot11WEPExcludedCount ,
			dot11WEPDefaultKeyID,
                	dot11WEPDefaultKeyValue,
	    	        dot11WEPKeyMappingWEPOn,
                	dot11WEPKeyMappingValue , dot11WEPKeyMappingAddress,
 			dot11WEPKeyMappingStatus }
        STATUS current
        DESCRIPTION
            "The SMTPrivacy package is a set of attributes that shall be
            present if WEP is implemented in the STA."
    ::= { dot11Groups 2 }

dot11MACbase OBJECT-GROUP
        OBJECTS {	dot11MACAddress, dot11Address,
			dot11GroupAddressesStatus,
			dot11RTSThreshold, dot11ShortRetryLimit,
			dot11LongRetryLimit, dot11FragmentationThreshold,
			dot11MaxTransmitMSDULifetime,
			dot11MaxReceiveLifetime, dot11ManufacturerID,
			dot11ProductID }
        STATUS current
        DESCRIPTION
        	"The MAC object class provides the necessary support for the
         	access control, generation, and verification of frame check
         	sequences (FCSs), and proper delivery of valid data to upper
         	layers."
    ::= { dot11Groups 3 }

dot11MACStatistics OBJECT-GROUP
        OBJECTS { 	dot11RetryCount, dot11MultipleRetryCount,
            		dot11RTSSuccessCount, dot11RTSFailureCount,
            		dot11ACKFailureCount, dot11FrameDuplicateCount }
        STATUS current
        DESCRIPTION
            "The MACStatistics package provides extended statistical
            information on the operation of the MAC.  This 
            package is completely optional."
    ::= { dot11Groups 4 }

dot11ResourceTypeID OBJECT-GROUP
        OBJECTS {	dot11ResourceTypeIDName, dot11manufacturerOUI,
            		dot11manufacturerName, dot11manufacturerProductName,
            		dot11manufacturerProductVersion }
        STATUS current
        DESCRIPTION
        	"Attributes used to identify a STA, its manufacturer,
            and various product names and versions."
    ::= { dot11Groups 5 }

dot11SmtAuthenticationAlgorithms OBJECT-GROUP
        OBJECTS {	dot11AuthenticationAlgorithm,
                 	dot11AuthenticationAlgorithmsEnable }
        STATUS current
        DESCRIPTION
        	"Authentication Algorithm Table."
    ::= { dot11Groups 6 }

dot11PhyOperationComplianceGroup OBJECT-GROUP
        OBJECTS { 	dot11PHYType, dot11CurrentRegDomain, dot11TempType }
        STATUS current
        DESCRIPTION
            "PHY layer operations attributes."
    ::= { dot11Groups 7 }

dot11PhyAntennaComplianceGroup OBJECT-GROUP
        OBJECTS {	dot11CurrentTxAntenna, dot11DiversitySupport,
               		dot11CurrentRxAntenna }
        STATUS current
        DESCRIPTION
            "Attributes for Data Rates for IEEE 802.11."
    ::= { dot11Groups 8 }

dot11PhyTxPowerComplianceGroup OBJECT-GROUP
        OBJECTS {	dot11NumberSupportedPowerLevels, dot11TxPowerLevel1,
            		dot11TxPowerLevel2, dot11TxPowerLevel3, dot11TxPowerLevel4,
            		dot11TxPowerLevel5, dot11TxPowerLevel6, dot11TxPowerLevel7,
            		dot11TxPowerLevel8, dot11CurrentTxPowerLevel }
        STATUS current
        DESCRIPTION
            "Attributes for Control and Management of transmit power."
    ::= { dot11Groups 9 }

dot11PhyFHSSComplianceGroup OBJECT-GROUP
        OBJECTS {	dot11HopTime, dot11CurrentChannelNumber, dot11MaxDwellTime,
            		dot11CurrentDwellTime, dot11CurrentSet, dot11CurrentPattern,
            		dot11CurrentIndex}
        STATUS current
        DESCRIPTION
            "Attributes that configure the Frequency Hopping for IEEE
            802.11."
    ::= { dot11Groups 10 }

dot11PhyDSSSComplianceGroup OBJECT-GROUP
        OBJECTS {	dot11CurrentChannel, dot11CCAModeSupported,
            		dot11CurrentCCAMode, dot11EDThreshold}
        STATUS current
        DESCRIPTION
            "Attributes that configure the DSSS for IEEE 802.11."
    ::= { dot11Groups 11 }

dot11PhyIRComplianceGroup OBJECT-GROUP
        OBJECTS {	dot11CCAWatchdogTimerMax, dot11CCAWatchdogCountMax,
       			dot11CCAWatchdogTimerMin, dot11CCAWatchdogCountMin}
        STATUS current
        DESCRIPTION
            "Attributes that configure the baseband IR for IEEE 802.11."
    ::= { dot11Groups 12 }

dot11PhyRegDomainsSupportGroup OBJECT-GROUP
        OBJECTS { dot11RegDomainsSupportedValue}
        STATUS current
        DESCRIPTION
            "Attributes that specify the supported Regulation Domains."
    ::= { dot11Groups 13}

dot11PhyAntennasListGroup OBJECT-GROUP
        OBJECTS { 	dot11SupportedTxAntenna,
             		dot11SupportedRxAntenna, dot11DiversitySelectionRx }
        STATUS current
        DESCRIPTION
            "Attributes that specify the supported Regulation Domains."
    ::= { dot11Groups 14 }

dot11PhyRateGroup OBJECT-GROUP
        OBJECTS {	dot11SupportedDataRatesTxValue,
            		dot11SupportedDataRatesRxValue }
        STATUS current
        DESCRIPTION
            "Attributes for Data Rates for IEEE 802.11."
    ::= { dot11Groups 15 }

dot11CountersGroup OBJECT-GROUP
        OBJECTS { 	dot11TransmittedFragmentCount,
			dot11MulticastTransmittedFrameCount,
			dot11FailedCount, dot11ReceivedFragmentCount,
			dot11MulticastReceivedFrameCount,
			dot11FCSErrorCount,
		    	dot11WEPUndecryptableCount,
	    		dot11TransmittedFrameCount }
        STATUS current
        DESCRIPTION
            "Attributes from the dot11CountersGroup that are not described
            in the dot11MACStatistics group.  These objects are
            mandatory."
    ::= { dot11Groups 16 }

dot11NotificationGroup NOTIFICATION-GROUP
		NOTIFICATIONS {	dot11Disassociate, 
				dot11Deauthenticate,
				dot11AuthenticateFail }
		STATUS current
		DESCRIPTION
			"IEEE 802.11 notifications"
	::= { dot11Groups 17 }

dot11SMTbase2 OBJECT-GROUP
        OBJECTS { 	dot11MediumOccupancyLimit, 
             		dot11CFPollable,
             		dot11CFPPeriod,
             		dot11CFPMaxDuration,
           		dot11AuthenticationResponseTimeOut,
			dot11PrivacyOptionImplemented,
		     	dot11PowerManagementMode,
		     	dot11DesiredSSID, dot11DesiredBSSType,
		 	dot11OperationalRateSet,
			dot11BeaconPeriod, dot11DTIMPeriod,
		 	dot11AssociationResponseTimeOut,
			dot11DisassociateReason,
             		dot11DisassociateStation,
             		dot11DeauthenticateReason,
             		dot11DeauthenticateStation,
             		dot11AuthenticateFailStatus,
             		dot11AuthenticateFailStation }
        STATUS current
        DESCRIPTION
         	"The SMTbase2 object class provides the necessary support at the
         	STA to manage the processes in the STA such that the STA may
         	work cooperatively as a part of an IEEE 802.11 network."
    ::= { dot11Groups 18 }

dot11PhyOFDMComplianceGroup OBJECT-GROUP
        OBJECTS {	dot11CurrentFrequency,
                  	dot11TIThreshold,
                  	dot11FrequencyBandsSupported }
        STATUS current
        DESCRIPTION
            "Attributes that configure the OFDM for IEEE 802.11."
    ::= { dot11Groups 19 }

dot11SMTbase3 OBJECT-GROUP
        OBJECTS { 	dot11MediumOccupancyLimit, 
             		dot11CFPollable,
             		dot11CFPPeriod,
             		dot11CFPMaxDuration,
             		dot11AuthenticationResponseTimeOut,
		     	dot11PrivacyOptionImplemented,
		     	dot11PowerManagementMode,
		     	dot11DesiredSSID, dot11DesiredBSSType,
		 	dot11OperationalRateSet,
			dot11BeaconPeriod, dot11DTIMPeriod,
			dot11AssociationResponseTimeOut,
			dot11DisassociateReason,
             		dot11DisassociateStation,
             		dot11DeauthenticateReason,
             		dot11DeauthenticateStation,
             		dot11AuthenticateFailStatus,
             		dot11AuthenticateFailStation, 
       	     		dot11MultiDomainCapabilityImplemented,
			dot11MultiDomainCapabilityEnabled, 
			dot11CountryString }
        STATUS current
        DESCRIPTION
		"The SMTbase3 object class provides the necessary support at the
		STA to manage the processes in the STA such that the STA may
		work cooperatively as a part of an IEEE 802.11 network, when the STA
		is capable of multi-domain operation. This object group should be
		implemented when the multi-domain capability option is implemented."    
	::= { dot11Groups 20 }

dot11MultiDomainCapabilityGroup OBJECT-GROUP
	OBJECTS {	dot11FirstChannelNumber,
			dot11NumberofChannels,
			dot11MaximumTransmitPowerLevel }
		STATUS current
		DESCRIPTION
			"The dot11MultiDomainCapabilityGroup object class provides 
			the objects necessary to manage the channels usable by a STA, 
			when the multi-domain capability option is implemented."    
		::= { dot11Groups 21 }
    
dot11PhyFHSSComplianceGroup2 OBJECT-GROUP
        OBJECTS {	dot11HopTime, dot11CurrentChannelNumber, dot11MaxDwellTime,
            		dot11CurrentDwellTime, dot11CurrentSet, dot11CurrentPattern,
            		dot11CurrentIndex, dot11EHCCPrimeRadix, 
            		dot11EHCCNumberofChannelsFamilyIndex,
            		dot11EHCCCapabilityImplemented, dot11EHCCCapabilityEnabled, 
            		dot11HopAlgorithmAdopted, dot11RandomTableFlag, 
            		dot11NumberofHoppingSets, dot11HopModulus, 
            		dot11HopOffset, dot11RandomTableFieldNumber }
        STATUS current
        DESCRIPTION
            "Attributes that configure the Frequency Hopping for IEEE
            802.11 when multi-domain capability option is implemented."
    ::= { dot11Groups 22 }

dot11PhyHRDSSSComplianceGroup OBJECT-GROUP
        OBJECTS {	dot11CurrentChannel, dot11CCAModeSupported,
                	dot11CurrentCCAMode, dot11EDThreshold,
                	dot11ShortPreambleOptionImplemented,
                	dot11PBCCOptionImplemented, dot11ChannelAgilityPresent,
                	dot11ChannelAgilityEnabled, dot11HRCCAModeSupported }
        STATUS current
        DESCRIPTION
        	"Attributes that configure the HRDSSS for IEEE 802.11."
    ::= { dot11Groups 23 }

-- **********************************************************************
-- *   End of 802.11 MIB
-- **********************************************************************

END
