;****************************************************************************************
;
;    FILE:
;            ATWCL452.inf
;
;    DESCRIPTION:
;            AT-WCL452 802.11b Wireless PCMCIA Radio inf file.
;            2002, Allied Telesyn, Inc.
;
;*******************************************************************************************

[Version]
DriverVer=09/04/2002, 2.0.2.36
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
;CatalogFile=ATWCL452.CAT

[Manufacturer]
%V_Provider%=Adapters

; All enumerated adapters must be excluded from select
;[ControlFlags]
;ExcludeFromSelect=PCMCIA\Allied_Telesyn-AT-WCL452_Wireless_PCMCIA_Radio-A9AB
;ExcludeFromSelect=PCMCIA\INTERSIL-HFA384x/IEEE-CC3C

; --- For non-Windows XP
[Adapters]
; DisplayName                Section                DeviceID
; -----------                -------                --------
%WCL452.DeviceDesc% = WCL452.ndi,   PCMCIA\Allied_Telesyn-AT-WCL452_Wireless_PCMCIA_Radio-A9AB
%WR2411.DeviceDesc%  = WCL452_1.ndi,   PCMCIA\INTERSIL-HFA384x/IEEE-CC3C
;----------------------------------------------------------------------------
; Windows 9X specific entries
;
[WCL452.ndi]
AddReg=WCL452.ndi.reg, Pcmcia9x.reg, Advanced.reg, Common.reg, Run.reg
CopyFiles=win9x.CopyFiles, @CheckDLL.DLL
DriverVer=09/04/2002, 2.0.2.36

[WCL452_1.ndi]
AddReg=WCL452.ndi.reg, Pcmcia9x_1.reg, Advanced.reg, Common.reg, Run.reg
CopyFiles=win9x.CopyFiles, @CheckDLL.DLL
DriverVer=09/04/2002, 2.0.2.36


[WCL452.ndi.reg]
HKR, ,                            NTMPDriver,      0, ATWCL452.sys

;
;HKR, ,                            RunningWin9X,    0, "1"
HKR, ,                            DevLoader,       0, *ndis
HKR, ,                            DeviceVxDs,      0, ATWCL452.sys
HKR, ,                            EnumPropPages,   0, "netdi.dll,EnumPropPages"
;
; NDIS Info
HKR, NDIS,                        LogDriverName,   0, "WCL452"
HKR, NDIS,                        MajorNdisVersion,1, 03
HKR, NDIS,                        MinorNdisVersion,1, 0A

HKR, ,                            BusType,         0, 8
HKR, NDI,                         CardType,        0, "PCMCIA"
;
; Interfaces
;
HKR, Ndi\Interfaces,              DefUpper,        0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,        0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,      0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,      0, "ethernet"
;
; Install sections
;HKR,Ndi\Install,ndis3,,"WCL452.install"

;[WCL452.install]
;CopyFiles=win9x.CopyFiles

;----------------------------------------------------------------------------
; PCMCIA specific
;
[Pcmcia9x.reg]
;
; All resources are dynamically configured
;
HKR, ,                            IOBaseAddress,   1, 02,00,00,00
HKR, ,                            InterruptNumber, 1, 04,00,00,00
HKR, ,                            EnableIRQSharing,1, 01,00,00,00
;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, "AT-WCL452 802.11b Wireless PCMCIA Radio"
HKR, Ndi,                         DeviceID,        0, "PCMCIA\Allied_Telesyn-AT-WCL452_Wireless_PCMCIA_Radio-A9AB"

[Pcmcia9x_1.reg]
;
; All resources are dynamically configured
;
HKR, ,                            IOBaseAddress,   1, 02,00,00,00
HKR, ,                            InterruptNumber, 1, 04,00,00,00
HKR, ,                            EnableIRQSharing,1, 01,00,00,00
;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, "AT-WR2411 802.11b Wireless Ethernet Adapter"
HKR, Ndi,                       DeviceID,          0, "PCMCIA\INTERSIL-HFA384x/IEEE-CC3C"


;----------------------------------------------------------------------------
; Window 2000, XP specific entries
;
;-----------------------------------------------------------------------
[WCL452.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg, Runonce.reg
Characteristics=0x84              ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
CopyFiles=NT.CopyFiles, NT.Setup.CopyFiles
DriverVer=09/04/2002, 2.0.2.36

[WCL452_1.ndi.NT]
AddReg=Advanced.reg, Common.reg, nt.reg, Runonce.reg
Characteristics=0x84              ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=8
CopyFiles=NT.CopyFiles, NT.Setup.CopyFiles
DriverVer=09/04/2002, 2.0.2.36

; NT services sections
[WCL452.ndi.NT.Services]
AddService=WCL452, 2, WCL452.Service, common.EventLog

[WCL452_1.ndi.NT.Services]
AddService=WCL452, 2, WCL452_1.Service, common.EventLog


[WCL452.Service]
DisplayName=%WCL452.Service.DispName%
ServiceType=1                ;%SERVICE_KERNEL_DRIVER%
StartType=3                ;%SERVICE_AUTO_START%
ErrorControl=1                ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\ATWCL452.sys
LoadOrderGroup=NDIS

[WCL452_1.Service]
DisplayName=%WR2411.Service.DispName%
ServiceType=1                ;%SERVICE_KERNEL_DRIVER%
StartType=3                ;%SERVICE_AUTO_START%
ErrorControl=1                ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\ATWCL452.sys
LoadOrderGroup=NDIS

;-----------------------------------------------------------------------

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\ATWCL452.sys"
HKR, , TypesSupported,   0x00010001, 7


[Runonce.reg]
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\RunOnce","WLPC",0x00000000,"rundll32 checkdll.dll,RunSetup"

[Run.reg]
HKLM,"SOFTWARE\Microsoft\Windows\CurrentVersion\Run","WLPC",0x00000000,"rundll32 checkdll.dll,RunSetup"


;----------------------------------------------------------------------------
; NT specific
;

[nt.reg]
HKR, Ndi,                         Service,         0, "WCL452"
HKR, Ndi\Interfaces,              UpperRange,      0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,      0, "ethernet"


;----------------------------------------------------------------------------
; common regs for NT and W9x
;
[Common.reg]
;
; auto download firmware
;
HKR, ,                            LoadFirmware,    0, 1

;
; AP Density
;
HKR, ,                            APDensity,       0, 1
HKR, defaults,                    APDensity,       0, 1
;
; SSID
;
HKR, ,                            SSID,            0, %SSID_DEF_STR%
HKR, defaults,                    SSID,            0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
HKR, NDI\params\SSID,             type,            0, edit
HKR, NDI\params\SSID,             limitText,       0, 32
HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%
HKR, NDI\params\SSID,             flag,            1, 30,00,00,00
;
; StationName
;
HKR, ,                            StationName,     0, "Client"
HKR, defaults,                    StationName,     0, "Client"
;
; Channel
;
HKR, ,                            DSChannel,       0, %CHANNEL%
HKR, defaults,                    DSChannel,       0, %CHANNEL%
HKR, NDI\params\DSChannel,        ParamDesc,       0, "Channel"
HKR, NDI\params\DSChannel,        type,            0, enum
HKR, NDI\params\DSChannel,        default,         0, %CHANNEL%
HKR, NDI\params\DSChannel,        flag,            1, 30,00,00,00
HKR, NDI\params\DSChannel\enum,   1,               0, "1"
HKR, NDI\params\DSChannel\enum,   2,               0, "2"
HKR, NDI\params\DSChannel\enum,   3,               0, "3"
HKR, NDI\params\DSChannel\enum,   4,               0, "4"
HKR, NDI\params\DSChannel\enum,   5,               0, "5"
HKR, NDI\params\DSChannel\enum,   6,               0, "6"
HKR, NDI\params\DSChannel\enum,   7,               0, "7"
HKR, NDI\params\DSChannel\enum,   8,               0, "8"
HKR, NDI\params\DSChannel\enum,   9,               0, "9"
HKR, NDI\params\DSChannel\enum,   10,              0, "10"
HKR, NDI\params\DSChannel\enum,   11,              0, "11"

;
; Encapsultion (i.e. Ethernet Translation)
;
HKR, ,                            Encapsulation,   0, 1
HKR, defaults,                    Encapsulation,   0, 1

;
; TxRate
;
HKR, ,                            TxRate,          0, 15
HKR, defaults,                    TxRate,          0, 15
HKR, NDI\params\TxRate,           ParamDesc,       0, "Transmit Rate"
HKR, NDI\params\TxRate,           type,            0, enum
HKR, NDI\params\TxRate,           default,         0, 15
HKR, NDI\params\TxRate,           flag,            1, 30,00,00,00
HKR, NDI\params\TxRate\enum,      1,               0, "Fixed 1 Mb/s"
HKR, NDI\params\TxRate\enum,      2,               0, "Fixed 2 Mb/s"
HKR, NDI\params\TxRate\enum,      3,               0, "Auto Select 1 or 2"
HKR, NDI\params\TxRate\enum,      4,               0, "Fixed 5.5 Mb/s"
HKR, NDI\params\TxRate\enum,      8,               0, "Fixed 11 Mb/s"
HKR, NDI\params\TxRate\enum,      15,              0, "Fully Auto"

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, defaults,                    NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, "Network Type"
HKR, NDI\params\NetworkType,      type,            0, enum
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      flag,            1, 30,00,00,00
HKR, NDI\params\NetworkType\enum, 0,               0, "Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1,               0, "Infrastructure"

;
;    Wep Required
;
HKR, ,                            WepReq,          0, %WEP_REQUIRED_DEF_STR%
HKR, defaults,                    WepReq,          0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq,           ParamDesc,       0, "Encryption"
HKR, NDI\params\WepReq,           flag,            1, 30,00,00,00
HKR, NDI\params\WepReq,           type,            0, enum
HKR, Ndi\params\WepReq,           default,         0, %WEP_REQUIRED_DEF_STR%
HKR, NDI\params\WepReq\enum,      0,               0, "Disabled"
HKR, NDI\params\WepReq\enum,      2,               0, "64 bit"
HKR, NDI\params\WepReq\enum,      6,               0, "128 bit"
HKR, NDI\params\WepReq,           optional,        0, 0

;
;    Wep Encrypt in Driver
;
HKR, ,                            EncryptInDriver, 0, 1
HKR, defaults,                    EncryptInDriver, 0, 1

;
;    Wep Decrypt in Driver
;
HKR, ,                            DecryptInDriver, 0, 1
HKR, defaults,                    DecryptInDriver, 0, 1

;
;    WEP Factor
;
HKR, ,                            WEPFactor,       0, 3
HKR, defaults,                    WEPFactor,       0, 3

;
;    Esarhpssap
;
HKR, ,                            Esarhpssap,      0, %PASSPHRASE_DEF_STR%
HKR, defaults,                    Esarhpssap,      0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap,       ParamDesc,       0, "WEP Passphrase"
HKR, NDI\params\Esarhpssap,       type,            0, edit
HKR, NDI\params\Esarhpssap,       limitText,       0, 64
HKR, NDI\params\Esarhpssap,       default,         0, %PASSPHRASE_DEF_STR%
HKR, NDI\params\Esarhpssap,       flag,            1, 30,00,00,00

;
;    IBSS in Driver mode control
;
HKR, ,                            IBSSInDriver,    0, 0
HKR, defaults,                    IBSSInDriver,    0, 0

HKR,, WEP64_KEY_1,            0,"0000000000"
HKR,, WEP64_KEY_2,            0,"0000000000"
HKR,, WEP64_KEY_3,            0,"0000000000"
HKR,, WEP64_KEY_4,            0,"0000000000"

HKR,, WEP128_KEY_1,           0,"00000000000000000000000000"
HKR,, WEP128_KEY_2,           0,"00000000000000000000000000"
HKR,, WEP128_KEY_3,           0,"00000000000000000000000000"
HKR,, WEP128_KEY_4,           0,"00000000000000000000000000"

HKR,, CurProfile,             0,"default"

[Advanced.reg]
;
; Listen Interval
;
HKR, ,                            ListenInterval,  0, 3
HKR, defaults,                    ListenInterval,  0, 3
HKR, NDI\params\ListenInterval,   ParamDesc,       0, "Maximum Listen Interval"
HKR, NDI\params\ListenInterval,   flag,            1, 30,00,00,00
HKR, NDI\params\ListenInterval,   type,            0, int
HKR, Ndi\params\ListenInterval,   default,         0, 3
HKR, NDI\params\ListenInterval,   min,             0, 0
HKR, NDI\params\ListenInterval,   max,             0, 77
HKR, NDI\params\ListenInterval,   step,            0, 1
HKR, NDI\params\ListenInterval,   optional,        0, 0

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, 2432
HKR, defaults,                    RTSThresh,       0, 2432
HKR, NDI\params\RTSThresh,        ParamDesc,       0, "RTS Threshold"
HKR, NDI\params\RTSThresh,        type,            0, int
HKR, Ndi\params\RTSThresh,        default,         0, 2432
HKR, NDI\params\RTSThresh,        min,             0, 0
HKR, NDI\params\RTSThresh,        max,             0, 2432
HKR, NDI\params\RTSThresh,        step,            0, 64
HKR, NDI\params\RTSThresh,        flag,            1, 20,00,00,00
HKR, NDI\params\RTSThresh,        optional,        0, 0
;
; Frag Threshold
;
HKR, ,                            FragThresh,      0, 2432
HKR, defaults,                    FragThresh,      0, 2432
HKR, NDI\params\FragThresh,       ParamDesc,       0, "Fragmentation Threshold"
HKR, NDI\params\FragThresh,       type,            0, int
HKR, Ndi\params\FragThresh,       default,         0, 2432
HKR, NDI\params\FragThresh,       min,             0, 256
HKR, NDI\params\FragThresh,       max,             0, 2432
HKR, NDI\params\FragThresh,       step,            0, 128
HKR, NDI\params\FragThresh,       flag,            1, 20,00,00,00
HKR, NDI\params\FragThresh,       optional,        0, 0

;
;    Short Preamble
;
HKR, ,                            PreambleMode,    0, 1
HKR, defaults,                    PreambleMode,    0, 1
HKR, NDI\params\PreambleMode,     ParamDesc,       0, %SHORT_PREAM_STR%
HKR, NDI\params\PreambleMode,     flag,            1, 30,00,00,00
HKR, NDI\params\PreambleMode,     type,            0, enum
HKR, Ndi\params\PreambleMode,     default,         0, 1
HKR, NDI\params\PreambleMode\enum,1,               0, "Long Tx Preamble"
HKR, NDI\params\PreambleMode\enum,2,               0, "Short Tx Preamble"
;HKR, NDI\params\PreambleMode\enum,3,               0, "Auto"
HKR, NDI\params\PreambleMode,     optional,        0, 0

;
;
; Authentication Type
;
HKR, ,                            AuthentAlg,      0, %AUTHENT_TYPE_DEF_STR%
HKR, defaults,                    AuthentAlg,      0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg,       ParamDesc,       0, "Authentication Algorithm"
HKR, NDI\params\AuthentAlg,       type,            0, enum
HKR, NDI\params\AuthentAlg,       default,         0, %AUTHENT_TYPE_DEF_STR%
HKR, NDI\params\AuthentAlg,       flag,            1, 30,00,00,00
HKR, NDI\params\AuthentAlg\enum,  1,               0, "WECA Compliant (always use Open)"
HKR, NDI\params\AuthentAlg\enum,  2,               0, "Must use Shared with WEP"
HKR, NDI\params\AuthentAlg\enum,  65535,           0, "Automatic based on WEP setting"

;
; PS Mode
;
HKR, ,                            PSMode,          0, 1
HKR, defaults,                    PSMode,          0, 1
HKR, NDI\params\PSMode,           ParamDesc,       0, "Power Save Mode"
HKR, NDI\params\PSMode,           type,            0, enum
HKR, NDI\params\PSMode,           default,         0, 1
HKR, NDI\params\PSMode,           flag,            1, 30,00,00,00
HKR, NDI\params\PSMode\enum,      1,               0, "Disabled"
HKR, NDI\params\PSMode\enum,      2,               0, "Enabled"


;----------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir    = 11
NT.CopyFiles      = 12    ; system32\drivers subdirectory on NT
win9x.CopyFiles   = 11    ; system32 subdirectory on win9x
NT.Setup.CopyFiles= 11

[win9x.CopyFiles]
ATWCL452.sys ; Win9x Installation

[NT.CopyFiles]
ATWCL452.sys,ATWCL452X.sys,,2


[NT.Setup.CopyFiles]
CheckDLL.dll

[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,

[SourceDisksFiles]
ATWCL452.sys = 1
ATWCL452X.sys = 1
CheckDLL.DLL = 1

;----------------------------------------------------------------------------
; Strings
;
[strings]
Provider="ATI"
V_Provider="Allied Telesyn, Inc."

WCL452.DeviceDesc="AT-WCL452 802.11b Wireless PCMCIA Radio"
WR2411.DeviceDesc="AT-WR2411 802.11b Wireless Ethernet Adapter"

WCL452.Service.DispName = "AT-WCL452 802.11b Wireless PCMCIA Radio Driver"
WR2411.Service.DispName="AT-WR2411 802.11b Wireless Ethernet Adapter"

INSTALL_DISK_STR="Allied Telesyn 802.11b Wireless PCMCIA Radio Installation Disk"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR="any"
NETWORK_TYPE_DEF_STR=1
CHANNEL=6
AUTHENT_TYPE_DEF_STR="65535"
PASSPHRASE_DEF_STR=""
WEP_REQUIRED_DEF_STR="0"
SHORT_PREAM_STR="Preamble Mode"

