PowerStorm 3D30 or 4D20 v3.0 Readme.1st
========================

This is the PowerStorm 3D30 or 4D20 v3.0 driver kit.  It contains drivers for 
Windows NT 3.51 or later running on Alpha platforms.

Due to licensing issues, this kit can not be used for the initial
installation of the PowerStorm 3D30 or 4D20 Accelerated OpenGL driver on your 
Alpha system.  It can only be used to upgrade the PowerStorm 3D30 or 4D20 
Accelerated OpenGL driver.  You can check whether you have installed the 
PowerStorm 3D30 or 4D20 Accelerated OpenGL driver by searching for the file:

              %WINDIR%\system32\tgaglclt.dll

If this file is not present on your system, you should first 
reinstall the PowerStorm 3D30 or 4D20 drivers from the floppy which was 
shipped to you with your PowerStorm 3D30 or 4D20 board.

This kit *can* be used to install or upgrade the 2D display
driver.

The drivers in this kit provide numerous performance and bug fixes.  See
the release notes in the file relnotes.wri for details.

To install the new PowerStorm 3D30 or 4D20 drivers, please follow these steps
(Which are also outlined in the Graphics Support Services for
Microsoft Windows NT v3.0 Installation Guide):

1) Unzip the kit into an empty directory.

2) Copy the files in the "disk1" directory to a blank floppy and label
   it "PowerStorm 3D30 or 4D20 V3.0 Driver Disk 1".  Copy the files in the 
   "disk2" directory to a second blank floppy and label it "PowerStorm 3D30 
   or 4D20 V3.0 Driver Disk 2".

3) Insert the PowerStorm 3D30 or 4D20 V3.0 Driver Disk 1 into the floppy drive.

4) Start the Control Panel Display applet.

5) Click on the "Change Display Type..." button.

6) In the Display Type dialog box, click on the "Change..." 
   button.

7) In the Select Device dialog box, click on the "Other..." 
   button.

8) In the Install From Disk dialog box, enter the path for your 
   floppy drive which will be used to find the PowerStorm 3D30 or 4D20 kit.  
   For example, "A:\".  Now click on "OK".

9) In the Select Device dialog box, the entry 
     "Digital ZLXp-E/PowerStorm 3D30 or 4D20"
   should have been added at the bottom of the list box and 
   selected.  Click on the "Install" button.

10) In the Installing Driver dialog box, click on "Yes" to allow 
    the system to install the drivers.

11) If you do not have the PowerStorm 3D30 or 4D20 Accelerated OpenGL drivers
    installed, you will see a dialog box informing you that the 
    installation procedure will not upgrade the OpenGL driver. 
    Click on "OK" to only upgrade the 2D driver or "Cancel" to 
    abort the installation.

12) In the Windows Net Setup dialog box, click on "New" to 
    install the drivers from the floppy.

13) In the Install From Disk dialog box, enter the path for your 
    floppy drive which will be used to find PowerStorm 3D30 or 4D20 kit.  
    For example, "A:\".  Now click on "Continue".

14) Windows NT will display a status box with a gauge to show you 
    the progress of the installation.  Insert the second driver floppy
    when the system prompts for it.  A dialog box announcing the
    completion of the installation process will  be displayed.  Click on
    "OK".

15) You will be informed that you must restart Windows NT to use 
    the new drivers.  Click on "OK".

16) The Display Settings Change dialog box will be displayed to 
    allow you to restart Windows NT.  Click on "Restart Now".

17) Your system will reboot and use the new PowerStorm 3D30 or 4D20 drivers.  
    You may want to reset the screen resolution and refresh
    rate using the Control Panel Display applet.

18) The installation is now complete.
