 


                              DIGITAL

Software
Product
Description

___________________________________________________________________

PRODUCT NAME:  DECset Clients for CMS and MMS Version 1.3       SPD
64.06.03

DESCRIPTION

DECset Clients for CMS and MMS provides access from the desktop per-
sonal computer (PC) to the DIGITAL Code Management System (CMS) li-
braries and DIGITAL Module Management System (MMS) features residing
on OpenVMS Alpha and OpenVMS VAX systems. CMS, a component of the DEC-
set software development tools, is an online library system that helps
track software development and maintenance. MMS, a component of the
DECset software development tools, is a software system builder that
simplifies the building of applications. MMS optimizes the build pro-
cess by tracking the complex dependencies and relationships that ex-
ist between software components. (For more information on CMS or MMS
for OpenVMS VAX systems refer to SPD 27.07. For more information on
CMS or MMS for OpenVMS Alpha systems refer to SPD 42.29.)

DECset Clients for CMS and MMS can be used from a personal computer
running Microsoft Windows 95, or Windows NT[TM]. Connection to a CMS
library or MMS feature from the PC is possible once the Server soft-
ware (provided with the Client) and the CMS and MMS for OpenVMS soft-
ware are installed at the server site.

The main DECset Clients windows offer menu access to most of the CMS
and MMS functions. DECset Clients commands can also be performed by
clicking the command buttons on the toolbar. In addition, DECset Clients
supports drag-and-drop functionality for manipulating data within the
DECset Clients window.

                                                      November 1997

                                                        AE-QKZDD-TH
 

Features

With DECset Clients for CMS and MMS, users can access many of the com-
mon features:

CMS Client

o  Access a CMS library on an OpenVMS server system.

o  Change the working (local) directory.

o  Create a element, class, or group.

o  Delete a specified class from a CMS library.

o  Delete an element from a CMS library.

o  Delete one or more element generations.

o  Delete a specified group from a CMS library.

o  Fetch or reserve a copy of an element generation from a CMS library
   and place it in the current local PC directory.

o  Insert or remove an element or group into or from a specified group.

o  Insert or remove a specified element generation into or from a class.

o  Replace the latest version of a modified file into a CMS library.

o  Store PC files in CMS on the OpenVMS system.

o  Create a new password for the local DECset Clients session.

o  Cancel an existing reservation of an element generation (Unreserve).

o  Display the names of all established groups in a CMS library.

o  Display a chronological list of transactions performed on a CMS li-
   brary.

o  Display information about current reservations and concurrent re-
   placements in effect currently.

MMS Client

o  Use MMS to build OpenVMS applications.

                                 2
 

o  Change the working (local and remote) directory.

o  Fetch and open MMS description files.

o  Activate MMS description file generation.

o  Activate MMS builds on the remote system.

HARDWARE REQUIREMENTS

o  PC using an 80486 or higher microprocessor, IBM or compatible OR

o  System using an Alpha/NT or Intel/NT processor

o  CD-ROM drive

o  Minimum of 8 MB of RAM (for Windows 95) or
   16 MB of RAM (for Windows NT)

Disk Space Requirements (Block Cluster Size = 1):

CLIENT:

Minimum disk space required for DECset Clients for CMS and MMS instal-
lation is 5 MB.

SERVER:

CMS Server VAX:

Disk space required for      1000 blocks
installation:
                             (.5 MB)

Disk space required for      200 blocks
permanent use:
                             (.25 MB)



                                 3
 

CMS Server Alpha:

Disk space required for      2000 blocks
installation:
                             (1 MB)

Disk space required for      1000 blocks
permanent use:
                             (.5 MB)

MMS Server VAX and Alpha:

Disk space required for      2000 blocks
installation:
                             (1 MB)

Disk space required for      200 blocks
permanent use:
                             (.25 MB)

These counts refer to the disk space required on the system disk. The
sizes are approximate. Actual sizes may vary depending on the user's
system environment, configuration, and software options.

SOFTWARE REQUIREMENTS

CMS and MMS Clients:

o  CMS Server Version 1.2a

o  MMS Server Version 1.0

o  Microsoft Windows 95, or Microsoft Windows NT
   Version 4.0

o  For DECnet:

   -  DIGITAL PATHWORKS 32 Version 7.0

o  For TCP/IP: (support via Window Sockets V1.1:)

   -  Microsoft TCP/IP-32

                                 4
 

CMS Server and MMS Server: (Provided with the Client)

o  CMS Client 1.2a

o  MMS Client 1.0

o  CMS Version 3.8 or 3.9 or DECset Version 12.1 or 12.2 for OpenVMS
   systems

o  MMS Version 3.1 or 3.2 or DECset Version 12.1 or 12.2 for OpenVMS
   systems

o  For DECnet:

   -  PATHWORKS for OpenVMS VAX Version 5.0 or higher OR

   -  PATHWORKS for OpenVMS Alpha Version 5.0 or higher

o  For TCP/IP:

   -  DIGITAL TCP/IP services for OpenVMS (UCX) Version 3.3 or Ver-
      sion 4.1 OR

   -  PathWay[TM] for OpenVMS Version 2.5.1
      (Attachmate Corporation) OR

   -  Cisco MultiNet® for OpenVMS Version 4.0
      (Cisco Systems®, Inc.) OR

   -  TCPware® for OpenVMS Version 5.1
      (Process Software Corporation)

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of
this product may be different from the requirements for the current
version.



                                 5
 

DISTRIBUTION MEDIA

CD-ROM
(dual formatted for windows and OpenVMS)

Note: Alternative media is available on request for the DECset Client
for CMS and MMS Servers. The order form is included in the media kit.

 o  TK50 magnetic tape

 o  1600 BPI magnetic tape

ORDERING INFORMATION

Software license, media, and documentation are combined in a single
package (QB-3WUAA-S*). Licenses and documentation may be ordered sep-
arately.

DECset Clients for CMS and MMS

Software Packages:
   DECset Clients 1 License Pkg: QB-3WUAA-SA
   DECset Clients 10 License Pkg: QB-3WUAA-SB
Software Licenses:
   DECset Clients 1 License: QM-3WUAA-AA
   DECset Clients 10 License: QM-3WUAA-AB
Software Documentation:
   CMS Client Guide: AA-QHXUA-TH
   MMS Client Guide: AA-R84AA-TE
Software Product Services: QT-3WUA*-**
Software Upgrades:
   DECset Clients 1 License Pkg: QB-3WUAA-MA
   DECset Clients 10 License Pkg: QB-3WUAA-MB
   DECset Clients 1 License: QM-3WUAA-CA
   DECset Clients 10 License: QM-3WUAA-CB





                                 6
 

SOFTWARE LICENSING

This software is furnished under the licensing provisions of Digital
Equipment Corporation's Standard Terms and Conditions. For more in-
formation about DIGITAL licensing terms and policies, contact your lo-
cal DIGITAL office.

SOFTWARE PRODUCT SERVICES

A variety of service options are available from DIGITAL. For more in-
formation, contact your local DIGITAL office.

SOFTWARE WARRANTY

Warranty for this software product is provided by DIGITAL with the pur-
chase of a license for the product. This means that DIGITAL will rem-
edy any nonconformance when it is reported to DIGITAL by the customer
during the warranty period.

The warranty period is one year. It begins when the software is in-
stalled or thirty days after delivery to the end user, whichever oc-
curs first and expires one year later. All warranty-related support
for this software will end one year after release of the subsequent
versions.

Warranty is provided in the country of purchase. DIGITAL will provide
a service location that will accept reporting (in format prescribed
by DIGITAL) of a nonconformance problem caused when using the licensed
software under normal conditions as defined by this SPD. DIGITAL will
remedy a nonconformance problem in the current unaltered release of
the licensed software by issuing correction information such as: cor-
rection documentation, corrected code; or a notice of availability of
corrected code; or a restriction or a bypass. The customer will be re-
sponsible for the preparation and submission of the problem report to
the service location.





                                 7
 

WARRANTY EXCLUSION

DIGITAL does not warrant that the software licensed to customer shall
be error free, that the software shall operate with any hardware and
software other than as specified in this SPD, that the software shall
satisfy customer's own specific requirements, or that copies of the
software other than those provided or authorized by
DIGITAL shall conform to the SPD.

DIGITAL makes no warranties with respect to the fitness and operabil-
ity of modifications not made by DIGITAL.

If the software fails to function for reasons stated previously, the
customer's warranty will be invalidated and all service calls will be
billable at the prevailing per call rates.

This Software Warranty is effective for licensed software products or-
dered in the United States after
October 1988 and supersedes all prior versions.

The previous information is valid at time of release. Please contact
your local DIGITAL office for the most up-to-date information.

®    Microsoft and Windows are registered trademarks of Microsoft
     Corporation.
®    Intel is a registered trademark of Intel Corporation.
®    Cisco Systems and MultiNet are registered trademarks of Cisco
     Systems, Inc.
®    TCPware is a registered trademark of Process Software Corpo-
     ration.
[TM] PathWay is a trademark of Attachmate Corporation.
[TM] Windows NT is a trademark of Microsoft Corporation.
[TM] DECnet, DECset, DIGITAL, OpenVMS,
     PATHWORKS, VAX, VMS, and the DIGITAL logo are trademarks
     of Digital Equipment Corporation.

© 1997 Digital Equipment Corporation.
All rights reserved.


                                 8
