# Instructions for installing RedHat 5.0 for use with bochs.

    First, you need to have the RedHat 5.0 installation CD
    and the boot & supplementary floppy disks.  Installing
    Linux from other vendors is also possible, but I assume
    you have RedHat 5.0 for the script file, and for these
    instructions.

    Second, you need a real Linux system to create the
    disk image file, for use with bochs.  This can be
    later transfered to another platform.

    Third, you should have already configured/compiled
    bochs on your target platform.

    ##########################################
    # This section done on your Linux system #
    ##########################################

    Copy both boot & supplementary floppy disks to image files.

      # stick in Boot disk
      linux-> cp /dev/fd0 1.44_redhat_boot
      # stick in Supplementary disk
      linux-> cp /dev/fd0 1.44_redhat_sup

    Mount your RedHat 5.0 CD.  The mountpoint and instructions
    may be different for your system.

      linux-root> mount /mnt/cdrom

    Now edit the install script in bochs-YYMMDD/misc, called
    'install_redhat50'.  It has a small section of configurable
    parameters you can edit.  Then run it as root.  Make sure
    you are in the directory.

      linux-root> cd bochs-YYMMDD/misc
      linux-root> ./install_redhat50

    If this went well, then you're hard disk image file
    is prepared for you, and has a small set of packages
    from the RedHat 5.0 CD on it.  You may add more later,
    using the script file as an example.

    #############################################
    # This section done on your target platform #
    #############################################

    If you have a target system, different from you
    original Linux system, transfer over the 2 floppy
    image files, and the hard disk image file now.

    Copy the boot floppy image to your working file

      unix-> cp 1.44_redhat_boot 1.44

    Point your floppya directive to this working file

      [edit .bochsrc]

    Boot bochs from the floppy

      unix-> bochs boot:a

    The Welcom To Red Hat Linux screen appears.  At the
    boot: prompt, enter 'rescue' and [Return]

      boot:  rescue [Return]

    The Color Choices menu appears
    press [Return] to take the default

    The Keyboard Type menu appears
    press [Return] to take the default

    The Second Floppy menu appears
    Copy the Supplementary floppy image to your working file

      unix-> cp 1.44_redhat_sup 1.44

    Type [Return] to let the install program know you inserted
    the new floppy.

    The SCSI Configuration menu appears
    Type [Return] to accept No.

    You will now be at the Linux root prompt '#'.
    Make an empty directory to mount the hard drive over.
    Then mount the hard drive.  I didn't use any partitions
    for this example, so use 'hda', not 'hda1'.

      # mkdir /mnt
      # mount -t ext2 /dev/hda /mnt

    Run lilo, so you can boot from the hard disk.  Then
    unmount the hard drive.

      # /mnt/sbin/lilo -r /mnt
      # umount /mnt

    Bomb out of bochs, by clicking on the Power button.  Now
    fire up bochs again, booting from the hard drive.

      unix-> bochs boot:c

    You can type [Return] at the LILO prompt:

      LILO boot: [Return]

    At the login prompt, login as root.  For kicks, try
    compiling the sample "hello.cc" program I included.
    It should already be in your /root directory, ready
    to be compiled.

      [root@bochs /root]# gcc -c hello.cc
      [root@bochs /root]# ./a.out

    When you're ready to shutdown Linux, you can
    shutdown as normal:

      [root@bochs /root]# shutdown -h now

    Enjoy,
    -Kevin