***********************************************************************  
  
			IMPORTANT INFORMATION  
				for  
	    Windows 95 mach64 enhanced display driver  
***********************************************************************  
Windows 95 mach64 enhanced display driver             December 31, 1996 
***********************************************************************  
  
READ THIS FILE COMPLETELY BEFORE ATTEMPTING TO USE THIS PRODUCT !  
  
****************************  
  
Contents  
  
1.0     Introduction  
2.0     Adapter Installation  
3.0     Installation Notes for Windows 95 mach64 enhanced display driver  
4.0     Windows 95 mach64 enhanced display driver problems  
5.0     Windows 95 property page problems  
  
  
****************************  
  
1.0     Introduction  
  
This file contains last-minute updates that are not found in the User's  
Guide or in any addendum accompanying the display adapter.  Please read  
this file before proceeding with the installation.  
  
****************************  
  
2.0     Adapter Installation  
  
Refer to the User's Guide for information on adapter installation.  
  
  
****************************  
  
3.0     Installation Notes for Windows 95 mach64 enhanced display driver  
  
The Windows 95 mach64 enhanced display driver is a Windows 95 mini driver.   
									   
NOTE: Windows 95 will require a re-start to implement certain display  
      settings  
 
Start Windows 95.  
 
For CD installation insert the ATI CD-ROM into your CD-ROM drive. 
 
Note:  CD ROM drives that are configured for Auto Insert Notification 
       will automatically load the ATI Installation application.  Proceed 
       to Step 4 to complete the installation. 
 
1) Click Start. 
 
2) Select Run. 
 
3) Type the following: 
       D:\ATISETUP  (D being the letter of your CD-ROM drive.) 
 
4) Click on Easy Install. 
 
5) Select 'Custom Setup' and click Next. 
 
6) Ensure that the 'Enhanced display driver' option is checked. 
 
! If you do not wish to install the ATI Video Player at this time, you
  must un-check the ATI VIDEO PLAYER checkbox. 
 
7) Click the Finish button. 
 
8) Follow the on screen instructions to complete the install. 
 
For Diskette installation insert the disk labeled Windows 95  
into a floppy drive. 
 
1) Click Start. 
 
2) Select Run. 
 
3) Type the following: 
       A:\SETUP  (A: being the letter of your floppy drive.) 
 
4) Select 'Custom Setup' and click Next. 
 
5) Ensure that the 'Enhanced display driver' option is checked. 
 
6) Click the Finish button. 
 
7) Follow the on screen instructions to complete the install. 
  
****************************  
  
4.0     Windows 95 mach64 enhanced display driver problems  
   
- The Windows 95 mach64 enhanced display driver is capable of using monitor  
   timing data contained within Windows 95. This data is selected by   
   configuring a monitor type at Windows 95 installation time or via the   
   "Settings" page of the display properties sheet. If you change the   
   selected monitor type via the "Settings" page of the display properties   
   sheet the new timing data may not take effect until after restarting   
   Windows 95. A solution to this problem is to always restart Windows 95   
   after changing the monitor type.  
  
 - The Windows 95 mach64 enhanced display driver is capable of using monitor  
   timing data contained within Windows 95. This data is selected by   
   configuring a monitor type at Windows 95 installation time or via the   
   "Settings" page of the display properties sheet. The Windows 95 mach64   
   enhanced display driver may incorrectly interpret Windows 95 monitor   
   timing data for some older monitors which require interlaced modes.   
   This may cause some options to be disabled. A solution to this problem   
   is to select one of the "(Standard monitor types)" available via the   
   settings page of the display properties sheet.  
  
 - In Windows 95, display drivers can be installed via the "Add New  
   Hardware" wizard ( although the procedure detailed in section 3.0 is  
   recommended ). When the Windows 95 mach64 enhanced display driver is  
   installed via the "Add New Hardware" wizard the "Settings" page does  
   not get installed into the mach64 display adapter property sheet. 
 
 - In Windows 95, Rapid Resuming with the Virtual Desktop on will cause 
   loss of the Virtual Desktop.  This is because Windows 95 reinitializes 
   the video mode on an APM resume.  No data loss occurs.  The desktop size 
   is reduced to the screen size.  Windows 95 also reinitializes the video 
   mode when windows is restarted on systems with Rapid Resume.  Again, no  
   data loss occurs and the desktop size is reduced to the screen size. 
    
 
****************************  
  
5.0     Windows 95 property page problems  
   
- While adjusting monitor settings in the Adjustment page of the Display 
  Properties sheet, your monitor could become unreadable. If this occurs, 
  press the ESC key to return to your previous monitor settings. 
 
