
  *************************************************************************
  * IRMate-210 can work with the Microsoft Windows 95 default IrDA driver *
  *************************************************************************

To install the Windows 95 driver you must obtain another driver developed
by Microsoft before getting started.

1). The following shows where you can get this IrDA driver for Windows 95 on
    the internet:

- http://www.microsoft.com/windows
  ( Windows Software Library -> Windows 95 Software Library -> IrDA )

- http://www.microsoft.com/windows/software/irda.htm

2). You can then proceed to download the driver. After you de-compress it,
copy the driver files to a diskette.

3). Reference RELNOTES.DOC on this diskette for more information about this
driver, if needed.

4). Copy the files IR210.VXD and INFRARED.INF, which are in the /WIN95.DRV
directory on the IR210's driver diskette #1, to the diskette you just
prepared in step 2).

5). Use the diskette made in step 4 and follow the standard procedures to
perform the driver Install/Un-install.

