
SiS Monitor Release Notes   12/29/1998

(1) The current SiS Monitor release version is 2.22


(2) Supporting Products:

    SiS 5591/5600/620/530 + SiS 5595A2/5595B2


(3) The versions of different OS are as follows :

    Windows 95
    Windows 98
    Windows NT 4.0
    Windows NT 5.0

(4) The following parts have been changed :

    [ v2.21b -> v2.22 ]

        (1) Fix the voltage accuracy problem
        (2) Add a new fan control attribute

    [ v2.21 -> v2.21b ]

        (1) Fix the unexpected fan warning message when window startup .

    [ v2.19 -> v2.21 ]

        (1) Fix the problem that the package can't be installed from CD-ROM.
                ( pcode.exe is obsolete )
        (2) Fix the warning message accuracy


    [ v2.18 -> v2.19 ]

        (1) Fix the Error Message Box display information problem

    [ v2.18 -> v2.19 ]

        (1) Fix the bug of reading thermistor temperature

    [ v2.17 -> v2.18 ]

        (1) Support new thermistor NTC-103AT-2
        (2) Add a ThermistorPullHighRegister factor into vendor.ini to control
            the accuracy of thermistor
        (3) Give a vendor.ini document : readme.txt
        (4) Give some vendor.ini samples ( reference readme.txt )

    [ v2.16 -> v2.17 ]

        (1) Support new thermistor NTC-103JT

    [ v2.15 -> v2.16 ]

        (1) Modify [Visable] menu according to the vendor setting description
        (2) Add linear interpolation algorithm to thermistor detection
        (3) Support new thermistor NTC-103JT


    [ v2.12 -> v2.15 ]

        (1) Support SiS 620/530 Chipset and SiS 5595B
        (2) Support external Diode temperature sensor
        (3) Support external Thmermistor temperatore sensor NTC-103KT-1608-1P
                ( = 10KC15-1608-1P )

    [ v2.11 -> v2.12 ]

        (1) improve the initial time delay and influence when Boot sound playing

    [ v2.10 -> v2.11 ]

        (1) Fix the bug of setting data lose if system reboot
        (2) Fix the Audio influence problem when system start up
            on window 95/osr2


    [ v2.00 -> v2.10 ]

        (1) Support SiS5600 chipset


