	    
	    FREEWARE PROGRAMS FOR POPULAR CDROM RECORDERS
                             VERSION 3.7


CHANGE HISTORY:
  
  Version 3.6
     - Added support for Acer 6206A, HP8100/8110, S&F 8020, and
       Yamaha 4261/2216/4216.

  Version 3.5
     - Added support for Sony CDU-948S.

  Version 3.4
     - Added support for Plextor PX-R412C.

  Version 3.3
     - Added support for Yamaha CRW2260/4260.

  Version 3.2
     - Added support for Philips Omniwriter, Memorex CRW-620,
       and S&F 2006PLUS.

  Version 3.1
    - Added support for the Ricoh MP6200S and JVC XR-W2020.

  Version 3.0
    - Added support for the Yamaha CDR400, Panasonic CW7501,
      Creative CDR4210, and Plasmon CDR4240.

  Version 2.4
    - Added support for the Philips CDD2600 and HP6020i.

  Version 2.3
    - Added support for the Pinnacle RCD-1000/5020/5040, JVC XR-W2001/2010,
      Teac CD-R50S, Sony CDU-940S, and Olympus CDS620E.

  Version 2.2
    - Added support for Ricoh RO-1420C (uses Philips command set)

  Version 2.1
    - Added support for the Olympus CDS615E, Pioneer DW-S114X,
      and Grundig CDR100IPW.

  Version 2.0
    - Added support for the Sony CDU-920S.
  
  Version 1.02
    - Added support for the Ricoh RS-1060C.

    - Recognizes the Yamaha CDR102 (uses CDR100 command set).

    - Recognizes the HP 4020i, Kodak PCD225, Kodak PCD-600, Philips 521,
      Philips CDD2000, and Plasmon RF4100 (all of these use the Philips
      command set).

    - Added new utilities TOC.EXE and FINALIZE.EXE

    - Using DOS read/write routines instead of C++ fread/fwrite for
      improved file I/O performance (using Borland C++ V4.0).

    - Cleaned up all command line interfaces (many new switches have
      also been added). 

  Version 1.01
    - Added support for Yamaha CDR100 recorder.

    - Fixed "read error" problem when making copies of existing
      CD-R discs (i.e. copy of a copy). CD-R discs that are recorded
      with the track-at-once method have two extra blocks (called runout
      blocks) at the end of the disc that are unreadable.
      
**********************************************************************

Freeware Program Descriptions:

CD2CD.EXE
  Copies a single-track data CD from any SCSI based CDROM drive
  directly to the CD recorder. The reader must be faster than the
  recorder (i.e. 4X reader when recording at 2X, or a 2X reader
  when recording at 1X).

CD2FILE.EXE and FILE2CD.EXE
  Copies a CD from any SCSI based CDROM drive to an "image" file
  on disk. This file can then be used by FILE2CD to write the image
  to the CD recorder. These two programs will allow someone who
  doesn't have a SCSI CDROM drive on their system to make copies of
  CDs using only their CD recorder for both reading the source disc
  and writing the new disc. FILE2CD can also be used to make ISO9660
  discs if you already have a program that can build ISO image files.
  You must use the /POSTGAP switch so that the proper track postgap
  is written to the disc.

DISK2CD.EXE
  Copies a SCSI harddrive block-by-block to the CD recorder. This
  program can be used to make native VMS and Unix CDs from the PC.
  The harddrive cannot be larger than the capacity of a CDROM (650Mb).
  NOTE: DOS and NT CDROMs must be in ISO9660 format, so making an
  image copy of a PC disk won't work.

CDTOOLS.EXE
   This program is a collection of miscellaneous CDROM/CD-R tools
   with the following functions...
     - Display a disc's table-of-contents.
     - Erase a disc (CD-RW only).
     - Finalize a session/disc.
     - Load a disc (tray models only).
     - Eject a disc.

   Please refer to CDTOOLS.TXT for more information.

***********************************************************************

>>> TIPS FOR WINDOWS 95 USERS <<<

If you are using the 32-bit version of this software under Windows 95,
then you must make sure that the following settings are enabled/disabled
for all CDROM readers and recorders on your system...

  1) Open the "Control Panel" folder and click on the "System" icon.

  2) Select the "Device Manager" tab.

  3) Click on the CDROM icon

  4) For each CDROM device in the list...
       Select the device.
       Select the "Settings" tab.
       Disable the "Auto Insert Notification" option.
       Enable the "Disconnect" option.
       Enable the "Sync Data Transfer" option. 
       Click on "OK"

If you have an Adaptec SCSI card and are unable to run any of the 
programs under Windows 95/NT, then download and install the latest
drivers from Adaptec's FTP site...

  Windows 95
    ftp://ftp.adaptec.com/pub/BBS/win95/win95mpd.exe
    ftp://ftp.adaptec.com/pub/BBS/win95/aspi32.exe

  Windows NT
    ftp://ftp.adaptec.com/pub/BBS/winnt/aspi32.exe

You must have WNASPI32.DLL to use the 32-bit version of the software.

**********************************************************************

NOTES:

  - You can display the command line switches for any of these
    programs by typing "program-name /?". There must be at least
    one space between each command line argument or switch.
	
  - These programs will only work on a DOS based system with an
    ASPI SCSI manager installed.

  - These programs will only copy single-track data CDs (with CDROM
    Mode-1 type sectors). They will *not* copy audio, CDROM-XA, CD-I,
    mixed-mode, or any type of multi-session disc. If you are not sure
    if your CD has more than one track, use CDTOOLS.EXE to display the
    table-of-contents.
  
  - When using CD2CD/FILE2CD/DISK2CD on any of the Pinnacle, JVC, or
    TEAC recorders, do *not* use the /NOFINALIZE option. This option
    is not supported and will result in a disc that cannot be finalized
    at a later date.

  - All of the programs that write to the recorder have a /TEST option
    that will put the recorder into "write emulation" mode. Please make
    use of this switch when you are trying these programs for the first
    time or are copying a disc that might have a format that these
    programs don't support.

  - You must have a blank CD-R disc in the recorder even when using
    the "write emulation" mode.

  - If you record a CD in "write emulation" mode, you usually have to
    eject the disc from the recorder and re-insert it before you
    can write the disc for real.

**********************************************************************

Please send all suggestions, comments, and bug reports to...

Golden Hawk Technology
125 Indian Rock Road
Merrimack, NH 03054

Phone: 603-429-1027
FAX  : 603-429-0073

Email: support@goldenhawk.com
URL  : http://www.goldenhawk.com

**********************************************************************

Updated on JUNE 23, 1999

