Nero - Burning Rom version 3.0.0.4
Copyright 1995 - 1997 ahead software gmbh
Updated 30-Sep-97


Changes of the new version
==========================
Nero - Burning Rom

* Recorder support
 + Supporting following ATAPI recorder:
   - Sony CDU928E
   - YAMAHA CDR401, CRW4001
   - Ricoh MP6200A
   - Philips CDD3610

* New CD formats
 + HFS CD
 + Hybrid CD
 + Bootable CD

* CD-Copy
 + Copy "on-the-fly" from CD-ROM drives


Changes in previous versions that you should be aware of
========================================================

Version 2.0
~~~~~~~~~~~
* CD-ROM
 + Multisession with track linking
 + Mixed Mode
 + User definable file select filter
* Audio-CD
 + Graphical representation of audio files
 + Audio index setting
 + Optional jitter and CRC-correction
* CD-Copy
 + Complex read-error handling
 + Optional jitter and CRC-correction
* Images
 + Track-at-once and disc-at-once
 + Importing ISO 9660, HFS-images and others
 + Writing third party images, also from other platforms

Version 1.1
~~~~~~~~~~~
+ User settable audio pause length for all recorders
  that support this feature in track-at-once (TAO)
  or that support with disc-at-once (DAO). Also ISRCs
  can be set. See recorder specific notes for details.
+ Joliet support.
+ Copying CDs is much faster as reading is done at
  the maximum speed supported by your recorder and
  system. Also, Nero uses disc-at-once whenever possible.
+ Supports CD-ReWritables with the Ricoh MP6200 
  and MP6201.
+ CD-Copy (from recorder to HD) is supported for 
  . all recorders (see list below).
  . selects best write mode (DAO or TAO) depending on
    recorder capabilities and selected format (CD-ROM 
    or Audio). 
  . CD-ROM, Audio-CDs, Mixed-Mode-CDs, Mode 2 CDs. 
    Exceptions see list below.
+ Audio tracks can be read as wave-files.


Nero Multi-Mounter for WIN 95 and Win NT 4.0
============================================

The Multi-Mounter is installed with the installation
process of Nero. Select any connected CD-ROM or 
CD-Recorder in the Explorer. Use your right mouse 
button to get to the properties of the inserted multi-
session CD. There the new property sheet 'volumes' 
allows you to select any of the existing volumes.

Features:   
- Includes Volume Mounter and Nero IO Driver for 
  Windows 95 and Windows NT 4.0.
- Auto-insert notification is automatically disabled 
  during burn process. 
- Drive letter access is possible also on NT.
- Co-existance with other file system drivers of 
  Easy CD Pro V1.2, Easy CD Pro V2.0, WinOnCd V3.0, 
  Corel CD Creator V2.00, Sony CD-RFS 1.0.



Supported recorders as of 30-Sep-97
==================================

HP 4020, 6020
IMS/Philips CDD2000, CDD2600, *CDD3610
JVC XR-W2010, XR-W2020
Mitsumi CD-R CR-2201CS, CR-2401TS
Pinnacle RCD 4X4
Pioneer CD-WO DW-S114X
Plextor CD-R PX-R24CS
Ricoh RO-1420C, MP6200S, MP6201S, MP6211S, *MP6200A
Sony CDU920S, CDU924S, CDU926S, *CDU928E
Teac CDR-50S-000
Yamaha CDR100, CDR102, CDR400, CDR200, *CDR401, *CRW4001

(* No Windows 3.1x support for ATAPI recorders)


More recorder infos...
======================

HP 4020
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.

HP 6020
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.
- The maximum audio read speed is 4x.

IMS/Philips CDD2000
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.

IMS/Philips CDD2600 
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.
- The maximum audio read speed is 4x.

Philips CDD3610
- Nero does not support Mode 2

JVC XR-W2010, XR-W2020
- CD-Copy uses disc-at-once for CD-ROMs
  and Audio-CD, but uses track-at-once for
  Mixed-Mode-CDs.
- Supports variable pause and ISRC with TAO.
- In some configurations you may encounter
  problems during burning (not simulation).
  If this happens, try turning off Auto-Insert.
- If getting SCSI errors by copying Mixed-Mode CDs,
  turn off reading audio data with sub-code.

Mitsumi CD-R CR-2201CS
- DAO is not supported. CD-Copy uses TAO.
- Does not support variable pause and ISRC.

Mitsumi CR-2401TS
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.

Pinnacle RCD 4X4
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.

Pioneer CD-WO DW-S114X
- CD-Copy uses track-at-once for all CDs.
- Does not support variable pause and ISRC.

Plextor CD-R PX-R24CS
- Recorder does not support DAO.
- CD-Copy uses disc-at-once for all CDs.
- Supports ISRC but not variable pause with TAO.

Ricoh RO-1420C
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.

Ricoh MP6200, MP6201, MP6200A
- CD-Copy uses disc-at-once for all CDs.
- Supports ISRC but not variable pause with TAO.
- Supports CD-ReWritables.

Sony CDU920S, CDU924S
- CD-Copy uses disc-at-once for all CDs.

Sony CDU926S
- Recorder does not support DAO.
- CD-Copy uses track-at-once for all CDs.

Sony CDU928E
- Recorder does not support DAO.
- CD-Copy uses track-at-once for all CDs.
- With firmware version 1.0f or earlier, CD-Info
  gets wrong session information from recorder.

Teac CDR-50S-000
- CD-Copy uses disc-at-once for all CDs.
- Supports variable pause and ISRC with TAO.

Yamaha CDR100, CDR102
- CD-Copy uses disc-at-once for all CDs.
- CD-Copy of Mixed-Mode CDs not supported.
- Does not support variable pause and ISRC.

Yamaha CDR400, CDR200
- CD-Copy uses disc-at-once for all CDs.
- Supports ISRC and variable pause with TAO.

Yamaha CRW4001
- Supports CD-ReWritables.



How to get technical support
============================
Send e-mail to 101776.1057@compuserve.com 
or visit us at http://www.ahead.de
or fax +49 7248 911 888 anytime

