[HDSCSIPFILE]
-1=Read error on SCSI device!
-2=Out of memory!
-3=Seek error on SCSI device!
-4=Illegal call (internal error)!

[HFSIMAGEITEM]
-1=Read error on SCSI device!
-2=Out of memory!
-3=Illegal call (internal error)!

[ISODOC]
-1=Error writing multisession info file!
-2=Error inserting multisession info file into compilation!
-3=Error recreating multisession CD stamp!
-4=Fatal error while trying to read HFS data from SCSI harddisk!
-5=Fatal error while trying to read boot image data!

[W95PARTREADFILE]
-1=Illegal logical drive specified!
-2=Canīt access vwin32.dll!
-3=Drive locking failed!
-4=Seek within logical drive failed!
-5=Open/Close mismatch!
-6=Read error!
-7=Canīt get drive information!
-8=Canīt write on a logical device!

[TRANSFER]
1=User aborted
2=Error opening file
3=Error closing file
4=Error reading file
5=Error reading cache file
-1=General Error
-2=Error: function not implemented
-3=Error: no user interface
-4=Error: phase error
-5=Error: not enough memory
-6=Error writing file
-7=Error opening cache file
-8=Error writing cache file
-9=Error: no driver
-10=Wrong Version
-11=Error accessing cache file
-12=Capability cannot be changed
-13=Error reading cache file
-14=Error writing cache file
-15=Cache file too small
-16=Could not perform StartTrack
-17=Could not perform ReadBuffer
-18=Could not perform EndTrack
-19=Could not perform Fixation
-20=Could not perform Write
-21=Error reading Audio
-22=Cannot cache with Audio-CD
-23=Currently ISO images may only be written on empty CDs!
-24=Could not perform end of Disc At Once
-25=Error reading Data
-26=Recorder doesnīt support Disc At Once
-27=Could not perform start of Disc At Once
-28=Could not generate CD Text information

[IMAGECOMP]
-1=Not enough memory
-2=Read error in image file
-3=Image file has illegal format
-4=Illegal function/method call
-5=Error building internal DAO structures
-6=Strange obscure internal error of unknown kind

[CDR]
-1   =Unspecified Recorder Error
-2   =Bad DLL version
-3   =Recorder function not implemented
-4   =Recorder function not supported
-14  =Capability read only
-15  =Capability unknown
-20  =Queuing failed
-21  =Waitqueue failed
-22  =Abortqueue failed
-23  =Out of memory
-24  =Waitqueue timeout
-100 =Parameter error
-101 =Invalid trackinfo
-102 =Invalid fixinfo
-103 =Invalid trackmode
-104 =Invalid pause length
-200 =Internal state error
-201 =Invalid writestate
-999 =No SCSI/IDE command
-1000=SCSI/IDE error
-1001=Absorption control error
-1002=Application code conflict
-1003=ATIP time miscompare
-1004=Attempt to cross track boundary
-1005=Audio play aborted
-1006=Audio play stopped due to error
-1007=Barcode reading error
-1008=Blocksize conflict
-1009=Blocksize format conflict
-1010=Buffer data size error
-1011=Buffer error during recording
-1012=Buffer overflow
-1013=Buffer underrun
-1014=Calibration area allmost full
-1015=Calibration area full
-1016=Cannot read ATIP
-1017=Cannot recover from leadin
-1018=Cannot recover from leadout
-1019=Cannot recover from PMA
-1020=Cannot recover from callibration area
-1021=Cannot recover from track
-1022=Command currently not valid
-1023=Command sequence error
-1024=Communication failure
-1025=Current command aborted
-1026=Current program area empty
-1027=Damaged track present
-1028=Damaged track detected
-1029=Data track length error
-1030=Diagnostic failure
-1031=Disc is write protected
-1032=Disc style mismatch
-1033=Drive not ready
-1034=Dummy blocks added
-1035=EEPROM failure
-1036=End of medium reached
-1037=End of user area of this track
-1038=Exist packet write area
-1039=Focus or tracking error
-1040=Illegal block size for command
-1041=Illegal cue sheet
-1042=Illegal cue sheet length
-1043=Illegal cue sheet parameter
-1044=Illegal field in command
-1045=Illegal form for reserved track
-1046=This CD is not a CD-Recordable
-1047=Illegal mode for this track
-1048=Illegal packet mode
-1049=Illegal reserve length
-1050=Illegal reserve packet length
-1051=Illegal track
-1052=Illegal track descriptor table
-1053=Illegal track descriptor unit
-1054=Illegal track mode
-1055=Illegal track number
-1056=Illegal track status
-1057=Illegal transfer length
-1058=Inappropriate command
-1059=Initiator detected error message received
-1060=Internal controller error
-1061=Internal target failure
-1062=Invalid audio address
-1063=Invalid bits in identify message
-1064=Invalid block address
-1065=Invalid command
-1066=Invalid field in command
-1067=Invalid field in parameter
-1068=Invalid LUN
-1069=Invalid message error
-1070=Invalid start address
-1071=Laser current over
-1072=Laser adjustment error
-1073=Link area encountered
-1074=Link blocks encountered
-1075=Logical unit is reserved
-1076=Medium changed
-1077=Medium format corrupted
-1078=Medium load mechanism failed
-1079=Medium load or eject failure
-1080=Medium not present
-1081=Medium removal prevented
-1082=Message error
-1083=Mode parameters changed
-1084=Monitor ATIP error
-1085=Non existent block encountered
-1086=Not enough space
-1087=Not ready to ready transition
-1088=No additional sense information
-1089=No barcode available
-1090=No EFM at search address
-1091=No packet
-1092=No pregap
-1093=No seek complete
-1094=No TOC
-1095=No track for finalize
-1096=Operator medium removal requested
-1097=Overlapped command attempted
-1098=Packet size mismatch
-1099=Parameter list length error
-1100=Parameter list too long
-1101=Parity error
-1102=PCA area full
-1103=PMA area full
-1104=Positioning error
-1105=Power calibration error
-1106=Power calibration error
-1107=Program area not empty
-1108=Recovered data with ECC
-1110=Recovered data with retries
-1111=Recovery needed
-1112=Request for fixation failed
-1113=Reserved track present
-1114=Reset occurred
-1115=Select or reselect failure
-1116=Selftest failure
-1117=Stopped on non data block
-1118=Track at once not in PMA
-1119=Track following error
-1120=Tray out
-1121=Unable to read TOC, PMA or subcode
-1122=Unable to recover TOC
-1123=Unable to reserve track, because track mode has been changed
-1124=Unknown medium format
-1125=Unrecordable disc
-1126=Unrecoverable damaged track cause too small writable area
-1127=Unrecoverable track descriptor encountered
-1128=Unrecoverable read error
-1129=Unwritten area encountered
-1130=Verify failed
-1131=Write append error
-1132=Write busy
-1133=Write complete
-1134=Write data error with CU
-1135=Write error
-1136=Write illegal block length
-1137=Write operation in progress
-1138=Writing leadin or leadout in progress
-1139=Audio play in progress
-1140=Audio play completed
-1141=Invalid parameter list length
-1142=Synchronous data transfer error
-1143=Blank CD
-1144=No PMA
-1145=OPC initialization error
-1146=OPC execution error
-1147=OPC ALPC error
-1148=OPC timeout
-1149=Read address is ATIP
-1150=Write address is EFM
-1151=Write emergency occurred
-1152=Medium speed error
-1153=Medium no identification
-1154=Medium not supported
-1155=Write emergency
-1156=Servo error
-1157=PLL error
-1158=Address error
-1159=Header monitor error
-1160=Header search error
-1161=EDC error
-1162=Link/RI/RO error
-1163=CDBD overrun error
-1164=Write audio on reserved track
-1165=Hardware error
-1166=Invisible track present
-1167=Incomplete track present (maybe a CD-RFS-CD?)
-1168=Unknown track present

[AUDIOGEN]
0	=No error
1	=User aborted
2	=File missing 
3	=File hat a wrong format
-1	=Unspecified Audiogenerator Error
-2	=Could not perform StartDisk
-3	=Could not perform StartSession
-4	=Could not perform StartTrack
-5	=Could not perform Write
-6	=Could not perform EndTrack 
-7	=Could not perform EndSession 
-8	=Could not perform EndDisk 
-9	=Could not generate DAO information

[IMAGEGEN]
0	=No error
1	=User aborted
2	=File missing 
3	=File hat a wrong format
-1	=Unspecified Imagegenerator Error
-2	=Could not perform StartDisk
-3	=Could not perform StartSession
-4	=Could not perform StartTrack
-5	=Could not perform Write
-6	=Could not perform EndTrack 
-7	=Could not perform EndSession 
-8	=Could not perform EndDisk 
-9	=Error during ISO relocation
-10 =The image chunks:

[ISO9660GEN]
-3	=Joliet names of these files (listed here in ISO-L3) are equal:
-4	=The ISO9660 Generator ran out of memory
-5	=The following fixed file has an illegal position
-6	=Prepartion of ISO9660 structures failed
-7	=Too many files in one group of interleaved files
-8	=IO error using the boot image
-9	=Cannot allocate space on the CD-R
-10	=Boot sector not recognized

[MAKEJOLIETNAMES]
-3	=The listed files have no unique Joliet name:

[PHASE]
20	=Start of read CD
21	=Read CD done
22	=Read CD failed
23	=Read CD aborted
24	=Start of caching files
25	=Caching files completed
26	=Caching of files failed
27	=Caching of files aborted
28	=Start of speed measurement
29	=Speed measurement done: %dx (%d KB/s)
30	=Speed measurement failed
31	=Speed measurement aborted
32	=Start of simulation at %dx (%d KB/s)
33	=Simulation done successfully at %dx (%d KB/s)
34	=Simulation failed at %dx (%d KB/s)
35	=Simulation aborted
36	=Start of burnprocess at %dx (%d KB/s)
37	=Burnprocess done successfully at %dx (%d KB/s)
38	=Burnprocess failed at %dx (%d KB/s)
39	=Burnprocess aborted
40	=User aborted
41	=Compilation will not fit onto a blank CD
48	=Analyzing CD
57  =DAO Oversize burning option activated
61	=Start of simulation
62	=Simulation done successfully
63	=Simulation failed
64	=Simulation aborted
65	=Start of burnprocess
66	=Burnprocess done successfully
67	=Burnprocess failed
68	=Burnprocess aborted

[CDCOPY]
1	=User aborted
-1	=CD is copyrighted
-2	=Copy for this cd is not supported
-3	=Error writing image file
-4	=Not enough memory
-5	=The CD will not fit onto a blank CD
-6	=Not enough space to copy this CD
-7	=Not enough space to save this wave file
-8	=Invalid track info
-9	=Invalid track mode
-10	=Warning: Unknown data format at
-11	=Warning: EDC, ECC Error at
-12	=Unrecoverable read error at 
-13	=Illegal select for audio track
-14	=Analyzing CD failed
-15	=This drive doesn't support audio extraction
-20	=Error: wrong file type
-21	=Error in StartDisk
-22	=Error in EndDisk
-23	=Error in StartSession
-24	=Error in EndSession
-25	=Error in Write
-26	=Not enough memory

[CDCOPYDOC]
1	=User aborted
-1	=Create image failed
-2	=Error in open image file
-3	=Error writing image file
-4	=Error in close image file
-5	=The image file is invalid
-6	=The format on the source CD isn't supported
-7	=This drive does not support audio extraction

[MMC]
0000=No additional sense information
0006=I/O process terminated
0011=Audio play in progress
0017=Cleaning requested
0200=No seek complete
0400=Logical unit not ready, cause not reportable
0401=Logical unit in process of becoming ready
0402=Logical unit not ready, initialization command required
0403=Logical unit not ready, manual intervention required
0404=Logical unit not ready, format in progress
0407=Logical unit not ready, operation in progress
0408=Logical unit not ready, long write in progress
0500=Logical unit does not respond to selection
0600=No reference position found
0700=Multiple peripherial devices selected
0800=Logical unit communication failure
0801=Logical unit communication time-out
0802=Logical unit communication parity error
0900=Track following error
0901=Track servo error
0902=Focus servo failure
0903=Spindle servo failure
0904=Head select fault
0a00=Error log overflow
0b00=Warning
0b01=Warning, specified temperaturee exceeded
0b02=Warning, enclosure degraded
0c00=Write error
0c07=Write error, recovery needed
0c08=Write error, recovery failed
0c09=Write error, loss of streaming
0c0a=Write error, padding blocks added
1000=Invalid block size for command
1001=Packet does not fit into available space
1002=Buffer underrun
1100=Unrecovered read error
1101=Read retries exhausted
1102=Error too long to correct
1105=L-EC uncorrectable error
1106=CIRC unrecovered error
110f=Error reading UPC/EAN number
1110=Error reading ISRC number
1111=Read error, loss of streaming
1500=Random positioning error
1501=Mechanical positioning error
1502=Positioning error detected by read of medium
1700=Recovered data with no error correction applied
1701=Recovered data with retries
1702=Recovered data with positive head offset
1703=Recovered data with negative head offset
1704=Recovered data with retries and/or CIRC applied
1705=Recovered data using previous secotr id
1707=Recovered data without ECC - recommend reassignment
1708=Recovered data without ECC - recommend rewrite
1709=Recovered data without ECC - data rewritten
1800=Recovered data with error correction applied
1801=Recovered data with error correction & retries applied
1802=Recovered data - data auto-reallocated
1803=Recovered data with CIRC
1804=Recovered data with L-EC
1805=Recoverred data - recommen reassignment
1806=Recoverred data - recommend rewrite
1a00=Parameter list length error
1b00=Synchronous data transfer error
1d00=Miscompare during verify operation
2000=Invalid command operation code
2100=Logical block out of range
2101=Invalid element address
2400=Invalid field in CDB
2500=Logical unit not supported
2600=Invalid field in parameter list
2601=Parameter not supported
2602=Parameter value invalid
2603=Threshold parameters not supported
2604=Invalid release of active persistent reservation
2700=Write protected
2701=Hardware write protected
2702=Logical unit software write protected
2703=Associated write protect
2704=Persistant write protect
2705=Permanent write protect
2800=Not ready to ready change, medium may have changed
2801=Import or export element accessed
2900=Power on, reset or bus device reset occurred
2901=Power on occurred
2902=SCSI bus reset occurred
2903=Bus device reset funtion occurred
2904=Device internal reset
2a00=Parameters changed
2a01=Mode parameters changed
2a02=Log parameters changed
2a03=Reservations preempted
2b00=Copy cannot execute since host cannot disconnect
2c00=Command sequence error
2c03=Current program area is not empty
2c04=Current program area is empty
2e00=Insufficient time for operation
2f00=Commands cleared by another initator
3000=Incompatible medium installed
3001=Cannot read medium - unknown format
3002=Cannot read medium - incompatible format
3003=Cleaning cartridge installed
3004=Cannot write medium - unknown format
3005=Cannot write medium - incompatible format
3006=Cannot format medium - incompatible medium
3007=Cleaning failure
3008=Cannot write - application code mismatch
3009=Current session not fixated for append
3100=Medium format corrupted
3101=Format command failed
3400=Enclosure failure
3500=Enclosure services failure
3501=Unsupported enclosure failure
3502=Enclosure services unavailable
3503=Enclosure services transfer failure
3504=Enclosure services transfer refused
3700=Rounded parameter
3900=Saving parameters not supported
3a00=Medium not present
3a01=Medium not present - tray closed
3a02=Medium not present - tray open
3b0d=Medium destination element full
3b0e=Medium source element empty
3b0f=End of medium reached
3b11=Medium magazine not accessible
3b12=Medium magazine removed
3b13=Medium magazine inserted
3b14=Medium magazine locked
3b15=Medium magazine unlocked
3d00=Invalid bits in identify message
3e00=Logical unit has not self-configured yet
3e01=Logical unit failure
3e02=Timeout on logical unit
3f00=Target operating conditions have changed
3f01=Microcode has been changed
3f02=Changed operating definition
3f03=Inquiry data has changed
4000=Diagnostic failure on component
4300=Message error
4400=Internal target failure
4500=Select or reselect failure
4600=Unsuccessful soft reset
4700=SCSI parity error
4800=Initiator detected error message received
4900=Invalid message error
4a00=Command phase error
4b00=Data phase error
4c00=Logical unit failed self-configuration
4d00=Tagged overlapped commands
4e00=Overlapped commands attempted
5100=Erase failure
5300=Media load or eject failed
5302=Medium removal prevented
5700=Unable to recover table of contents
5a00=Operator request or state change input
5a01=Operator medium removal request
5a02=Operator selected write protect
5a03=Operator selected write permit
5b00=Log exception
5b01=Threshold condition met
5b02=Log counter at maximum
5b03=Log list codes exhausted
5d00=Failure prediction threshold exceeded
5dff=Failure prediction threshold exceeded (FALSE)
5e00=Low power condition on
5e01=Idle condition activated by timer
5e02=Standby condition activated by timer
5e03=Idle condition activated by command
5e04=Standby condition activated by command
6300=End of user area encountered on this track
6301=Packet does not fit in available space
6400=Illegal mode for this track
6401=Invalid packet size
6500=Voltage fault
7200=Session fixation error
7201=Session fixation error writing lead-in
7202=Session fixation error writing lead-out
7203=Session fixation error - incomplete track in session
7204=Empty or partially written reserved track
7300=CD control error
7301=Power calibration area almost full
7302=Power calibration area is full
7303=Power calibration area error
7304=Program memory area update failure
7305=Program memory area is full
8900=Inappropriate command
9082=Read Write Control Task Error
9141=Mechanism Control Task Error
91A1=Mechanism Control Task Error
C100=Illegal track status
C200=Reserved track present
C400=Illegal reserve length for reserve track command
C500=Buffer underrun
C601=Unwritten area encountered
C602=Link blocks encountered
CC00=Not enough space
CD00=No track present to close session
CE00=Unrecordable track descriptor encountered
CF00=Damaged track present
D000=PMA area full
D100=PCA area full
D400=Exit from pseudo track at once recording

[MP6200]
0000=No additional sense information
0006=I/O process terminated
0011=Audio play in progress
0012=Audio play paused
0100=Recovery needed
0101=Recovery failed
0200=No seek complete
0400=Logical unit not ready, cause not reportable
0401=Logical unit in process of becoming ready
0402=Logical unit not ready, initialization command required
0403=Logical unit not ready, manual intervention required
0601=Power calibration area almost full
0800=Logical unit communication failure
0900=Track following error
0901=Track servo error
0902=Focus servo failure
0903=Spindle servo failure
0980=Radial skating error
0981=Sledge servo failure
0982=PLL no lock
0983=Servo off track
0984=ATIP sync error
0985=ATIP/subcode jumped error
0c00=Write error
1000=Invalid block size for command
1001=Packet does not fit into available space
1002=Buffer underrun
1003=Disc is not empty
1004=Current program area is empty
1005=Current program area is not empty
1100=Unrecovered read error
1200=Invalid UPC/EAN number
1201=Error reading UPC/EAN number
1202=Invalid ISRC number
1500=Random positioning error
1700=Recovered data with no error correction applied
1701=Recovered data with retries
1800=Recovered data with error correction applied
1801=Recovered data with error correction & retries applied
1a00=Parameter list length error
2000=Invalid command parameter list
2100=Logical block out of range
2400=Invalid field in CDB
2500=Logical unit not supported
2600=Invalid field in parameter list
2601=Parameter not supported
2602=Parameter value invalid
2700=Write protected
2800=Not ready to ready change, medium changed
2900=Power on, reset or bus device reset occurred
2a00=Parameters changed
2a01=Mode parameters changed
2a02=Padding blocks added
2c00=Command sequence error
2f00=Commands cleared by another initator
3000=Incompatible medium installed
3001=Cannot read medium - unknown format
3002=Cannot read medium - incompatible format
3004=Cannot write medium - unknown format
3005=Cannot write medium - incompatible format
3100=Medium format corrupted
3101=Format command failed
3900=Saving parameters not supported
3a00=Medium not present
3f00=Target operating conditions have changed
3f01=Microcode has been changed
3f03=Inquiry data has changed
4000=Diagnostic failure on component
4400=Internal target failure
4500=Select or reselect failure
4700=SCSI parity error
4800=Initiator detected error message received
4900=Invalid message error
4e00=Overlapped commands attempted
5000=Write append error
5300=Media load or eject failed
5302=Medium removal prevented
5700=Unable to recover table of contents
57c0=Subcode not found
57c1=ATIP not found
57c2=No ATIP or subcode
57c3=PMA error
57c4=TOC read error
57c5=Disc information error
5a00=Operator request or state change input
5a01=Operator medium removal request
6300=End of user area encountered on this track
6400=Illegal mode for this track
6480=Read in lead-in
6481=Read in lead-out
7100=Session fixation error
7101=Session fixation error while writing lead-in
7102=Session fixation error while writing lead-out
7103=Session fixation error - incomplete track in session
7104=Session fixation error - empty or partially written track
7105=Cannot write session at once, no cue sheet
8200=Command now not valid
9000=Reserve track check error
9082=Read Write Control Task Error
9141=Mechanism Control Task Error
91A1=Mechanism Control Task Error
9200=Header search error
9801=Header monitor error
9802=EDC error
9803=Read link, run-in or run-out
9804=Last one block error
9805=Illegal block size
9806=Not all data transferred
9807=CDBD overrun error
a100=Invalild start address
a500=Application code mismatch
aa00=End of medium reached
c101=Invalid track number
c280=Syscon ROM error
c281=Syscon RAM error
c290=EFM encoder error
c291=EFM decoder error
c292=DAC error
c295=Syscon EEPROM error
c2a0=Block decoder communication error
c2a1=Block encoder communication error
c2a2=Block encoder/decoder path error
c300=CD-R engine selftest error
c400=Buffer parity error
c500=Data transfer error
c601=Unwritten area encounterred
c900=Illegal block length
ca00=Power calibration error
ca80=Power range error
ca81=Modulation error
ca82=Beta upper range error
ca83=Beta lower ranger error
ca84=Alpha upper range error
ca85=Alpha lower range error
cd00=No track present to complete
d000=PMA area is full
d001=PMA update failed
d102=Power calibration area is full
e000=12V failure
e100=Undefined syscon error
e101=Syscon communication error
e102=Unknonw syscon error
e200=Syscon not ready
e300=Command rejected
e400=Command not accepted
e500=Verify erro at the beginning of track
e501=Verify error at the ending of track
e502=Verify error at the beginning of lead-in
e503=Verify error at the ending of lead-in
e504=Verify error at the beginning of lead-out
e505=Verify error at the ending of lead-out
ff00=Command phase timeout error
ff01=Data in phase timeout error
ff02=Data out phase timeout error
ff03=Status phase timeout error
ff04=Message in phase timeout error
ff05=Message out phase timeout error
