======================================================================
AU8830 NT 4.0 Driver                                        README.TXT
======================================================================

Release Notes
-----------------
This is version 2.04.04 of the Aureal AU8830 NT 4.0 driver.


I.  Overview
---------------------------

A.  SYSTEM REQUIREMENTS:

	1.  Windows NT 4.0 PC with:
	    * Pentium 166MHz or faster CPU
	    * 32MB RAM
	    * Available PCI slot.
	    * Windows NT installed.
	    * 15MB hard disk space in the Windows NT partition.
	    * CD-ROM drive.
	2.  Good-quality speakers or headphones and connecting cables. 
	3.  Joystick and MIDI keyboard (optional). 


B.  NEW FEATURES:

   1.  Added support for additional Codecs.
  
C.  WINDOWS NT 4.0 DRIVER ISSUES:

   1.  BIOS Settings - For proper operation, any BIOS support for 
       "Plug and Play OS" or "Windows 95 OS" must be disabled. The NT 
       drivers attempt to configure the audio card if the BIOS setting 
       is set correctly, but are not successful on all machine types.

   2.  Matrox Display Adapters - The Matrox drivers shipping with NT 
       4.0 are poorly behaved in the system and hog the PCI bus during 
       heavy graphics usage, which can cause noticable audio dropouts. 
       If using Matrox Millennium II driver v3.20, (4.0.55), try 
       upgrading to the latest Matrox drivers. Upgrading to the latest 
       driver will not guarantee any improvement.  In this case, you 
       may want to contact Matrox directly to address this problem.

   3.  Number Nine Display Adapters - The Number Nine Imagine128 
       drivers shipping with NT4.0 are poorly behaved in the system 
       and hog the PCI bus during heavy graphics usage, which can 
       cause noticable audio dropouts. 

   4.  Riva 128 Display Adapters - The Riva 128 drivers shipping 
       with NT4.0 are poorly behaved in the system and hog the PCI bus 
       during heavy graphics usage, which can cause noticable audio 
       dropouts. A new set of drivers for Riva128 display adapters
       fixes the problem and is available from:

       http://www.stb.com/drivers/velocity/vl128.html

   5.  3COM network card drivers - Version 1.0 of the XL 3COM network 
       card driver found on the NT distribution CD can cause blue 
       screens during installations. Be sure to use 1.1 or above.

II. INSTALLATION
-----------------------

A.  HARDWARE SETUP:

	1.  Power off your computer.
	2.  Remove the cover on your computer.
	3.  Remove the screw and bracket from any free PCI slot.
	4.  Insert the Vortex AU8830 sound card into the free PCI slot.
	5.  Screw in the sound card bracket.
	6.  Replace the cover on the computer.

B.  WINDOWS NT 4.0 DRIVER INSTALLATION:

    If you have an older version of the drivers, please uninstall them 
    now using the uninstallation steps in section C.  After installing 
    the card, you can install multimedia drivers from the CDROM's 
    \NT40 directory. Here are step-by-step directions on Windows 
    NT 4.0 installation:

    First, ensure that any BIOS support for Plug and Play OS or 
    Windows 95 OS is disabled. 

    1. Select Settings->Control Panel from the Start menu, double-
       click on the Multimedia icon, switch to the Devices tab and 
       press the Add button.

    2. Select Unlisted or Updated Driver from the list of drivers 
       and press the Ok button.

    3. Enter the folder of your Vortex NT device driver into the 
       text box and press the "Ok" button. 

    4. Select "Aureal Vortex PCI Audio AU8830" and press the "Ok" 
       button. This also installs the Vortex joystick drivers.

    5. If the driver has already been installed on your computer, you 
       will see a dialog box that lets you choose whether to add a new 
       driver or continue to use the current driver. If you get this 
       prompt, press the "New" button, then press the "Ok" button.

    6. A dialog box with a picture and a joystick settings box is 
       displayed. To enable joystick select the check the enable box, 
       select a port and press the "Ok" button.
	    
    7. Reboot the machine.

       All Vortex drivers are now installed on your system.
	
C.  UNINSTALLING THE WINDOWS NT 4.0 DRIVER:

    1. Open the Multimedia control panel, and remove main Vortex 
       device under the audio key. Follow the on-line instructions 
       to close the system control panel. 


For Technical Support please contact your board manufacturer.


Aureal. A3D, A3D-I, A3D-Interactive, and the Aureal logo are 
trademarks and Vortex is a registered trademark of Aureal 
Semiconductor Inc. All other trademarks are property of their 
respective owners.

=====================================================================
Aureal Semiconductor, Inc.           (c) 1996-98, All Rights Reserved
=====================================================================

