Banshee Windows NT Driver Kit
-----------------------------
Banshee Driver kit: 1.00.00
Banshee WinNT Display Driver and Miniport: 4.00.1381.0077
Banshee Glide 2.X Driver: 2.60.00.0003
Banshee Glide 3.X Driver: 3.10.00.0003
Banshee Control Panel: 1.0.0.0017

Copyright ( 1998 3Dfx Interactive, Inc. )
All Rights Reserved
3Dfx Interactive, Inc.

This product may be covered by one or more of the following
US patents: 5,724,561  5,740,343

NOTE: Use of this software is subject to the terms in the 3Dfx 
license agreement.

=======================================================================
What's in the distribution?
=======================================================================
This distribution contains Voodoo Banshee display drivers and control 
panel for Windows NT 4.0 or higher. 

=======================================================================
Installation 
=======================================================================

Requirements
------------
- Windows NT 4.0 or higher
- PC with a Pentium II, Pentium Pro, Pentium or similar processor
- 16MB of RAM or more Suggested


Fresh Installation / Upgrade Existing Drivers
---------------------------------------------

NOTE: For Fresh Installations, complete Steps 1 - 9 before removing 
your existing 2D card.  If existing Voodoo Banshee drivers are being updated,
installation is complete once step 9 is done.

1) Extract the files for the Voodoo Banshee driver to a directory.
2) Log-in to Windows NT as Administrator.
3) Click Start, Contol Panel.  Double-click on Display.
4) Click the settings tab then click "Change"
6) Click "Have Disk" and enter the path to the extracted drivers.
7) When asked to choose a device, select "Voodoo Banshee"
8) You may then be prompted to insert the Windows NT Voodoo Banshee Driver Disk.
   Enter the path to the drivers again.
9) Windows NT will copy the drivers.   

Steps 10-13 are only used during a fresh installation

10) Power off the system and remove your existing 2D card.
11) Install the Voodoo Banshee Card in a free PCI/AGP Slot
12) Power on the system and verify that video appears during post
13) Start Windows NT.  If problems occur, revert to "Last Known Good"
    from within the Windows NT startup options.

