
  The readme.txt file includes the following topics :

  -- 1. Windows NT 4.0 Driver Installation

  -- 2. Windows 95 Driver Installation

  -- 3. BIOS Flash Utilities


=====================================
1. Windows NT 4.0 Driver Installation
=====================================

Step  1. Reboot your system and enter Windows NT 4.0 (VGA) from the Boot Manager.

Step  2. Launch Windows NT. From your Windows NT wallpaper area,press your
         mouse right buttin then select the "Properties".

Step  3. From "Display Properties", select Settings.

Step  4. Click Display Type.

Step  5. Click Change...  .

Step  6. Click Have Disk...  .

Step  7. Insert the "Windows NT 4.0 Driver" diskette into floppy drive A: . 

Step  8. Change to A:\ directory then select OK when ready.

Step  9. From "Display", select "WinFast 3D S3500/S3600 Display Adapter".

Step 10. From "Third-party Drivers", select Yes.

Step 11. From "Installing Drivers", select OK.

Step 12. From "Display type", select Close.

Step 13. From "Display Properties", select Close.

Step 14. From "System Settings Change", Select Yes.

Step 15. Select Yes to restart Windows NT 4.0 with the new driver.

=================================
2.  Windows 95 Driver Installation
=================================

2.0 Install the Windows 95 with WinFast 3D S3500/S3500ZX board in the PC

    In order to use all of the AGP features,you must usr OSR 2.1 or later
    operating system.

    Install Windows 95 OSR2.0 in the usual way. When installation has
    completed, then upgrade to OSR 2.1 with a USB upgrade .
    Windows 95 should be booted on the VGA. Follow the
    section 2.1 "Fitting WinFast 3D S3500/S3500ZX board with Windows 95
    already installed" to install the drivers of WinFast 3D S3500/S3500ZX.

2.1 Fitting WinFast 3D S3500/S3500ZX board with Windows 95 already installed

    During the booting of Windows 95 OSR 2.1,the "Update Device Wizard"
    window will appear on the screen.Please follow the list steps below
    to install "Standard PCI Graphics Adapter (VGA)" driver.

    Step 1   Click "Next" to let Windows 95 search for "Standard PCI
             Graphics Adapter (VGA)" driver   
    Step 2   Click "Finish" to install the VGA driver
    Step 3   When installation has completed,Windows 95 will prompt you to
             restart your system.Click "No" and follow "2.2 Updating existing
             WinFast 3D S3500/S3500ZX Windows 95 Driver" to install WinFast 3D
             S3500/S3500ZX Windows 95 driver.

2.2 Updating existing WinFast 3D S3500/S3500ZX Windows 95 drivers

    Step 1   Insert the "Windows 95 Driver" diskette into floppy drive A: .
    Step 2   Press the right button of mouse in the Windows 95 wallpaper area.
    Step 3   Select the "Properties" item, a window titled "Display
             Properties" will appear.
    Step 4   Choose the "Settings" tab in the "Display Properties" window.
    Step 5   Select the "Change Display Type" button, a window titled
             "Change Display Type" will appear.
    Step 6   Select the "Change" button in the "Adapter Type" section,
             a window titled "Select Device" will appear.
    Step 7   Select the "Have Disk" button, a window titled
             "Install from Disk" will appear.
    Step 8   Specify the path A: and select the "OK" button in the
             "Install from Disk" window.
    Step 9   Select the "OK" button in the "Select Device" window.
    Step 10  After all new drivers are installed, select the "Close" button
             in the "Change Display Type" window.
    Step 11  Select the "Apply" or "Close" button in the "Display Properties"
             window.
    Step 12  A windows will appear to ask you to restart Windows 95 now.
             Restart the Windows 95 now to use the new drivers.

2.3 Installing VgartD

    AGP support is provided in DirectX-5.  DirectX-5 uses new AGP memory
    management services.  These services provide support for working with AGP
    memory.  Starting with Beta-2 (build 129) DirectX-5 AGP support is
    compatible with Windows 98 and OSR2.1 with the VgartD VxD.

    VgartD is a static VxD that includes support for the new AGP memory
    management services.  If it is running on OSR2.1 the VxD patches the VMM
    service table to direct the VMM service addresses to point to VgartD
    services.  After the VMM service table is patched OSR2.1 supports the AGP
    services that DirectX-5 requires for AGP.

    Vgartd installation depends on the chipsets of the main board. To install
    Vgartd,follow the installation procedures stated in the packing disk of
    the mainboard.

In any case if the VxD is installed on Windows 98 (or any OS other than OSR2.1) it will
not patch the OS - it will silently do nothing.

---------------------------------------------------------------------------
NOTE: It is recommended that the VxD should not be installed on Windows 98.
---------------------------------------------------------------------------



=======================
3. BIOS Flash Utilities
=======================

  Note : Please obtain the BIOS binary file from WEB site or from your local
         dealer.

Step 1. Reboot into DOS or Command Prompt only of Windows 95
Step 2. Insert the "Window NT 4.0 Driver" diskette into floppy drive A: .
Step 3. Copy DOS4GW.EXE, FLASH.EXE to a new directory from A:\FLASH sub-directory .
Step 4. Copy the new BIOS binary file to the new directory
Step 5. Change to the new directory and type the following command :
        FLASH [Filename]
        Note : Filename represents the file name of BIOS binary code.



