===========================
Windows NT 4.0 Installation
===========================

Step  1. Reboot your system and enter Windows NT 4.0 (VGA) from the Boot Manager.

Step  2. Launch Windows NT. Choose Start\Setting\Control Panel\Display.

Step  3. From "Display Properties", select Settings.

Step  4. Click Display Type.

Step  5. Click Change...  .

Step  6. Click Have Disk...  .

Step  7. Insert the release floppy into drive A:\ .

Step  8. Select OK when ready.

Step  9. From "Display", select "WinFast 3D L-Series".

Step 10. From "Third-party Drivers", select Yes.

Step 11. From "Installing Drivers", select OK.

Step 12. From "Display type", select Close.

Step 13. From "Display Properties", select Close.

Step 14. From "System Settings Change", Select Yes.

Step 15. Select Yes to restart Windows NT 4.0 with the new driver.

