12/01/94

This diskette contains the Tseng Laboratoriess ET4000/w32,  /w32i, /w32p
display driver for OS/2 Warp intended to make Warp work with
the w32p Rev D chip. Create a floppy with the 3 files in this zipfile
If you have installed WARP in a directory other than one called OS2, before
installing this, edit the install.cmd file on this floppy so the driver gets
copied to the correct directory. In install.cmd file in the line
copy %1\tliw32pm.dll %2\os2\dll\tliw32pm.dll, change os2 to whatever directory
you installed os2 in.


                    INSTALLATION  INSTRUCTIONS

        Install OS/2 WARP as per instructions from IBM.
        If WARP and the ET4000/W32, /W32i, /W32p display drivers were
        installed without the W32PREVD in place then install vga drivers
        and then replace your display board with W32PREVD board.
        i.e. Step 2 should be done with the REVD board in place.

1.      Enter OS/2 System.
2.      Choose " System Setup "
3.      Choose " Selective Install "
4.      Wait a moment to enter " System Configuration "
5.      Change " Primary Display "
6.      Choose " Tseng Laboratories ET4000/W32, W32i, W32p "
7.      Type your Source Directory
8.      Follow the screen prompts to install the drivers

9.      Install ET4000/W32, /W32i, /W32p display drivers
        that are packaged with WARP.
10.     After Installation, if your video is corrupted:
11.     Hit Ctrl-Alt-Del to reboot your computer.
        When a small white box appears in the upper left hand
        corner of your screen, press ALT+F1. When the Recovery Choices
        screen appears, press C.
12      When the OS2 command line appears:
        Insert the new driver Installation diskette in drive A.
13.     Type:
                A: [enter]
                OS2INST A: C: [enter]

        Where A: is the drive with the new driver diskette,
        and C: is the drive with OS/2 installed.
14.     After the file is copied type:
                  C: [enter]
                  EXIT
        This will continue the reboot started in 4. above and after
        reboot the new driver will be active.

