IF YOU CLOSE THIS FILE BY MISTAKE, YOU CAN FIND IT IN THE 
WINDOWS NT DIRECTORY ON YOUR HARD DISK. THE NAME OF THE FILE
IS HELP.TXT.

This document explains the steps to follow for creating a printer 
using Print Manager.

1. Select the menu-item Printer | Create Printer... in the 
	Print Manager.
2. Give the printer name 'OKIPAGE 4w'.
3. In the 'Print to' combo box, select the item 'Other...' 
	(The last item in the list).
4. In the resulted 'Print Destinations' dialog box, select 
	'Other...' in the list box.
5. Make sure that the edit box of 'Install Print Monitor' dialog 
	contains the drive letter of floopy disk, and click the OK button.
6. In the resulted 'Select Port Monitor' dialog, hilight the item 
	'OPML4W Port' in the list. Make sure that the edit box reads 
	the drive letter of floopy disk and click OK button. This adds the item 
	'OPML4W Port' to the 'Available Print Monitors' list box in 
	the 'Print Destinations' dialog box.
7. Hilight the item 'OPML4W Port' in the list and click OK button 
	in the 'Print Destinations' dialog box. Click OK button of 
	any resulted message box. This puts 'BiLPT1:' in the 'Print to' 
	combo box of 'Create Printer' dialog.
8. In the 'Driver' combo box of 'Create Printer' dialog, select 
	'Other...' (the last item in the list).
9. In the resulted 'Install Driver' dialog box, make sure that the
	edit box contains the drive letter of floopy disk, and click the OK button.
10. In the resulted 'Select Driver' dialog box, hilight the 
	'OKIPAGE 4w' in the list box and make sure that the 
	edit box contains the drive letter of floopy disk. Click OK button.
11. Click OK button of the Create Printer dialog box.
12. Click OK button of the resulted Printer Setup dialog box. 
	This adds a printer to your print system, which can be seen 
	in the Print Manager.
13. Close the Print Manager to continue any remaining file copying
	of the setup.