LSI Logic SDMS 4.0 BTLDPCI-4.06.00 Diskette Building Instructions:


Symbios™ SDMS 4.0 PCI OpenServer
Building the SCO OpenServer BTLD Diskette

To create a BTLD diskette for SCO OpenServer installations, copy the 
raw dd image file onto a 1.44 MB floppy. This process is dependent 
upon the operating system that you are using to create this diskette.
See the instructions below for UNIX System and DOS System Users.

For UNIX System Users

Follow these steps to create the BTLD diskette:
 
1. Insert a 3.5" diskette into the floppy drive. 

2. At the UNIX prompt type: 

   dd if=/<path>/<image_file> of=/dev/fd0135ds18

   The <path> is where the dd image is located. On this CD, the dd 
   image file is located here:

   {UNIX CD-ROM path}/DRIVERS/UNIXES/SCOUNIX

   and the <image_file> is called something similar to SCOX0X00.DD,
   for example:

   SCO40600.DD

   This command will dd the image to the floppy to create a BTLD diskette.
 
For DOS System Users

1. Use a utility that will copy the raw .DD image onto a 1.44 MB floppy.
   "Rawrite", which is a public domain utility, is available. 
   Instructions for using this utility are included in its accompanying 
   "RAWRITE.HTM" file. 

   This .DD image is located at:

   {DOS CD-ROM path}:\DRIVERS\UNIXES\SCOUNIX 

   and the .DD image is called something similar to SCOX0X00.DD,
   for example:

   SCO40600.DD

2. Rawrite is included on this CD-ROM at this location: 

   {DOS CD-ROM path}:\SDMS45\HTML\RAWRITE.HTM

   After the image has been copied to a 3.5" diskette, use this BTLD 
   diskette for SCO OpenServer installations as instructed.

   -OR-

  The other DOS alternative is to use the self-extracting image file,
  which will be called something similar to SCOXXXX.EXE and located at:

  {DOS CD-ROM path}:\DISKIMAG\SCO_UNIX.EXE

 