Symbios Logic SDMS 4.0 PCI UnixWare 2.0 C8XX-4.08.00 BTLD Diskette Building 
Instructions:


To create a C8XX BTLD disk to use with UnixWare 2.0, you must copy the raw dd 
image file onto a 1.44 MB floppy.  The process for doing this will depend on 
what operating system you are using to create the disk.

----------

IF YOU ARE USING A UNIX SYSTEM:
 
1)  Insert a 3.5" diskette into the  floppy drive.  

2)  At the UNIX prompt type:

dd if=/<path>/UW40800.DD of=/dev/rfd0

The <path> is where the dd image is located. This command will dd  the image to 
the floppy to create a C8XX  BTLD disk.

----------

IF YOU ARE USING A DOS SYSTEM:

1)  Use a utility which will copy a raw image onto a 1.44 MB floppy to copy the 
file "UW40800.DD" onto a 3.5" diskette.  (One such utility is "Rawrite" which is 
public domain.  Instructions for using this utility are included in its 
accompanying "doc" file.)

Upon copying the image to a 3.5" disk, it is ready to use as a C8XX BTLD disk 
with UnixWare 2.0.

