# Static Route

1. Click Add to add a new static route to the list.
2. Enter the information for the new static route:
   - Network Address: Enter the IP address of the remote computer for which to set a static route.
   - Subnet Mask: Enter the subnet mask of the remote network for which to set a static route.
   - Gateway: Enter the WAN IP address of the gateway to the remote network.

3. Click SAVE SETTINGS.