# Password Settings

Use this page to change the password for your ADSL2+ Ethernet/USB Router.

The ADSL2+ Ethernet/USB Router lets you set a password up to 12 characters long. These fields are case-sensitive.

Note: If you lost the password, or you cannot gain access to the Web User Interface, press in and hold the Reset button on the rear panel for at least 5 seconds to restore the factory defaults. By default, there is no password to log in to the WUI.

## Reset Your Password

1. Enter your Current Password.
2. Enter the New Password.
3. Re-enter your password to confirm the new password.
4. Enter a maximum Idle Time Out (in minutes) to define a maximum period of time for which the login session is maintained during inactivity. If the connection is inactive for longer than the maximum idle time, it will perform a system logout and you will have to log in again to access the WUI. The default is 10 minutes.
5. Click SAVE SETTINGS.