The USRobotics ADSL2+ Ethernet/USB Router lets you share your ADSL2+ Internet service among multiple devices. Delivering ADSL2+ download speeds up to 24 Mbps, this router has filtering options, as well as a SPI firewall.

# Package Contents

1. USRobotics ADSL2+ Ethernet/USB Router
2. 12V DC Power Supply
3. Ethernet Cable
4. Telephone Cable
5. USB Cable
6. Installation CD-ROM
7. Quick Installation Guide

# Physical Features

## Front

The router has the following status LEDs:

Symbol | Name | State | Condition
| Power | Off | Not receiving power.
Solid | Receiving power.
| LAN | Off | No LAN connection.
Solid | LAN connection is achieved.
Flashing | Sending and receiving data.
| USB | Off | No USB connection.
Solid | USB connection is established.
Flashing | Sending and recieving data.
| ADSL | Off | No ADSL connection.
Solid | ADSL connection is established.
Flashing | ADSL connection is being established
| Internet | Off | No Internet connection.
Flashing | Sending and receiving data.

## Back

The back of the router has the following items:

Item | Function
ADSL | Connects your router to your ADSL line.
12VDC/1A | Connects your router to the supplied power adapter.
Reset | Reboots your router or restores your router to the factory default settings. To reboot your router without changing your current settings, press in and hold the Reset button for 1 to 2 seconds. To restore your router to the factory default settings, press in and hold the Reset button for 5 seconds.
Ethernet | Connects the router to your computer’s Ethernet adapter.
USB | Connects the router to your computer’s USB adapter.

# System Requirements

- ADSL line installed by your Internet Service Provider
- For USB installation: Windows® XP, Windows 2000, Windows Me, or Windows 98SE
- A computer with an Ethernet adapter (NIC) installed
- An HTML 4.01-compliant Web Browser (such as Internet Explorer 5.5 or later or Netscape 8.0 or later) with JavaScript enabled

R46.1576.00
rev 1.7
2/07