# Specifications

Below is an outline of the technical specifications for the ADSL2+ Ethernet/USB Router:

## System Requirements

- ADSL line installed by your Internet Service Provider
- A computer with an Ethernet adapter (NIC) installed
- An HTML 4.01-compliant Web Browser (such as Internet Explorer 5.5 or later or Netscape 7.0 or later) with JavaScript enabled

## Physical Characteristics

- One 10/100Mbps RJ-45 Port
- One ADSL RJ-11 Port

## ADSL Features

- Supports DMT line modulation
- Supports Annex A Full-Rate ADSL: up to 8 Mbps downstream, up to 1 Mbps upstream (G.992.1 &T1.413, Issue 2)
- Supports ADSL2+: up to 24 Mbps downstream, up to 1 Mbps upstream (G.992.5)
- Supports G.Lite ADSL: up to 1.5 Mbps downstream, up to 512 Kbps upstream
- Dying GASP support

## ATM Features

- RFC1483 Encapsulation (IP, Bridging and encapsulated routing)
- PPP over ATM (LLC &VC multiplexing) (RFC2364)
- Classical IP (RFC1577)
- Traffic shaping (UBR, CBR)
- OAM F4/F5 support
- PPP over Ethernet Client

## Management Features

- Firmware update via web based management
- Web based management (configuration)
- Power indicators
- Event and history logging
- Network ping
- QoS

## Security Features

- Password protected configuration access
- User authentication (PAP/CHAP) with PPP
- Firewall NAT NAPT
- VPN pass through (IPSec-ESP Tunnel mode,L2TP, PPTP)

## LAN Features

- IEEE 802.1d (self-learning transparent Bridging)
- DHCP Server
- DNS Proxy
- Static Routing, RIPv1 and RIPv2

## Environmental

Complies with the following standards:

Temperature: IEC 68-2-14

- -10 to 50 degrees C (Standard Operating)

- -40 to 70 degree C (Non-operation)

Humidity

- 10% to 95% (Non-condensing)

Vibration

- IEC 68-2-36, IEC 68-2-6

Shock

- IEC 68-2-29

Drop

- IEC 68-2-32

Dimensions

- 220 x 132 x 30 (mm)

Weight

- 550 g

Input Power

- 12 VDC

## IEEE Standards

- IEEE 802.3, 802.3u, 802.11b, 802.11g, 802.1d
- ITU G.dmt
- ITU G.Handshake
- ITU T.413 issue 2 - ADSL full rate
- ITU G.lite

## Standards Conformance Electromagnetic Compatibility

- CE, ETSI, R&TTE, ETS 300 328, ETS 301 489

## Safety

- EN60950

## Internet Standards

- RFC 826 ARP, RFC 791 IP, RFC 792 ICMP, RFC 768 UDP, RFC 793 TCP, RFC 783 TFTP, RFC 1483 AAL5 Encapsulation, RFC 1661 PPP, RFC 1866 HTML, RFC 2068 HTTP, RFC 2364 PPP over ATM, RFC 2516 PPP over Ethernet