# ISP uses 1483 Bridging-Fixed IP

1. Enter the following Bridging settings provided by your ISP:
   - IP Address: Enter the IP address provided by your ISP.
   - Subnet Mask: Enter the subnet mask address.
   - Default Gateway: Enter the gateway address.
   - DNS Server: Enter the Domain Name Server address.
   - VPI/VCI: Enter the Virtual Path Identifier (VPI) and Virtual Circuit Identifier (VCI).
   - Encapsulation: Select the encapsulation method for your ISP.

2. Click NEXT to continue to the Confirm page.