SPECIFIC TECHNICAL CRITERIA 	
	
UL 60950-1, First Edition
Information technology equipment - Safety- 
Part 1: General Requirements 	
Report Reference No	:	E234083-A8-UL-1	
Compiled by 	:	Gregory Kusnandar		
Reviewed by 	:	Joseph Petilla		
Date of issue 	:	2006-04-10	
Standards 	:	UL 60950-1:2003, First Edition
CSA C22.2 No. 60950-1-03 1st Ed. April 1, 2003	
Test procedure 	:	Listing	
Non-standard test method 	:	N/A	
Test item description 	:	Cordless Telephone System	
Trademark 	:	None	
Model and/or type reference 	:	Cordless Telephone Set (Base, Charging Cradle, and Handset), Model VOIP321XY/ZZ, CIT300, 
(where XYZZ are alphanumeric characters for marketing purpose) and US Robotic 9630

Charging Cradle only, Model VOIP321C, CIT200C, 9630C

Handset and Charging Cradle only, Model VOIP3210Y/ZZ, 9630H
	
Rating(s) 	:	Model VOIP321XY/ZZ and 9630:
Base Input Rating: 9 V dc, 300 mA, Charging Station Input Rating: 9 V dc, 150 mA

Model CIT300:
Base Input Rating: 9 V dc, 300 mA, Charging Station Input Rating: 9 V dc, 150 mA	

Particulars: test item vs. test requirements 	
Equipment mobility 	:	movable	
Operating condition 	:	continuous	
Mains supply tolerance (%) 	:	N/A	
Tested for IT power systems 	:	No	
IT testing, phase-phase voltage (V) 	:	N/A	
Class of equipment 	:	Class III (supplied by SELV)	
Mass of equipment (kg) 	:	< 18 kg	
Protection against ingress of water 	:	IP X0	
	
Possible test case verdicts: 	
- test case does not apply to the test object 	:	N / A	
- test object does meet the requirement 	:	Pass	
- test object does not meet the requirement 	:	Fail (acceptable only if a corresponding, less stringent national requirement is "Pass") 	
General remarks: 	
- "(see Enclosure #)" refers to additional information appended to the Test Report 	
- "(see appended table)" refers to a table appended to the Test Report 	
- Throughout the Test Report a point is used as the decimal separator 	

GENERAL PRODUCT INFORMATION: 	
	
CA1.0 	Report Summary 	
CA1.1 	N/A	
	
CB1.0 	Product Description 	
CB1.1 	The product covered in this report is a desktop single line cordless telephone system. There are no accessible live parts and it is powered by a Class 2 or LPS direct plug-in power supply. An independent charging cradle is supplied by Class 2 / LPS  direct plug-in power supply. The unit is intended for use in a pollution degree 2 environment, connects to TNV-3, and has been evaluated for use in ambient 25°C. 	
	
CC1.0 	Model Differences 	
CC1.1 	Model CIT300 and Model VOIP321XY/ZZ share the following similarities.  Identical Base PWB's except for Phone Jack and Power Connector orientation.  

Model VOIP321C is the Charging Cradle for Model VOIP321XY/ZZ.
Model CIT200C is the Charging Cradle for Model CIT300.
Model VOIP3210Y/ZZ is the Handset and Charging Cradle for Model VOIP321XY/ZZ.
Model CIT300 may also be used to represent the Handset and Charging Cradle only.

Model 9630 is identical with VOIP321XY/ZZ except for enclosure design, shape and model designation.
Model 9630C is the Charging Cradle for model 9630.	
	
CD1.0 	Additional Information 	
CD1.1 	N/A	
	
CE1.0 	Technical Considerations 	
CE1.2	The product was submitted and tested for use at the maximum ambient temperature (Tma) permitted by the manufacturer’s specification of: 25°C 	
CE1.3	The means of connection to the mains supply is: Pluggable A (Direct plug-in power aapter provided with the unit). 	
CE1.4	The product is intended for use on the following power systems: TN 	
CE1.5	The equipment disconnect device is considered to be: Blades of Direct Plug-in Power supply provided with the unit. 	
CE1.10	The following Telecommunication Network Voltage (TNV) circuit locations (with circuit/schematic designation) with exposed plant leads were investigated to Clause 6: JK2 (TNV-3)