1.6.2	TABLE: electrical data (in normal conditions)	Pass	
fuse #	I rated (A)	U (V)	P (W)	I (mA)	I fuse (mA)	condition/status	
MODEL VOIP321XY/ZZ, CHARGING STATION	--	--	--	--	--	--	
--	0.15	10.49	0.85	80.7	--	Charging w/ drained battery, On-Hook,  phone ringing	
--	0.15	10.52	0.83	79.06	--	Charging w/ drained battery, Off-Hook, Talking	
--	0.15	10.49	0.83	79.20	--	Charging w/ drained battery, Handset Off	
MODEL VOIP321XY/ZZ, BASE (Represents model CIT300)	--	--	--	--	--	--	
--	0.3	12.11	1.11	92	--	Off-Hook, connected to Skype	
--	0.3	12.37	1.36	110	--	Off-Hook, connected to POTS	
--	0.3	12.36	1.16	94	--	On-Hook	
--	0.3	12.06	1.45	120	--	Paging	
supplementary information:	
The steady state input current did no exceed the rated current at the rated voltage by more than 10 percent under maximum normal load.	

2.10.3 and 2.10.4	TABLE: clearance and creepage distance measurements	Pass	
clearance cl and creepage distance dcr at/of:	Up
(V)	U r.m.s. (V)	required cl (mm)	cl (mm)	required dcr (mm)	dcr
(mm)	
SELV -> TNV-3	<170	<120	1.5	2.4	1.3	2.4	
supplementary information:	
--	

2.10.5	TABLE: distance through insulation measurements	N/A	
distance through insulation di at/of:	Up 
(V)	test voltage (V)	required di (mm)	di
(mm)	
					
supplementary information:	

4.5	TABLE: temperature rise measurements	N/A	
	test voltage (V)	 :						—	
	t1 (°C)	 :						—	
	t2 (°C)	 :						—	
maximum temperature T of part/at:	T (°C)	allowed Tmax (°C)	
							
temperature T of winding:	R1 ()	R2 ( )	T (°C)	allowed Tmax (°C)	insulation class	
						
supplementary information:	

4.5.2	TABLE: ball pressure test of thermoplastics	N/A	
	allowed impression diameter (mm)	 :		—	
part	test temperature (°C)	impression diameter (mm)	
			
supplementary information:	

4.7	TABLE: resistance to fire	N/A	
part	manufacturer of material	type of material	thickness(mm)	flammability class	
					
supplementary information:	

5.2	TABLE: electric strength tests, impulse tests and voltage surge tests	Pass	
test voltage applied between:	test voltage (V) a.c./d.c.	breakdown
Yes / No	
Transformer (T1), TNV-3 -> SELV	1500 V ac	No	
Transformer (T1), TNV-3 -> Core	1500 V ac	No	
Transformer (T1), SELV -> Core	1500 V ac	No	
Ring & Tip -> Base Enclosure (wrapped in foil)	1500 V ac	No	
Ring & Tip -> USB Connector pins	1414 V dc	No	
supplementary information:	
--	

5.3	TABLE: fault condition tests	N/A	
	ambient temperature (°C)	 :		—	
	model/type of power supply	 :		—	
	manufacturer of power supply	 :		—	
	rated markings of power supply	 :			
component No.	fault	test voltage (V)	test time	fuse No.	fuse current (A)	result	
 	 	 	 	 	 	 	
supplementary information: