******   U.S. Robotics Courier V.Everything V.92 update  ******

- Make sure you have updated the modem's firmware as outlined in Firmware.txt before
  proceeding.

There are three sections to this Readme.

1. Driver update
2. Internet Call Notification (ICN)
3. Instant Update Utility



Section 1:
******************************
*****   Driver update    *****
******************************

Windows XP Users
****************
Note: Log in to an account with administrator rights to update the modem driver.

- Open the Windows Control Panel.
	(Click Windows "Start" and "Control Panel")
  	 or
	(Click Windows "Start", "Settings", and "Control Panel")
- Double-click the "Phone and Modem Options" icon.
	(If you do not see the "Phone and Modems options" icon,
	 click "Switch to Classic View" on the left side of the Control Panel window.)
- Click the Modems tab and select the entry for your Courier modem.
- Click "Properties".
- Select the "Drivers" tab.
- Click "Update Driver".
- Select "Install from a list or specific location" and click "Next".
- Select "Don't Search" and click "Next".
- Click "Have Disk" and click "Browse".
- Browse to the folder where the driver 3453v92.inf is located and click "Open".
- Click "OK" and click "Next".
- A "Hardware Installation" window may appear.
  If it does, click "Continue Anyway" to proceed with the installation.
- Click "Finish" to complete the update procedure.

Windows Me Users
****************

- Right-click the "My Computer" icon on your desktop and click "Properties".
- Click the Device Manager tab and double-click the "Modem" icon.
- Double-click the entry for your Courier modem and select the "Driver" tab.
- Click "Update Driver".
- Select "Specify the location of the driver".
- Click "Next".
- Select "Specify a location" and click "Browse".
- Browse to the folder where the driver 3453v92.inf is located and click "OK".
- Click "Next".
- Click "Next".
- Click "Finish" to complete the update procedure.

Windows 2000 Users
******************

Note: Log in with administrator rights to update the modem driver.

- Right-click the "My Computer" icon on your
  desktop and click "Properties".
- Click the Hardware tab, click "Device Manager", and then 
  double-click "Modems".
- Double-click the entry for your Courier modem and select the "Driver" tab.
- Click "Update Driver".
- Click "Next".
- Make sure that "Display a list of the known drivers for this device..." is selected
  and click "Next".
- Click "Have Disk".
- Browse to the folder where the driver 3453v92.inf is located and click "Open".
- Click "OK".
- Select "U.S. Robotics Courier V.Everything EXT PnP".
- Click "Next".
- Click "Next".
- A "Digital Signature Not Found" warning may appear.
  If it does, click "Yes" to proceed with the installation.
- Click "Finish" to complete the update procedure.

Note: You must now modify your dial up connection to use the new modem.

- Click Windows "Start", "Programs", "Accesories", "Communications", "Network and Dial-up Connections".
- Right-click on the Dial-up icon for your internet connection, then click "Properties".
- Place a checkmark in the box "All devices call the same numbers"
- In the "Connect Using:" field, place a checkmark in the box
  "Modem- U.S. Robotics Courier V.Everything EXT PnP".
- Remove the checkmark in the box "Modem- Courier V.Everything Ext PnP".
- Click "OK" to save your changes.

Windows NT Users
****************

Note: Log in with administrator rights to remove the modem.

- Click Windows "Start", "Settings", and "Control Panel".
- Double-click the "Modems" icon.
- Select "Courier V.Everything EXT" and click "Remove".
- Click "Yes".
- Click "Add".
- Click "Next".
- Click "Change"
- Click "Have Disk". 
- Click "Browse".

     (If a "Locate File" warning appears, click "Cancel".)

- Browse to the folder where the driver 3453v92.inf is located and click "Open".
- Click "OK".
- Select "U.S. Robotics Courier V.Everything EXT" and click "OK".
- Click "Next".
	(If a "Modem Setup" screen appears, click "OK".)
- Click "Finish" to complete the installation procedure.

Note: Dial-up Networking will need to configured for the updated modem.

- Click "Close" to exit the "Modem Properties" screen.
- A "Modem Setup" screen will appear prompting you to configure Dial-up Networking.
- Click "Yes".
- In the "Remote Access Setup" screen, select the entry that contains "Courier V.Everything EXT".
- Click "Remove" and click "Yes".
- Click "Add".
- Select the entry that contains "U.S. Robotics Courier V.Everything EXT" and click "OK".
- Verify the "Configure" and "Network" settings are correct, then Click "Continue".
- Click "Yes" to restart your computer.

Windows 98 Users
****************

- Right-click the "My Computer" icon on your desktop and click "Properties".
- Click the Device Manager tab and double-click the "Modem" icon.
- Double-click the entry for your Courier modem and select the "Driver" tab.
- Click "Update Driver".
- Click "Next".
- Click "Next".
- Select "Specify a location" and click "Browse".
- Browse to the folder where the driver 3453v92.inf is located and click "OK".
- Click "Next".
- Click "Next".
- Click "Finish" to complete the update procedure.

Note: You must now modify your dial up connection to use the new modem.

- Click Windows "Start", "Programs", "Accesories", "Communications", "Dial-Up Networking".
- Right-click on the Dial-up icon for your internet connection, then click "Properties".
  (If a "Dial-Up Networking" message appears, click "OK".)
- In the "Connect Using:" field, select "U.S. Robotics Courier V.Everything EXT PnP".
- Click "OK" to save your changes.

Windows 95B (OSR2) Users
****************

- Right-click the "My Computer" icon on your desktop and click "Properties".
- Click the Device Manager tab and double-click the "Modem" icon.
- Double-click the entry for your Courier modem and select the "Driver" tab.
- Click "Update Driver".
- Click "Next".
- Click "Other Locations" and click "Browse".
- Browse to the folder where the driver 3453v92.inf is located and
  click "OK".
- Click "OK".
- Click "Finish" to complete the update procedure.

Section 2:
************************************************
*****  Internet Call Notification (ICN)   ******
************************************************

Internet Call Notification is required for V.92 Modem on Hold functionality.
ICN supports only Win 9x, ME, 2000, & XP operating systems.

Note: Before using ICN, make sure that DIP switch 9 "located on the
bottom of the modem" is in the ON or down position.

- If you have not downloaded Internet Call Notification (ICN), Go to
  http://www.usr.com/v92/v-upgrade.asp?patch=3453
- Download the ICN installation file to a temporary location on your
  hard drive.
- In Windows Explorer, double-click the "ICNsetup" icon.
  The installation will start. Follow the prompts to complete the installation.


Section 3:
******************************
*****  Instant Update   ******
******************************

The Instant Update utility automatically checks the U.S. Robotics Web site for
firmware updates when you’re online and downloads new features at your convenience.

Installation is optional and not required.

- Go to
  http://www.usr.com/support/3453b/3453b-files/IUsetup.exe
  or
  ftp://ftp.usr.com/usr/3453b/IUsetup.exe
- Download the installation file to a temporary location on your
  hard drive.
- In Windows Explorer, double-click the "IUSetup" icon.
  The installation will start. Follow the prompts to complete the installation.

