******   U.S. Robotics Courier V.Everything V.92 update  ******

Changes from V.90 firmware

- X2 capabilities have been removed.
- Added V.92 functionality.
- Dial security accounts reduced to 80 from 100.


******************************************
*****   Automatic Firmware update   ******
***  (Windows Operating Systems Only)  ***
******************************************

- Browse to the folder where 3453V92.exe is located.
- Double-click on the file to begin updating the firmware.
- (Windows users only) When the update is complete, follow the insructions in the
  Windows.txt file.

**************************************
*****   Manual Firmware update   *****
*****  (All Operating Systems)  *****
**************************************

To send the new code to your modem, all you need is a terminal program that can send files
using the XMODEM protocol. 

Start your terminal program. Adjust the settings, if necessary, so you can send AT to your
modem and get an OK response.
Enter ATXMODEM. The modem should respond as follows:

atxmodem
Firmware Update
---------------
Options:
(1) Read firmware
(2) Write firmware
ESCape Exits
>

Select "2" to begin updating the code. The modem will respond with:

Ready to receive firmware update


Send the file to your modem using either the XMODEM-Checksum or XMODEM-CRC protocol. 
After the transfer is complete, you will see a *TRANSFER SUCCESSFUL* message. 
Press ESC. Modem will automatically reset. Firmware update is complete.

- (Windows users only) When the update is complete, follow the instructions in the
  Windows.txt file.

