******   Mise à jour du U.S. Robotics Courier V.Everything V.92   ******

Veuillez trouver ci-dessous la liste des commandes AT suplémentaires pour le V.92.
Vous pouvez afficher les valeurs par défaut avec la commande ATI92.

+p Command format
        +Pcc=nn Assign value
        +Pcc=?  Display allowed values
        +Pcc?   Display current value

+pBI=n  n=0  Biased upstream
        n=1  Balanced
        n=2  Biased downstream

+pCR=n  n=0  Request fast reconnect to server
        n=1  Disconnect from server
        n=2  Request to accept call
        n=3  Flash hook and reconnect
        n=4  Flash hook and disconnect
        n=8  Switch to telephone
        n=9  Switch back to data

+pCW=n  n=0  Process call waiting
        n=1  Disconnect on call waiting
        n=2  Ignore call waiting

+pIG=n  n=0  Enable PCM upstream
        n=1  Disable PCM upstream

+pMH=n  n=0  Enable Modem on Hold
        n=1  Disable Modem on Hold

+pMHR   Request Modem on Hold

+pMHT?  Display Modem on Hold timeout

+pQC=n  n=0  Enable phase 1 and phase 2 of QC
        n=1  Disable phase 1 and enable phase 2
        n=2  Enable phase 1 and disable phase 2
        n=3  Disable phase 1 and phase 2 of QC

+pSS=n  n=0  Modem decides on short sequences
        n=1  Short sequence as per +pQC
        n=2  Force full startup procedure
