# Uses of Package
com.digi.xbee.api.models

- Packages that use com.digi.xbee.api.models
  Package | Description
  --- | ---
  com.digi.xbee.api |
  com.digi.xbee.api.connection |
  com.digi.xbee.api.exceptions |
  com.digi.xbee.api.listeners |
  com.digi.xbee.api.models |
  com.digi.xbee.api.packet |
  com.digi.xbee.api.packet.common |
  com.digi.xbee.api.packet.raw |

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api
  Class and Description
  AssociationIndicationStatus Enumerates the different association indication status.
  DiscoveryOptions Enumerates the different options used in the discovery process.
  HardwareVersion This class represents the hardware version number of an XBee device.
  OperatingMode Enumerates the different working modes of the XBee device.
  PowerLevel Enumerates the different power levels.
  XBee16BitAddress This class represents a 16-bit network address.
  XBee64BitAddress This class represents a 64-bit address (also known as MAC address).
  XBeeMessage This class represents an XBee message containing the remote XBee device the message belongs to, the content (data) of the message and a flag indicating if the message is a broadcast message (was received or is being sent via broadcast).
  XBeeProtocol Enumerates the available XBee protocols.

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api.connection
  Class and Description
  OperatingMode Enumerates the different working modes of the XBee device.
  XBeePacketsQueue This class represents a queue of XBee packets used for sequential packets reading within the XBee Java API.

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api.exceptions
  Class and Description
  ATCommandStatus Enumerates all the possible states of an AT Command after executing it.
  OperatingMode Enumerates the different working modes of the XBee device.
  XBeeTransmitStatus Enumerates the different transmit status.

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api.listeners
  Class and Description
  ModemStatusEvent Enumerates the different modem status events.
  XBeeMessage This class represents an XBee message containing the remote XBee device the message belongs to, the content (data) of the message and a flag indicating if the message is a broadcast message (was received or is being sent via broadcast).

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api.models
  Class and Description
  AssociationIndicationStatus Enumerates the different association indication status.
  ATCommand This class represents an AT command used to read or set different properties of the XBee device.
  ATCommandStatus Enumerates all the possible states of an AT Command after executing it.
  ATStringCommands Enumerates several AT commands used to parse AT command packets.
  DiscoveryOptions Enumerates the different options used in the discovery process.
  HardwareVersion This class represents the hardware version number of an XBee device.
  HardwareVersionEnum Enumerates the different hardware versions of the XBee devices.
  ModemStatusEvent Enumerates the different modem status events.
  OperatingMode Enumerates the different working modes of the XBee device.
  PowerLevel Enumerates the different power levels.
  SpecialByte Enumerates all the special bytes of the XBee protocol that must be escaped when working on API 2 mode.
  XBee16BitAddress This class represents a 16-bit network address.
  XBee64BitAddress This class represents a 64-bit address (also known as MAC address).
  XBeeDiscoveryStatus Enumerates all the possible states of the discovery.
  XBeeProtocol Enumerates the available XBee protocols.
  XBeeTransmitStatus Enumerates the different transmit status.

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api.packet
  Class and Description
  OperatingMode Enumerates the different working modes of the XBee device.

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api.packet.common
  Class and Description
  ATCommandStatus Enumerates all the possible states of an AT Command after executing it.
  ModemStatusEvent Enumerates the different modem status events.
  XBee16BitAddress This class represents a 16-bit network address.
  XBee64BitAddress This class represents a 64-bit address (also known as MAC address).
  XBeeDiscoveryStatus Enumerates all the possible states of the discovery.
  XBeeTransmitStatus Enumerates the different transmit status.

- Classes in com.digi.xbee.api.models used by com.digi.xbee.api.packet.raw
  Class and Description
  XBee16BitAddress This class represents a 16-bit network address.
  XBee64BitAddress This class represents a 64-bit address (also known as MAC address).
  XBeeTransmitStatus Enumerates the different transmit status.

© Copyright 2014–2014 Digi International Inc. All rights reserved.