- iDigi Dia Home
- User
  - Getting Started
  - Dia Concepts
  - Devices
  - Loggers
  - Presentations
  - Services
  - Tracing
- Developer
  - Overview
  - Drivers
  - Loggers
  - Presentations
  - Services
  - Integrating Application
  - Tracing Manager
  - Debugging
  - Specific Considerations
  - API Reference

- Email
- Phone
- Contact us:

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Presentations »

# TCP CSV

## Overview

TCPCSV Presentation is a simple TCP client which transmits CSV channel data

Each row of the CSV data is given as following format:

`channel_name,timestamp,value,unit`

<Channel Name> | <Timestamp> | <Value> | <Unit>

Where timestamp is adjusted to GMT and given in the format

`YYYY-mm-dd HH:MM:SS`

Warning

Be careful! String samples are not escaped for commas at this time.

## Configuration

A typical TCP CSV configuration block looks like this:

    - name: tcpcsv
      driver: presentations.tcpcsv.tcpcsv:TCPCSV
      settings:
          server: <host IP address>
          port: <host port number>
          interval: 120
          channels: [sensor0.light, sensor0.temperature]

### Settings

server (required)
  IP address or hostname to connect to.
port (required)
  TCP port number to connect to.
interval (optional, default: 60)
  How often (in seconds) to emit CSV data.
channels (optional)
  List of channels to include in the data set. If this setting is not given, all channels will be included.

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Presentations »