- iDigi Dia Home
- User
  - Getting Started
  - Dia Concepts
  - Devices
  - Loggers
  - Presentations
  - Services
  - Tracing
- Developer
  - Overview
  - Drivers
  - Loggers
  - Presentations
  - Services
  - Integrating Application
  - Tracing Manager
  - Debugging
  - Specific Considerations
  - API Reference

- Email
- Phone
- Contact us:

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Device Drivers »
- Rabbit »

# Rabbit XBee GPIO

## Overview

XBee Rabbit General-Purpose I/O (GPIO) Client creates channels based upon the results of a GPIO discovery query to the BL4S100.

## Configuration

A typical Rabbit XBee GPIO configuration block looks like this:

    - name: rabbit_gpio0
      driver: devices.rabbit.xbee_gpio_client:XBeeGPIOClient
      settings:
          xbee_device_manager: <instance name>
          extended_address: <XBee module address>
          poll_rate: 2.0

### Settings

xbee_device_manager (required)
  Name of the XBee_device_manager device declared in the devices section. This setting is necessary because this device will configure all the XBee devices.
extended_address (required)

  MAC address of the BL4S100’s XBee module.

  Notice that the value must have an exclamation sign at end and is between quotes.

poll_rate (optional)
  The number of seconds between each GPIO polling. If the GPIO server is pushing data, this should either be set to 0, or not set at all.

## Channels

The driver creates a channel for each signal based upon the results of a GPIO discovery query to the target device.

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Device Drivers »
- Rabbit »