- iDigi Dia Home
- User
  - Getting Started
  - Dia Concepts
  - Devices
  - Loggers
  - Presentations
  - Services
  - Tracing
- Developer
  - Overview
  - Drivers
  - Loggers
  - Presentations
  - Services
  - Integrating Application
  - Tracing Manager
  - Debugging
  - Specific Considerations
  - API Reference

- Email
- Phone
- Contact us:

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Device Drivers »
- <no title> »
- Massa »

# Massa m300

## Overview

## Configuration

A typical Massa m300 device configuration block looks like this:

    - name: m300
      driver: devices.vendors.massa.m300:MassaM300
      settings:
          xbee_device_manager: <instance name>
          extended_address: <XBee module address>

### Settings

xbee_device_manager (required)
  The name of an XBeeDeviceManager instance to manage this device.
extended_address (required)

  MAC address of the end device’s XBee module.

  Notice that the value must have an exclamation sign at end and is between quotes.

poll_rate_sec (optional, default: 0)

bus_id (optional, default: 0)

## Channels

strength (Get, type: string, unit: %)

target_detected (Get, type: Boolean)

error_flag (Get, type: Boolean)

range (Get, type: integer, unit: in)

temperature (Get, type: float, unit: C)

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Device Drivers »
- <no title> »
- Massa »