- iDigi Dia Home
- User
  - Getting Started
  - Dia Concepts
  - Devices
  - Loggers
  - Presentations
  - Services
  - Tracing
- Developer
  - Overview
  - Drivers
  - Loggers
  - Presentations
  - Services
  - Integrating Application
  - Tracing Manager
  - Debugging
  - Specific Considerations
  - API Reference

- Email
- Phone
- Contact us:

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Device Drivers »
- <no title> »
- B&B Electronics »

# Autotap

## Overview

## Configuration

A typical AutoTap configuration block looks like this:

    - name: autotap
      driver: devices.vendors.bb_electronics.autotap_ldvds:AutoTapLDVDS
      settings:
          xbee_device_manager: <instance name>
          extended_address: <XBee module address>
          update_rate: 10.0

### Settings

xbee_device_manager (required)
  The name of an XBeeDeviceManager instance to manage this device
extended_address (required)

  MAC address of the end device’s XBee module.

  Notice that the value must have an exclamation sign at end and is between quotes.

update_rate (optional, default: 10.0)
  The number of seconds between each parameters polling.

## Channels

### Vehicle parameters

vehicle_speed (Get, type: float)

engine_speed (Get, type: float)

throttle_position (Get, type: float)

odometer (Get, type: float)

fuel_level (Get, type: float)

fuel_level_remaining (Get, type: float)

transmission_gear (Get, type: string)

ignition_status (Get, type: string)

mil_status (Get, type: string)

airbag_dash_indicator (Get, type: string)

abs_dash_indicator (Get, type: string)

fuel_rate (Get, type: float)

battery_voltage (Get, type: float)

pto_status (Get, type: string)

seatbelt_fastened (Get, type: string)

misfire_monitor (Get, type: string)

fuel_system_monitor (Get, type: string)

comprehensive_component_monitor (Get, type: string)

catalyst_monitor (Get, type: string)

heated_catalyst_monitor (Get, type: string)

evaporative_system_monitor (Get, type: string)

secondary_air_system_monitor (Get, type: string)

ac_system_refrigerant_monitor (Get, type: string)

oxygen_sensor_monitor (Get, type: string)

oxygen_sensor_heater_monitor (Get, type: string)

egr_system_monitor (Get, type: string)

brake_switch_status (Get, type: string)

cruise_control_status (Get, type: string)

turn_signal_status (Get, type: string)

oil_pressure_lamp (Get, type: string)

coolant_hot_light (Get, type: string)

trip_odometer (Get, type: float)

trip_fuel_consumption (Get, type: float)

### Static vehicle parameters

vin (Get, type: string)

supported_parameters (Get, type: string)

diagnostic_trouble_codes (Get, type: string)

ready_for_communication (Get, type: integer)

force_redetect (Set, type: integer)

### Navigation

- index
- next |
- previous |
- iDigi Dia |
- User Documentation »
- Device Drivers »
- <no title> »
- B&B Electronics »