1. Connect two USB micro cables to the connectors J7 and J8 to hardware 
2. Power up the hardware
3. Check which serial port has been assigned and configure a terminal program with 
	this configuration (115200/8/N/1)
4. Change switch S1.2 to off
5. Download over USB serial eboot_ivt.sb to target using the command 
	sb_loader /f eboot_ivt.bin
6. In the terminal console hit SPACE or ENTER to stop the boot loader
7. Open the Platform Builder project and open Project->Project Properties
8. Changed manually the Target file name for debugger from nk.bin to eboot_ivt.msb. 
	Click OK.
9. Select Attach Device in Platform Builder
10. Return back to terminal console and select from the bootloader menu the [D] option
11. You will be asked if you would like to store the image into flash press "y" 
12. After storing the image into teh flashthe board is reset. Stop with SPACE the
	bootloader and press [5] to set boot device to NAND.
13. Then select [L] to boot the image from Flash. 

