AnywhereUSB Drivers
Version 3.30 32 bit
Windows XP, Windows Vista, Windows 7
Windows Server 2003 & 2008
Release Version

The installation package will extract the files to the directory: <SystemDrive>:\AnywhereUSB

Release Notes:
===================
v3.30 February 2012

1. Updated driver to use Microsoft's new value of USBD_STATUS_CANCELED.
   Using the old value caused some devices to hang.  
2. Initialize the wValue field of the setup packet. This fixed support for Aladin EToken.
3. A device with a very long USB serial number string could cause a blue screen.  Fixed.
4. IonHub ignored IOCTL_INTERNAL_USB_CYCLE_PORT.  Fixed.  Some USB functional drivers depend 
   on this IOCTL. 
5. If a functional driver used the WdfDeviceAssignS0IdleSettings/IdleUsbSelectiveSuspend method for its device,
   it failed because IonHub reported that the device could wake from PowerDeviceD3.  It (ionhub.sys) has
   been fixed by reporting PowerDeviceD2 in DeviceWake.  This fixes a problem seen with Texas Instruments
   umpusbvista.sys functional driver for its 3410 USB to serial converter.
6. A column in Configuration Utility that was used to display the address of the host in the Host to group
   assignments was too narrow for an IP address of 12 digits.  This caused a line wrap in
   the Host Column and all subsequent group assignments were displayed off by one.




