                      Release Notes PN 93000747_D

                         Digi ConnectPort X2e SE
                       Manufactured with 82002847_H 
					    Firwmare Version 3.2.3.2
                              Jan 20, 2014



INTRODUCTION

    This is a release of manufacturing firmware for the Digi ConnectPort X2e SE. 
	
	The ConnectPort X2e is an enhanced Smart Energy gateway optimized for large 
	deployments of Smart Energy devices in a Home Area Network (HAN) including 
	utility meters, thermostats and in-home displays. The wireless gateway provides 
	a low-cost connection between Smart Energy devices and remote web applications, 
	Digi's SmartleeŽ application for iPhone and Android, or utility-hosted websites 
	designed for consumer engagement. By sharing the homeowner's broadband internet 
	connection, the wireless gateway provides near real-time energy data access 
	and control capabilities based on the Smart Energy devices enabled in the 
	customer's home.


SUPPORTED PRODUCTS

	X2E-Z1C-E1-A	 ConnectPort X2e Smart Energy Coodinator Ethernet 
	X2E-Z1C-E1-W	 ConnectPort X2e Smart Energy Coodinator Ethernet International
	X2E-Z1C-W1-A	 ConnectPort X2e Smart Energy Coodinator Ethernet / Wi-Fi 
	X2E-Z1C-W1-W	 ConnectPort X2e Smart Energy Coodinator Ethernet / Wi-Fi International

	X2E-Z1R-E1-A	 ConnectPort X2e Smart Energy Router Ethernet 
	X2E-Z1R-E1-W	 ConnectPort X2e Smart Energy Router Ethernet International
	X2E-Z1R-W1-A	 ConnectPort X2e Smart Energy Router Ethernet / Wi-Fi 
	X2E-Z1R-W1-W	 ConnectPort X2e Smart Energy Router Ethernet / Wi-Fi International


Firmware Version 3.2.3.2 2014-01-20
===================================

HIGHLIGHTED PRODUCT CHANGES

	- Update Smart Energy Firmware to version 1.6.5


ENHANCEMENTS


    [DBL-135]	- Add feedback to wifi wizard to help user enter the correct information (#40742)
				- Wi-Fi configuration enhancement	
    [DBL-184]	- removed 'iDigi Service Configuration' from 'Ethernet Service Configuration'
				- Added Enable/Disable Network interfaces selection on Web UI
				- Added Source routing 
				- Legal Notice on new page or tab

BUG FIXES


    [DBL-460]	- Security:  Hole found in python SSL - CVE-2013-4328
					Mandriva Linux Security Advisory MDVSA-2013:214
					http://www.mandriva.com/en/support/security/
    [DBL-354]	- Security:  Ignore SRR packets
    [DBL-355]	- Security:  disabled ICMP redirects
	[DBL-444]	- Bug fix in Basic Web UI Authentication
	[DBL-425]	- Reflected Cross Site Scripting in Device Configuration Error Mechanism 
	[DBL-459]  	- If you log in to web GUI with python/no password you have to restart browser 
	[DBL-468]	- Deadlock at a lower level in Python
				- Do not reboot if a firmware update fails
				- Fixed issue with GPS status RCI 
				- Fix issue with WEP / WPA PSK 
	[DBL-437]	- Fixed problem where XBee communications would fail under multi-threaded operations
	[DBL-461]	- Fixed an issue with Firmware update.  If device is rebooted during firmware update
				  it may not accept a subsequent firmware update.


KNOWN ISSUES

    None.


DOCUMENTATION ERRATA

    None.


ADDITIONAL INFORMATION

    NOTE: if you have firmware older than 3.2.0 on your device, you must install 3.2.0.16 before you can upgrade to this version.



Firmware Version 3.2.0.16
=========================

HIGHLIGHTED PRODUCT CHANGES

	- Update Smart Energy Firmware to version 1.6.4.1


Firmware Version 3.2.0.8
=========================

HIGHLIGHTED PRODUCT CHANGES

	- Update Smart Energy Firmware to version 1.6.3.5 and XBee firmware to 5x32

			Bug Fixes: SEF 1.6.3.5

			* SEF-94: Reporting using ZigBee cluster reporting mechanisms now
			  works correctly.  Previously, all reporting was pseudo-reporting.
			* SEF-83: Reporting of configurations using intervals less than one
			  minute no longer generate a backlog.
			* SEF-26: When DRLC GetScheduleEvent requests occurred with a
			  populated StartTime, we would not respond with the proper events.
			* SEF-11: Error reporting and robustness changes to support partner
			  link-key exchange for a multi-ESI scenario.


ENHANCEMENTS

	- Added dropdown box to web page for system log files
	- Various security enhancements
	- Added a firewall on Cellular network interface
	- Separated log files to report on specific component such as smart energy or python scripts
	- Added time server log messages to eventlog.txt 
	- Processor temperature not available via Device Cloud
	- Added support to enter static GPS information via Web UI or Device Cloud
	- Disable TCP timestamps and removed all but one time server entry to reduce traffic on Cellular networks


BUG FIXES

	- Device can be converted from Coordinator to Router without loosing Link Key
	- Fixed an issue where gateway could stop logging 
	- Fixed an issue where timestamps on log files was incorrect
	- Removed XBee network node identifier from Web UI for smart energy gateway
	- Fixed problem where timezone in digi.log was incorrect after a firmware update
	- Fixed an issue where gateway was ignoring Device Cloud keepalive settings
	- Fixed issue where gateway could become unresponsive.	(/tmp was full)


KNOWN ISSUES

    None.


DOCUMENTATION ERRATA

    None.


ADDITIONAL INFORMATION

    None.




Version 3.0.6.17
================

HIGHLIGHTED PRODUCT CHANGES

	None.


ENHANCEMENTS

	Updated ConnectPort X2e SE to include Smart Energy Framework 1.61 and XBee radio firmware V5123


BUG FIXES

43021 - CP-X2e SE:  button-enabled WebUI web page has heading:  ConnectPort X2 Configuration and Management
43121 - CP-X2e SE Quick Start Guide:  need a change made to promote better experiences with Router variant
41476 - zigbee.ddo_command packs parameter with incorrect order
44705 - Negative CPU value reporting. When checking gateway statistics from iDigi the CPX2e SE WiFi module was showing -24 % CPU.
45027 - error message on successful remove_device
44911 - x2e-se:  SE framework isn't starting the first boot after a firmware update
44940 - x2e se:  Python autostart doesn't reboot the system when script throws exception (onexit = reboot)
43362 - device failed to reboot after RCI reboot request
43591 - Sometimes during a reboot chronyd will try and start before the network is ready, which results in a chronyd crash


KNOWN ISSUES

 	None.   

DOCUMENTATION ERRATA

    None.


ADDITIONAL INFORMATION

	There is a hardware update required to fix Vantive #39249. This firmware contains a backward compatible update to support the new hardware.  
	This will require a hardware swap out (see Andrew Lund for more details)


HISTORY

    None.
