                      Release Notes PN 93000783_E

                   Digi ConnectPort X2e SE Cellular
                      Manufactured with 82003141_E
                       Firmware Version 3.2.3.2
                              April 16, 2014


INTRODUCTION

    This is a release of firmware for the Digi ConnectPort X2e SE Cellular. 
	
	The ConnectPort X2e is an enhanced Smart Energy gateway optimized for large 
	deployments of Smart Energy devices in a Home Area Network (HAN) including 
	utility meters, thermostats and in-home displays. The wireless gateway provides 
	a low-cost connection between Smart Energy devices and remote web applications, 
	Digi's SmartleeŽ application for iPhone and Android, or utility-hosted websites 
	designed for consumer engagement. By sharing the homeowner's broadband internet 
	connection, the wireless gateway provides near real-time energy data access 
	and control capabilities based on the Smart Energy devices enabled in the 
	customer's home.



SUPPORTED PRODUCTS

		  X2E-Z1C-H1-A		ConnectPort X2e SE Cellular Coord GSM (UMTS)
		  X2E-Z1R-H1-A		ConnectPort X2e SE Cellular Router GSM (UMTS)
	   	  X2E-Z1C-D2-A		ConnectPort X2e SE Cellular Coord EVDO (Verizon)
		  X2E-Z1R-D2-A		ConnectPort X2e SE Cellular Router EVDO (Verizon)
		  X2E-Z1C-D1-A		ConnectPort X2e SE Cellular Coord EVDO (Sprint)
		  X2E-Z1R-D1-A		ConnectPort X2e SE Cellular Router EVDO (Sprint)


Firmware Version 3.2.3.10 2014-04-16
====================================


HIGHLIGHTED PRODUCT CHANGES
	Add support for Micrel KSZ8081 10Base-T/100Base-TX Ethernet physical-layer transceiver
	Remove SSL HeartBeat extension from openssl library (HeartBleed workaround for openssl CVE-2014-0160)

ENHANCEMENTS
    [DBL-545] - Add support for Micrel KSZ8081 Ethernet PHY


BUG FIXES
	[DBL-624] - Update OpenSSL to resolve the 'heartbleed' vulnerability
    [DBL-614] - Time backs up on reboot until NTP time received
	  
KNOWN ISSUES

    None.


DOCUMENTATION ERRATA

    None.


ADDITIONAL INFORMATION

	 NOTE: if you have firmware older than 3.2.0 on your device, you must install 3.2.0.16 before you can upgrade to this version.




Firmware Version 3.2.3.2 2014-01-20
===================================
HIGHLIGHTED PRODUCT CHANGES


	- Update Smart Energy Firmware to version 1.6.5


ENHANCEMENTS

    [DBL-135]	- Add feedback to wifi wizard to help user enter the correct information (#40742)
				- Wi-Fi configuration enhancement	
    [DBL-184]	- removed 'iDigi Service Configuration' from 'Ethernet Service Configuration'
    [DBL-370]	- Time Server traffic reduction for cellular devices. Added standard and high precision selections
				- Added Enable/Disable Network interfaces selection on Web UI
				- Log password changes in event file 
				- Legal Notice on new page or tab
	[CPX2E-273]	- Added Web Page for sprint provisioning.


BUG FIXES

	[CPX2e-259] - CPX2e Cellular units fail to Register/Provision to Verizon network
    [DBL-460]	- Security:  Hole found in python SSL - CVE-2013-4328
					Mandriva Linux Security Advisory MDVSA-2013:214
					http://www.mandriva.com/en/support/security/
    [DBL-354]	- Security:  Ignore SRR packets
    [DBL-355]	- Security:  disabled ICMP redirects
	[DBL-444]	- Bug fix in Basic Web UI Authentication
	[DBL-425]	- Reflected Cross Site Scripting in Device Configuration Error Mechanism 
	[DBL-459]  	- If you log in to web GUI with python/no password you have to restart browser 
	[DBL-468]	- Deadlock at a lower level in Python
				- Do not reboot if a firmware update fails
				- Fixed issue with GPS status RCI 
				

KNOWN ISSUES

    None.


DOCUMENTATION ERRATA

    None.


ADDITIONAL INFORMATION

	 NOTE: if you have firmware older than 3.2.0 on your device, you must install 3.2.0.16 before you can upgrade to this version.




Firmware Version 3.2.0.16
=========================
HIGHLIGHTED PRODUCT CHANGES

	- Update Smart Energy Firmware to version 1.6.4.1



Firmware Version 3.2.0.6
=========================

HIGHLIGHTED PRODUCT CHANGES

	- Update Smart Energy Firmware to version 1.6.3.3 and XBee firmware to 5x32

			Bug Fixes: SEF 1.6.3.3

			* SEF-94: Reporting using ZigBee cluster reporting mechanisms now
			  works correctly.  Previously, all reporting was pseudo-reporting.
			* SEF-83: Reporting of configurations using intervals less than one
			  minute no longer generate a backlog.
			* SEF-26: When DRLC GetScheduleEvent requests occurred with a
			  populated StartTime, we would not respond with the proper events.
			* SEF-11: Error reporting and robustness changes to support partner
			  link-key exchange for a multi-ESI scenario.


ENHANCEMENTS

	- Added dropdown box to web page for system log files
	- Various security enhancements
	- Added a firewall on Cellular network interface
	- Separated log files to report on specific component such as smart energy or python scripts
	- Added time server log messages to eventlog.txt 
	- Processor temperature not available via Device Cloud
	- Added support to enter static GPS information via Web UI or Device Cloud
	- Disable TCP timestamps and removed all but one time server entry to reduce traffic on Cellular networks


BUG FIXES

	- Device can be converted from Coordinator to Router without loosing Link Key
	- Fixed an issue where gateway could stop logging 
	- Fixed an issue where timestamps on log files was incorrect
	- Removed XBee network node identifier from Web UI for smart energy gateway
	- Fixed problem where timezone in digi.log was incorrect after a firmware update
	- Fixed an issue where gateway was ignoring Device Cloud keepalive settings
	- Fixed issue where gateway could become unresponsive.	(/tmp was full)


KNOWN ISSUES

    None.


DOCUMENTATION ERRATA

    None.


ADDITIONAL INFORMATION

    None.


Firmware Version 3.1.0.6
=========================

HIGHLIGHTED PRODUCT CHANGES

	Initial Release

ENHANCEMENTS

	None.	

BUG FIXES

	None.

KNOWN ISSUES

    None.


DOCUMENTATION ERRATA

    None.


ADDITIONAL INFORMATION

    None.



HISTORY

   	None


