
		Release Notes for Digi ConnectTank 


			Firmware Part Numbers 

		1. 82003325            F/W,Connect Tank, MCU.bin  (for MCU code upgrade over the air)                    
		2. 82003326            F/W,Connect Tank, SingleTank, IEM.bin (for IEM code upgrade over the air)
		
		


INTRODUCTION

This is a production release for the Digi ConnectTank

Digi ConnectTank is a cost-effective solution for single tank monitoring.
This is a battery powered cellular tank sensor device that has built in sensor.


SUPPORTED PRODUCTS & VERSIONS

1. CTANK-M210(Verizon)
2. CTANK-M510(UMTS)
3. CTANK-M110(Sprint)
4. CTANK-M220(Verizon)
5. CTANK-M520(UMTS)
6. CTANK-M120(Sprint) 

 
FEATURE DESCRIPTION

1. Supports ConnectTank requirements like,

	a. Wake on RTC interrupt
	b. Log and send the tank levels to Etherios Device Cloud
	c. Generate tank specific alerts 
	d. Optimised battery life with low power mode.

2. Supports configuration through Etherios Device Cloud

3. Supports Firmware upgrade over the air from Etherios Device Cloud. 

4. Supports enabling and disbling GPS.


Digi ConnectTank Getting Started Guide - http://www.digi.com/products/wireless-sensors-and-cameras/digi-connect-tank#docs



 


	
		





       