<< Previous | Next >>

> AND JKHL,BCDE Bitwise AND Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> ED E6 | AND JKHL,BCDE | 4 (2,2) | JKHL = JKHL & BCDE

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · | · |  |  |

> #### Description

> Performs a bitwise AND operation between the 32-bit registers JKHL and BCDE. The result is stored in JKHL.

<< Previous | Next >>