<< Previous | Next >>

> RR BC Rotate Right Through Carry Rabbit 4000 Instruction

> Opcode | Instruction | Clocks | Operation
> 63 | RR BC | 2 | {BC,CF} = {CF,BC}

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | · | · | · |  |  |

> #### Description

> Rotates to the right with the C flag the data in BC. See the figure below.

> Figure 9: The bit logic of the RR instruction

<< Previous | Next >>