<< Previous | Next >>

> SBC A,(HL) Subtract with Carry Rabbit 2000/3000/3000A Instruction

> Opcode | Instruction | Clocks | Operation
> 9E | SBC A,(HL) | 5 (2,1,2) | A = A - (HL) - CF

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | V | · | · | · |  | · |

> #### Description

> Subtracts the C flag and the data whose address is the data in HL from the data in A. The result is stored in A.

> These operations output an inverted carry:

> - The C flag is set if A is less than the data being subtracted from it.

> - The C flag is cleared if A is greater than the data being subtracted from it.

> - The C flag is unchanged if A is equal to the data being subtracted from it.

<< Previous | Next >>